{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["PAHs in PDMS","PCBs in PDMS","Dioxins in PDMS","PAHs in PE","PCBs in PE","Dioxins in PE"],"not_rendered":{"charts":6,"images":0,"macros":1,"external_links":1,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PAHs in PDMS","index":0,"n_rows":99,"n_cols":26,"rows_kept":99,"cut":false,"hidden":false,"merged":[]}
["PAH PRC CALIBRATION MODEL FOR PDMS SAMPLER"]
["Shen, X., & Reible, D. (2019). An analytical model for the fate and transport of performance reference compounds and target compounds around cylindrical passive samplers. Chemosphere."]
["Version 1.7"]
["2021-08-05",null,null,null,null,null,"Brief techical note"]
[null,null,null,null,null,null,"1. The 'Fss' values refer to the fractional approach to steady state, which is the 1-C/C0 for PRCs and C/Ceq for target compounds"]
["Parameters","Symbol","Value","Unit",null,null,"2. The 'Kpw' values refer to the PDMS-water partition coefficients, and can be estimated from octanol-water coefficients Kow using the correlations "]
["Inner radius","Li",2.4850000000000001E-2,"cm",null,null,null,"Log Kpw = 0.725 * Log Kow + 0.049",null,"(Ghosh et al., 2014)"]
["Outer radius","Lo",2.835E-2,"cm",null,null,"3. The fitting process is to find parameters for the following correlation between sediment retardation factor R and Kow at given effective diffusivities D"]
["Sampling time","t",14,"days",null,null,null,"Log R = α * Log Kow + β"]
[null,null,null,null,null,null,"4. The fitted parameters (Row 28) is automatically derived by maximizing r2 from simulated results at different Ds  "]
["Number of PRCs",4,null,null,null,null,"5. The ‘Nonlinear’ in 'Option' is set to minimize the difference in Fss from calibrated to measurements, 'Linearized' is to minimuze the calibrated R values "]
["PRC #",{"$f":"PRCNumber(1,$B$11)","v":1},{"$f":"PRCNumber(2,$B$11)","v":2},{"$f":"PRCNumber(3,$B$11)","v":3},{"$f":"PRCNumber(4,$B$11)","v":4},{"$f":"PRCNumber(5,$B$11)","v":""},"6. The alpha value of the above correlation could be fixed to a given constant  ",null,null,null,{"$f":"PRCNumber(13,$B$11)","v":""},{"$f":"PRCNumber(14,$B$11)","v":""},{"$f":"PRCNumber(15,$B$11)","v":""},{"$f":"PRCNumber(16,$B$11)","v":""},{"$f":"PRCNumber(14,$B$11)","v":""},{"$f":"PRCNumber(15,$B$11)","v":""},{"$f":"PRCNumber(16,$B$11)","v":""},{"$f":"PRCNumber(17,$B$11)","v":""},{"$f":"PRCNumber(18,$B$11)","v":""},{"$f":"PRCNumber(19,$B$11)","v":""},{"$f":"PRCNumber(20,$B$11)","v":""},{"$f":"PRCNumber(21,$B$11)","v":""},{"$f":"PRCNumber(22,$B$11)","v":""},{"$f":"PRCNumber(23,$B$11)","v":""},{"$f":"PRCNumber(24,$B$11)","v":""},{"$f":"PRCNumber(25,$B$11)","v":""}]
["PRC name","C13-phenanthrene","C13-fluoranthene","C13-chrysene","C13-indeno[1,2,3-CD]pyrene"]
["Log Kow",4.74,5.29,5.9,7.09,null,"Procedure"]
["Log Kpw",3.9155000000000002,4.3142499999999995,4.7565,5.6192500000000001,null,"1. Update the properties of sampler and PRCs on this sheet in Green "]
["Measured PRC Fss",0.6,0.5,0.4,0.2,null,"2. Input a list of desired effective diffusivity (D) in column A starting row 33."]
[null,null,null,null,null,null,"3. Start the fitting by clicking on  \"Fit fss Data\""]
[null,null,null,null,null,null,"4. Check the fitted results (parameters in Row 28, results in the following figure), if it is not desired, change the list of D  "]
[null,null,null,null,null,null,"5. View model results in the following figure, the returned data are in cyl_fitted_plot"]
[]
[null,null,null,null,null,null,"Database of frequently used PRCs"]
[]
[null,null,null,null,null,null,"PRCs set 1"]
[null,null,null,null,null,null,"PRC name","C13-phenanthrene","C13-fluoranthene","C13-chrysene","C13-indeno[1,2,3-CD]pyrene"]
[null,null,null,null,null,null,"Log Kow",4.74,5.29,5.9,7.09]
[null,null,null,null,null,null,"Log Kpw",3.9155000000000002,4.3142499999999995,4.7565,5.6192500000000001]
["Results"]
["Cylindrical diffusion model","Log R = α * Log Kow + β"]
["D",9.9999999999999995E-8]
["α",0.87758661013561212]
["β",-0.33347817291629317]
["r2",0.99949621707571623]
[]
[]
["Model prediction"]
["Target Compound","Log Kow","Log Kpw","Log R","ξ","τ","ω","fss"]
["naphthalene ",3.41,{"$f":"B37*0.725+0.479","v":2.9512499999999999},{"$f":"B37*$B$30+$B$31","v":2.6590921676461443},{"$f":"10^C37*($C$8^2-$C$7^2)/10^D37/$C$8^2","v":0.45397442009777256},{"$f":"$B$29*$C$9*86400/10^D37/$C$8^2","v":0.32994646826686824},{"$f":"IF(E37>1,(1/E37-1/E37^2)^0.5,(1/E37^2-1/E37)^0.5)","v":1.6277028047921749},{"$f":"IFERROR(IF(E37>1,1-(EXP((1/E37^2-G37^2)*F37)*((COS(G37/E37*F37*2)*(1-erfzR(1/E37*F37^0.5,G37*F37^0.5))-SIN(G37/E37*F37*2)*(-erfzI(1/E37*F37^0.5,G37*F37^0.5)))+(COS(G37/E37*F37*2)*(-erfzI(1/E37*F37^0.5,G37*F37^0.5))+SIN(G37/E37*F37*2)*(1-erfzR(1/E37*F37^0.5,G37*F37^0.5)))/E37/G37)),1-((1/E37+G37)*EXP((1/E37+G37)^2*F37)*ERFC((1/E37+G37)*F37^0.5)-(1/E37-G37)*EXP((1/E37-G37)^2*F37)*ERFC((1/E37-G37)*F37^0.5))/2/G37),1)","v":0.84898493131737141}]
["acenaphthylene ",4,{"$f":"B38*0.725+0.479","v":3.379},3.1768682676261553,{"$f":"10^C38*($C$8^2-$C$7^2)/10^D38/$C$8^2","v":0.36898208667378724},0.10015378899598167,{"$f":"IF(E38>1,(1/E38-1/E38^2)^0.5,(1/E38^2-1/E38)^0.5)","v":2.1528588739901355},{"$f":"IFERROR(IF(E38>1,1-(EXP((1/E38^2-G38^2)*F38)*((COS(G38/E38*F38*2)*(1-erfzR(1/E38*F38^0.5,G38*F38^0.5))-SIN(G38/E38*F38*2)*(-erfzI(1/E38*F38^0.5,G38*F38^0.5)))+(COS(G38/E38*F38*2)*(-erfzI(1/E38*F38^0.5,G38*F38^0.5))+SIN(G38/E38*F38*2)*(1-erfzR(1/E38*F38^0.5,G38*F38^0.5)))/E38/G38)),1-((1/E38+G38)*EXP((1/E38+G38)^2*F38)*ERFC((1/E38+G38)*F38^0.5)-(1/E38-G38)*EXP((1/E38-G38)^2*F38)*ERFC((1/E38-G38)*F38^0.5))/2/G38),1)","v":0.75109266098876515}]
["acenaphthene ",4.0599999999999996,3.4224999999999999,3.2295234642342918,0.36128512915314948,8.8718090835830918E-2,2.2120932365390007,{"$f":"IFERROR(IF(E39>1,1-(EXP((1/E39^2-G39^2)*F39)*((COS(G39/E39*F39*2)*(1-erfzR(1/E39*F39^0.5,G39*F39^0.5))-SIN(G39/E39*F39*2)*(-erfzI(1/E39*F39^0.5,G39*F39^0.5)))+(COS(G39/E39*F39*2)*(-erfzI(1/E39*F39^0.5,G39*F39^0.5))+SIN(G39/E39*F39*2)*(1-erfzR(1/E39*F39^0.5,G39*F39^0.5)))/E39/G39)),1-((1/E39+G39)*EXP((1/E39+G39)^2*F39)*ERFC((1/E39+G39)*F39^0.5)-(1/E39-G39)*EXP((1/E39-G39)^2*F39)*ERFC((1/E39-G39)*F39^0.5))/2/G39),1)","v":0.74013590331466506}]
["fluorene ",4.2,3.524,3.3523855896532777,0.34394417646430742,6.6857489076546803E-2,2.3549540464529466,{"$f":"IFERROR(IF(E40>1,1-(EXP((1/E40^2-G40^2)*F40)*((COS(G40/E40*F40*2)*(1-erfzR(1/E40*F40^0.5,G40*F40^0.5))-SIN(G40/E40*F40*2)*(-erfzI(1/E40*F40^0.5,G40*F40^0.5)))+(COS(G40/E40*F40*2)*(-erfzI(1/E40*F40^0.5,G40*F40^0.5))+SIN(G40/E40*F40*2)*(1-erfzR(1/E40*F40^0.5,G40*F40^0.5)))/E40/G40)),1-((1/E40+G40)*EXP((1/E40+G40)^2*F40)*ERFC((1/E40+G40)*F40^0.5)-(1/E40-G40)*EXP((1/E40-G40)^2*F40)*ERFC((1/E40-G40)*F40^0.5))/2/G40),1)","v":0.71402088546022857}]
["phenanthrene ",4.74,3.9155000000000002,3.826282359126508,0.28450584363840414,2.2451909995887833E-2,2.9731160026788155,{"$f":"IFERROR(IF(E41>1,1-(EXP((1/E41^2-G41^2)*F41)*((COS(G41/E41*F41*2)*(1-erfzR(1/E41*F41^0.5,G41*F41^0.5))-SIN(G41/E41*F41*2)*(-erfzI(1/E41*F41^0.5,G41*F41^0.5)))+(COS(G41/E41*F41*2)*(-erfzI(1/E41*F41^0.5,G41*F41^0.5))+SIN(G41/E41*F41*2)*(1-erfzR(1/E41*F41^0.5,G41*F41^0.5)))/E41/G41)),1-((1/E41+G41)*EXP((1/E41+G41)^2*F41)*ERFC((1/E41+G41)*F41^0.5)-(1/E41-G41)*EXP((1/E41-G41)^2*F41)*ERFC((1/E41-G41)*F41^0.5))/2/G41),1)","v":0.60835594192370901}]
["anthracene ",4.6900000000000004,3.8792500000000003,3.7824030286197283,0.28954796806325561,2.4838915101602892E-2,2.9110311907262512,{"$f":"IFERROR(IF(E42>1,1-(EXP((1/E42^2-G42^2)*F42)*((COS(G42/E42*F42*2)*(1-erfzR(1/E42*F42^0.5,G42*F42^0.5))-SIN(G42/E42*F42*2)*(-erfzI(1/E42*F42^0.5,G42*F42^0.5)))+(COS(G42/E42*F42*2)*(-erfzI(1/E42*F42^0.5,G42*F42^0.5))+SIN(G42/E42*F42*2)*(1-erfzR(1/E42*F42^0.5,G42*F42^0.5)))/E42/G42)),1-((1/E42+G42)*EXP((1/E42+G42)^2*F42)*ERFC((1/E42+G42)*F42^0.5)-(1/E42-G42)*EXP((1/E42-G42)^2*F42)*ERFC((1/E42-G42)*F42^0.5))/2/G42),1)","v":0.61833688236265338}]
["fluoranthene ",5.29,4.3142499999999995,4.3089549947010948,0.23451388183999988,7.3889147688234961E-3,3.7307839880720279,{"$f":"IFERROR(IF(E43>1,1-(EXP((1/E43^2-G43^2)*F43)*((COS(G43/E43*F43*2)*(1-erfzR(1/E43*F43^0.5,G43*F43^0.5))-SIN(G43/E43*F43*2)*(-erfzI(1/E43*F43^0.5,G43*F43^0.5)))+(COS(G43/E43*F43*2)*(-erfzI(1/E43*F43^0.5,G43*F43^0.5))+SIN(G43/E43*F43*2)*(1-erfzR(1/E43*F43^0.5,G43*F43^0.5)))/E43/G43)),1-((1/E43+G43)*EXP((1/E43+G43)^2*F43)*ERFC((1/E43+G43)*F43^0.5)-(1/E43-G43)*EXP((1/E43-G43)^2*F43)*ERFC((1/E43-G43)*F43^0.5))/2/G43),1)","v":0.49899647235956912}]
["pyrene ",5.25,4.2852499999999996,4.2738515302956701,0.23783294843676736,8.0109518499202111E-3,3.6707352746138526,{"$f":"IFERROR(IF(E44>1,1-(EXP((1/E44^2-G44^2)*F44)*((COS(G44/E44*F44*2)*(1-erfzR(1/E44*F44^0.5,G44*F44^0.5))-SIN(G44/E44*F44*2)*(-erfzI(1/E44*F44^0.5,G44*F44^0.5)))+(COS(G44/E44*F44*2)*(-erfzI(1/E44*F44^0.5,G44*F44^0.5))+SIN(G44/E44*F44*2)*(1-erfzR(1/E44*F44^0.5,G44*F44^0.5)))/E44/G44)),1-((1/E44+G44)*EXP((1/E44+G44)^2*F44)*ERFC((1/E44+G44)*F44^0.5)-(1/E44-G44)*EXP((1/E44-G44)^2*F44)*ERFC((1/E44-G44)*F44^0.5))/2/G44),1)","v":0.50682910820732729}]
["benz(a)anthracene",5.85,4.7202500000000001,4.8004034963770374,0.19262828311464447,2.3830445168029654E-3,4.664624746597184,{"$f":"IFERROR(IF(E45>1,1-(EXP((1/E45^2-G45^2)*F45)*((COS(G45/E45*F45*2)*(1-erfzR(1/E45*F45^0.5,G45*F45^0.5))-SIN(G45/E45*F45*2)*(-erfzI(1/E45*F45^0.5,G45*F45^0.5)))+(COS(G45/E45*F45*2)*(-erfzI(1/E45*F45^0.5,G45*F45^0.5))+SIN(G45/E45*F45*2)*(1-erfzR(1/E45*F45^0.5,G45*F45^0.5)))/E45/G45)),1-((1/E45+G45)*EXP((1/E45+G45)^2*F45)*ERFC((1/E45+G45)*F45^0.5)-(1/E45-G45)*EXP((1/E45-G45)^2*F45)*ERFC((1/E45-G45)*F45^0.5))/2/G45),1)","v":0.3940504115909409}]
["chrysene ",5.9,4.7565,4.8442828268838189,0.18927389669740824,2.1540353428721741E-3,4.7571446251849885,{"$f":"IFERROR(IF(E46>1,1-(EXP((1/E46^2-G46^2)*F46)*((COS(G46/E46*F46*2)*(1-erfzR(1/E46*F46^0.5,G46*F46^0.5))-SIN(G46/E46*F46*2)*(-erfzI(1/E46*F46^0.5,G46*F46^0.5)))+(COS(G46/E46*F46*2)*(-erfzI(1/E46*F46^0.5,G46*F46^0.5))+SIN(G46/E46*F46*2)*(1-erfzR(1/E46*F46^0.5,G46*F46^0.5)))/E46/G46)),1-((1/E46+G46)*EXP((1/E46+G46)^2*F46)*ERFC((1/E46+G46)*F46^0.5)-(1/E46-G46)*EXP((1/E46-G46)^2*F46)*ERFC((1/E46-G46)*F46^0.5))/2/G46),1)","v":0.38522687957299584}]
["benzo(b)fluoranthene ",6.58,5.2495000000000003,5.4410417217760347,0.14904994784824732,5.4512227653342614E-4,6.1889960598843761,{"$f":"IFERROR(IF(E47>1,1-(EXP((1/E47^2-G47^2)*F47)*((COS(G47/E47*F47*2)*(1-erfzR(1/E47*F47^0.5,G47*F47^0.5))-SIN(G47/E47*F47*2)*(-erfzI(1/E47*F47^0.5,G47*F47^0.5)))+(COS(G47/E47*F47*2)*(-erfzI(1/E47*F47^0.5,G47*F47^0.5))+SIN(G47/E47*F47*2)*(1-erfzR(1/E47*F47^0.5,G47*F47^0.5)))/E47/G47)),1-((1/E47+G47)*EXP((1/E47+G47)^2*F47)*ERFC((1/E47+G47)*F47^0.5)-(1/E47-G47)*EXP((1/E47-G47)^2*F47)*ERFC((1/E47-G47)*F47^0.5))/2/G47),1)","v":0.27680310963552501}]
["benzo(k)fluoranthene ",6.5,5.1914999999999996,5.3708347929651854,0.15329880068712937,6.4076806464421132E-4,6.0024193052637349,{"$f":"IFERROR(IF(E48>1,1-(EXP((1/E48^2-G48^2)*F48)*((COS(G48/E48*F48*2)*(1-erfzR(1/E48*F48^0.5,G48*F48^0.5))-SIN(G48/E48*F48*2)*(-erfzI(1/E48*F48^0.5,G48*F48^0.5)))+(COS(G48/E48*F48*2)*(-erfzI(1/E48*F48^0.5,G48*F48^0.5))+SIN(G48/E48*F48*2)*(1-erfzR(1/E48*F48^0.5,G48*F48^0.5)))/E48/G48)),1-((1/E48+G48)*EXP((1/E48+G48)^2*F48)*ERFC((1/E48+G48)*F48^0.5)-(1/E48-G48)*EXP((1/E48-G48)^2*F48)*ERFC((1/E48-G48)*F48^0.5))/2/G48),1)","v":0.28836170325829824}]
["benzo(a)pyrene ",6.54,5.2205000000000004,5.4059382573706101,0.15115944643857232,5.9101349064870823E-4,6.0950569398369518,{"$f":"IFERROR(IF(E49>1,1-(EXP((1/E49^2-G49^2)*F49)*((COS(G49/E49*F49*2)*(1-erfzR(1/E49*F49^0.5,G49*F49^0.5))-SIN(G49/E49*F49*2)*(-erfzI(1/E49*F49^0.5,G49*F49^0.5)))+(COS(G49/E49*F49*2)*(-erfzI(1/E49*F49^0.5,G49*F49^0.5))+SIN(G49/E49*F49*2)*(1-erfzR(1/E49*F49^0.5,G49*F49^0.5)))/E49/G49)),1-((1/E49+G49)*EXP((1/E49+G49)^2*F49)*ERFC((1/E49+G49)*F49^0.5)-(1/E49-G49)*EXP((1/E49-G49)^2*F49)*ERFC((1/E49-G49)*F49^0.5))/2/G49),1)","v":0.28254089093253376}]
["indeno(123-cd)pyrene ",7.09,5.6192500000000001,5.8886108929451968,0.12459845501855311,1.9450230784053531E-4,7.5091537592197879,{"$f":"IFERROR(IF(E50>1,1-(EXP((1/E50^2-G50^2)*F50)*((COS(G50/E50*F50*2)*(1-erfzR(1/E50*F50^0.5,G50*F50^0.5))-SIN(G50/E50*F50*2)*(-erfzI(1/E50*F50^0.5,G50*F50^0.5)))+(COS(G50/E50*F50*2)*(-erfzI(1/E50*F50^0.5,G50*F50^0.5))+SIN(G50/E50*F50*2)*(1-erfzR(1/E50*F50^0.5,G50*F50^0.5)))/E50/G50)),1-((1/E50+G50)*EXP((1/E50+G50)^2*F50)*ERFC((1/E50+G50)*F50^0.5)-(1/E50-G50)*EXP((1/E50-G50)^2*F50)*ERFC((1/E50-G50)*F50^0.5))/2/G50),1)","v":0.21095427088615715}]
["dibenzo(ah)anthracene ",7.39,5.8367499999999994,6.1518868759858805,0.11213383469930591,1.0608372858252548E-4,8.4030525391340092,{"$f":"IFERROR(IF(E51>1,1-(EXP((1/E51^2-G51^2)*F51)*((COS(G51/E51*F51*2)*(1-erfzR(1/E51*F51^0.5,G51*F51^0.5))-SIN(G51/E51*F51*2)*(-erfzI(1/E51*F51^0.5,G51*F51^0.5)))+(COS(G51/E51*F51*2)*(-erfzI(1/E51*F51^0.5,G51*F51^0.5))+SIN(G51/E51*F51*2)*(1-erfzR(1/E51*F51^0.5,G51*F51^0.5)))/E51/G51)),1-((1/E51+G51)*EXP((1/E51+G51)^2*F51)*ERFC((1/E51+G51)*F51^0.5)-(1/E51-G51)*EXP((1/E51-G51)^2*F51)*ERFC((1/E51-G51)*F51^0.5))/2/G51),1)","v":0.17841742787189341}]
["benzo(ghi)perylene ",7.04,5.5830000000000002,5.8447315624384162,0.126806637828838,2.1518108314178011E-4,7.3690792151481048,{"$f":"IFERROR(IF(E52>1,1-(EXP((1/E52^2-G52^2)*F52)*((COS(G52/E52*F52*2)*(1-erfzR(1/E52*F52^0.5,G52*F52^0.5))-SIN(G52/E52*F52*2)*(-erfzI(1/E52*F52^0.5,G52*F52^0.5)))+(COS(G52/E52*F52*2)*(-erfzI(1/E52*F52^0.5,G52*F52^0.5))+SIN(G52/E52*F52*2)*(1-erfzR(1/E52*F52^0.5,G52*F52^0.5)))/E52/G52)),1-((1/E52+G52)*EXP((1/E52+G52)^2*F52)*ERFC((1/E52+G52)*F52^0.5)-(1/E52-G52)*EXP((1/E52-G52)^2*F52)*ERFC((1/E52-G52)*F52^0.5))/2/G52),1)","v":0.21681489140087451}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"A96*10^0.02","v":0},1,14.883034744223696,0.98710318949221576]
[0,1,-81.52211188194967,0.98659157472021164]
[{"$f":"A98*10^0.02","v":0},1,17.534850078544217,0.98538337426517375]

{"sheet":"PCBs in PDMS","index":1,"n_rows":245,"n_cols":17,"rows_kept":245,"cut":false,"hidden":false,"merged":[]}
["PCB PRC CALIBRATION MODEL FOR PDMS SAMPLER"]
["Shen, X., & Reible, D. (2019). An analytical model for the fate and transport of performance reference compounds and target compounds around cylindrical passive samplers. Chemosphere."]
["Version 1.7"]
["2021-08-05",null,null,null,null,null,null,null,null,"Brief techical note"]
[null,null,null,null,null,null,null,null,null,"1. The 'Fss' values refer to the fractional approach to steady state, which is the 1-C/C0 for PRCs and C/Ceq for target compounds"]
["Parameters","Symbol","Value","Unit",null,null,null,null,null,"2. The 'Kpw' values refer to the PDMS-water partition coefficients, and can be estimated from octanol-water coefficients Kow using the correlations "]
["Inner radius","Li",2.4850000000000001E-2,"cm",null,null,null,null,null,null,"Log Kpw = 0.947 * Log Kow-0.017",null,"(Ghosh et al., 2014)"]
["Outer radius","Lo",2.835E-2,"cm",null,null,null,null,null,"3. The fitting process is to find parameters for the following correlation between sediment retardation factor R and Kow at given effective diffusivities D"]
["Sampling time","t",30,"days",null,null,null,null,null,null,"Log R = α * Log Kow + β"]
[null,null,null,null,null,null,null,null,null,"4. The fitted parameters (Row 28) is automatically derived by maximizing r2 from simulated results at different Ds  "]
["Number of PRCs",7,null,null,null,null,null,null,null,"5. The ‘Nonlinear’ in 'Option' is set to minimize the difference in Fss from calibrated to measurements, 'Linearized' is to minimuze the calibrated R values "]
["PRC #",{"$f":"PRCNumber(1,$B$11)","v":1},{"$f":"PRCNumber(2,$B$11)","v":2},{"$f":"PRCNumber(3,$B$11)","v":3},{"$f":"PRCNumber(4,$B$11)","v":4},{"$f":"PRCNumber(5,$B$11)","v":5},{"$f":"PRCNumber(6,$B$11)","v":6},{"$f":"PRCNumber(7,$B$11)","v":7},null,"6. The alpha value of the above correlation could be fixed to a given constant  ",null,null,null,{"$f":"PRCNumber(13,$B$11)","v":""},{"$f":"PRCNumber(14,$B$11)","v":""},{"$f":"PRCNumber(15,$B$11)","v":""},{"$f":"PRCNumber(16,$B$11)","v":""}]
["PRC name","13C-PCB28","13C-PCB47","13C-PCB70","13C-PCB80","13C-PCB111","13C-PCB141","13C-PCB182"]
["Log Kow",5.67,5.85,6.2,6.48,6.76,6.82,7.2,null,"Procedure"]
["Log Kpw",5.3524899999999995,5.5229499999999989,5.8543999999999992,6.1195599999999999,6.3847199999999988,6.4415399999999998,6.8013999999999992,null,"1. Update the properties of sampler and PRCs on this sheet in Green "]
["Measured PRC Fss",0.9,0.8,0.7,0.6,0.5,0.4,0.3,null,"2. Input a list of desired effective diffusivity (D) in column A starting row 33."]
[null,null,null,null,null,null,null,null,null,"3. Start the fitting by clicking on  \"Fit fss Data\""]
[null,null,null,null,null,null,null,null,null,"4. Check the fitted results (parameters in Row 28, results in the following figure), if it is not desired, change the list of D  "]
[null,null,null,null,null,null,null,null,null,"5. View model results in the following figure, the returned data are in cyl_fitted_plot"]
[]
[]
[null,null,null,null,null,null,null,null,null,"Database of frequently used PRCs"]
[null,null,null,null,null,null,null,null,null,"High sensitivity group"]
[null,null,null,null,null,null,null,null,null,"PRC name","13C-PCB28","13C-PCB47","13C-PCB70","13C-PCB80","13C-PCB111","13C-PCB141","13C-PCB182"]
[null,null,null,null,null,null,null,null,null,"Log Kow",5.67,5.85,6.2,6.48,6.76,6.82,7.2]
[null,null,null,null,null,null,null,null,null,"Log Kpw",{"$f":"K25*0.947-0.017","v":5.3524899999999995},5.5229499999999989,5.8543999999999992,6.1195599999999999,6.3847199999999988,6.4415399999999998,6.8013999999999992]
["Results"]
["Cylindrical diffusion model","Log R = α * Log Kow + β",null,null,null,null,null,null,null,"Low sensitivity group"]
["D",9.7017233784872537E-6,null,null,null,null,null,null,null,"PRC name","13C-PCB 37 ","13C-PCB 47 ","13C-PCB 54 ","13C-PCB 111","13C-PCB 138 ","13C-PCB 178 "]
["α",0.57015706235306285,null,null,null,null,null,null,null,"Log Kow",5.83,5.85,5.21,6.76,6.83,7.14]
["β",2.1388249670669328,null,null,null,null,null,null,null,"Log Kpw",{"$f":"K30*0.947-0.017","v":5.5040099999999992},5.5229499999999989,4.9168699999999994,6.3847199999999988,6.4510099999999992,6.7445799999999991]
["r2",0.99836701907003988]
[]
[]
["Model prediction"]
["Target Compound","Log Kow","Log Kpw","Log R","ξ","τ","ω","fss"]
["PCB 1",4.46,{"$f":"B37*0.947-0.017","v":4.2066199999999991},{"$f":"B37*$B$30+$B$31","v":4.6817254651615929},{"$f":"10^C37*($C$8^2-$C$7^2)/10^D37/$C$8^2","v":7.7583270825042988E-2},{"$f":"$B$29*$C$9*86400/10^D37/$C$8^2","v":0.65110689315923465},{"$f":"IF(E37>1,(1/E37-1/E37^2)^0.5,(1/E37^2-1/E37)^0.5)","v":12.379283257372267},{"$f":"IFERROR(IF(E37>1,1-(EXP((1/E37^2-G37^2)*F37)*((COS(G37/E37*F37*2)*(1-erfzR(1/E37*F37^0.5,G37*F37^0.5))-SIN(G37/E37*F37*2)*(-erfzI(1/E37*F37^0.5,G37*F37^0.5)))+(COS(G37/E37*F37*2)*(-erfzI(1/E37*F37^0.5,G37*F37^0.5))+SIN(G37/E37*F37*2)*(1-erfzR(1/E37*F37^0.5,G37*F37^0.5)))/E37/G37)),1-((1/E37+G37)*EXP((1/E37+G37)^2*F37)*ERFC((1/E37+G37)*F37^0.5)-(1/E37-G37)*EXP((1/E37-G37)^2*F37)*ERFC((1/E37-G37)*F37^0.5))/2/G37),1)","v":0.98547308306580683}]
["PCB 2",4.6900000000000004,{"$f":"B38*0.947-0.017","v":4.4244300000000001},{"$f":"B38*$B$30+$B$31","v":4.8128615895027984},{"$f":"10^C38*($C$8^2-$C$7^2)/10^D38/$C$8^2","v":9.4720059172053367E-2},{"$f":"$B$29*$C$9*86400/10^D38/$C$8^2","v":0.48141117665909922},{"$f":"IF(E38>1,(1/E38-1/E38^2)^0.5,(1/E38^2-1/E38)^0.5)","v":10.044989520646451},{"$f":"IFERROR(IF(E38>1,1-(EXP((1/E38^2-G38^2)*F38)*((COS(G38/E38*F38*2)*(1-erfzR(1/E38*F38^0.5,G38*F38^0.5))-SIN(G38/E38*F38*2)*(-erfzI(1/E38*F38^0.5,G38*F38^0.5)))+(COS(G38/E38*F38*2)*(-erfzI(1/E38*F38^0.5,G38*F38^0.5))+SIN(G38/E38*F38*2)*(1-erfzR(1/E38*F38^0.5,G38*F38^0.5)))/E38/G38)),1-((1/E38+G38)*EXP((1/E38+G38)^2*F38)*ERFC((1/E38+G38)*F38^0.5)-(1/E38-G38)*EXP((1/E38-G38)^2*F38)*ERFC((1/E38-G38)*F38^0.5))/2/G38),1)","v":0.97742655733166528}]
["PCB 3",4.6900000000000004,4.4244300000000001,4.8128615895027984,9.4720059172053367E-2,0.48141117665909922,10.044989520646451,{"$f":"IFERROR(IF(E39>1,1-(EXP((1/E39^2-G39^2)*F39)*((COS(G39/E39*F39*2)*(1-erfzR(1/E39*F39^0.5,G39*F39^0.5))-SIN(G39/E39*F39*2)*(-erfzI(1/E39*F39^0.5,G39*F39^0.5)))+(COS(G39/E39*F39*2)*(-erfzI(1/E39*F39^0.5,G39*F39^0.5))+SIN(G39/E39*F39*2)*(1-erfzR(1/E39*F39^0.5,G39*F39^0.5)))/E39/G39)),1-((1/E39+G39)*EXP((1/E39+G39)^2*F39)*ERFC((1/E39+G39)*F39^0.5)-(1/E39-G39)*EXP((1/E39-G39)^2*F39)*ERFC((1/E39-G39)*F39^0.5))/2/G39),1)","v":0.97742655733166528}]
["PCB 4",4.6500000000000004,4.3865499999999997,4.7900553070086751,9.1488865707056041E-2,0.50736727426386197,10.418300597780863,{"$f":"IFERROR(IF(E40>1,1-(EXP((1/E40^2-G40^2)*F40)*((COS(G40/E40*F40*2)*(1-erfzR(1/E40*F40^0.5,G40*F40^0.5))-SIN(G40/E40*F40*2)*(-erfzI(1/E40*F40^0.5,G40*F40^0.5)))+(COS(G40/E40*F40*2)*(-erfzI(1/E40*F40^0.5,G40*F40^0.5))+SIN(G40/E40*F40*2)*(1-erfzR(1/E40*F40^0.5,G40*F40^0.5)))/E40/G40)),1-((1/E40+G40)*EXP((1/E40+G40)^2*F40)*ERFC((1/E40+G40)*F40^0.5)-(1/E40-G40)*EXP((1/E40-G40)^2*F40)*ERFC((1/E40-G40)*F40^0.5))/2/G40),1)","v":0.97907768451949506}]
["PCB 5",4.97,4.689589999999999,4.9725055669616545,0.12076969881550623,0.33332830306216588,7.7641396854312621,{"$f":"IFERROR(IF(E41>1,1-(EXP((1/E41^2-G41^2)*F41)*((COS(G41/E41*F41*2)*(1-erfzR(1/E41*F41^0.5,G41*F41^0.5))-SIN(G41/E41*F41*2)*(-erfzI(1/E41*F41^0.5,G41*F41^0.5)))+(COS(G41/E41*F41*2)*(-erfzI(1/E41*F41^0.5,G41*F41^0.5))+SIN(G41/E41*F41*2)*(1-erfzR(1/E41*F41^0.5,G41*F41^0.5)))/E41/G41)),1-((1/E41+G41)*EXP((1/E41+G41)^2*F41)*ERFC((1/E41+G41)*F41^0.5)-(1/E41-G41)*EXP((1/E41-G41)^2*F41)*ERFC((1/E41-G41)*F41^0.5))/2/G41),1)","v":0.96189049949396599}]
["PCB 6",5.0599999999999996,{"$f":"B42*0.947-0.017","v":4.7748199999999992},{"$f":"B42*$B$30+$B$31","v":5.0238197025734301},0.13057915311486903,0.29618158695379604,7.1407064046958029,{"$f":"IFERROR(IF(E42>1,1-(EXP((1/E42^2-G42^2)*F42)*((COS(G42/E42*F42*2)*(1-erfzR(1/E42*F42^0.5,G42*F42^0.5))-SIN(G42/E42*F42*2)*(-erfzI(1/E42*F42^0.5,G42*F42^0.5)))+(COS(G42/E42*F42*2)*(-erfzI(1/E42*F42^0.5,G42*F42^0.5))+SIN(G42/E42*F42*2)*(1-erfzR(1/E42*F42^0.5,G42*F42^0.5)))/E42/G42)),1-((1/E42+G42)*EXP((1/E42+G42)^2*F42)*ERFC((1/E42+G42)*F42^0.5)-(1/E42-G42)*EXP((1/E42-G42)^2*F42)*ERFC((1/E42-G42)*F42^0.5))/2/G42),1)","v":0.95503973325470815}]
["PCB 7",5.07,4.7842899999999995,5.029521273196961,0.1317171353806573,0.29231862361832511,7.074379250593485,{"$f":"IFERROR(IF(E43>1,1-(EXP((1/E43^2-G43^2)*F43)*((COS(G43/E43*F43*2)*(1-erfzR(1/E43*F43^0.5,G43*F43^0.5))-SIN(G43/E43*F43*2)*(-erfzI(1/E43*F43^0.5,G43*F43^0.5)))+(COS(G43/E43*F43*2)*(-erfzI(1/E43*F43^0.5,G43*F43^0.5))+SIN(G43/E43*F43*2)*(1-erfzR(1/E43*F43^0.5,G43*F43^0.5)))/E43/G43)),1-((1/E43+G43)*EXP((1/E43+G43)^2*F43)*ERFC((1/E43+G43)*F43^0.5)-(1/E43-G43)*EXP((1/E43-G43)^2*F43)*ERFC((1/E43-G43)*F43^0.5))/2/G43),1)","v":0.95421056414984029}]
["PCB 8",5.07,4.7842899999999995,5.029521273196961,0.1317171353806573,0.29231862361832511,7.074379250593485,{"$f":"IFERROR(IF(E44>1,1-(EXP((1/E44^2-G44^2)*F44)*((COS(G44/E44*F44*2)*(1-erfzR(1/E44*F44^0.5,G44*F44^0.5))-SIN(G44/E44*F44*2)*(-erfzI(1/E44*F44^0.5,G44*F44^0.5)))+(COS(G44/E44*F44*2)*(-erfzI(1/E44*F44^0.5,G44*F44^0.5))+SIN(G44/E44*F44*2)*(1-erfzR(1/E44*F44^0.5,G44*F44^0.5)))/E44/G44)),1-((1/E44+G44)*EXP((1/E44+G44)^2*F44)*ERFC((1/E44+G44)*F44^0.5)-(1/E44-G44)*EXP((1/E44-G44)^2*F44)*ERFC((1/E44-G44)*F44^0.5))/2/G44),1)","v":0.95421056414984029}]
["PCB 9",5.0599999999999996,4.7748199999999992,5.0238197025734301,0.13057915311486903,0.29618158695379604,7.1407064046958029,{"$f":"IFERROR(IF(E45>1,1-(EXP((1/E45^2-G45^2)*F45)*((COS(G45/E45*F45*2)*(1-erfzR(1/E45*F45^0.5,G45*F45^0.5))-SIN(G45/E45*F45*2)*(-erfzI(1/E45*F45^0.5,G45*F45^0.5)))+(COS(G45/E45*F45*2)*(-erfzI(1/E45*F45^0.5,G45*F45^0.5))+SIN(G45/E45*F45*2)*(1-erfzR(1/E45*F45^0.5,G45*F45^0.5)))/E45/G45)),1-((1/E45+G45)*EXP((1/E45+G45)^2*F45)*ERFC((1/E45+G45)*F45^0.5)-(1/E45-G45)*EXP((1/E45-G45)^2*F45)*ERFC((1/E45-G45)*F45^0.5))/2/G45),1)","v":0.95503973325470815}]
["PCB 10",4.84,4.5664799999999994,4.8983851488557573,0.10788682224083178,0.39535989205229688,8.7547061961696873,{"$f":"IFERROR(IF(E46>1,1-(EXP((1/E46^2-G46^2)*F46)*((COS(G46/E46*F46*2)*(1-erfzR(1/E46*F46^0.5,G46*F46^0.5))-SIN(G46/E46*F46*2)*(-erfzI(1/E46*F46^0.5,G46*F46^0.5)))+(COS(G46/E46*F46*2)*(-erfzI(1/E46*F46^0.5,G46*F46^0.5))+SIN(G46/E46*F46*2)*(1-erfzR(1/E46*F46^0.5,G46*F46^0.5)))/E46/G46)),1-((1/E46+G46)*EXP((1/E46+G46)^2*F46)*ERFC((1/E46+G46)*F46^0.5)-(1/E46-G46)*EXP((1/E46-G46)^2*F46)*ERFC((1/E46-G46)*F46^0.5))/2/G46),1)","v":0.97006394127933426}]
["PCB 11",5.28,4.9831599999999998,5.1492542562911048,0.15804446617339654,0.22188273068140354,5.8058429516337897,{"$f":"IFERROR(IF(E47>1,1-(EXP((1/E47^2-G47^2)*F47)*((COS(G47/E47*F47*2)*(1-erfzR(1/E47*F47^0.5,G47*F47^0.5))-SIN(G47/E47*F47*2)*(-erfzI(1/E47*F47^0.5,G47*F47^0.5)))+(COS(G47/E47*F47*2)*(-erfzI(1/E47*F47^0.5,G47*F47^0.5))+SIN(G47/E47*F47*2)*(1-erfzR(1/E47*F47^0.5,G47*F47^0.5)))/E47/G47)),1-((1/E47+G47)*EXP((1/E47+G47)^2*F47)*ERFC((1/E47+G47)*F47^0.5)-(1/E47-G47)*EXP((1/E47-G47)^2*F47)*ERFC((1/E47-G47)*F47^0.5))/2/G47),1)","v":0.93310449223805336}]
["PCB 12",5.22,4.9263399999999988,5.1150448325499207,0.15002675563231982,0.24006725452586639,6.1451701161600631,{"$f":"IFERROR(IF(E48>1,1-(EXP((1/E48^2-G48^2)*F48)*((COS(G48/E48*F48*2)*(1-erfzR(1/E48*F48^0.5,G48*F48^0.5))-SIN(G48/E48*F48*2)*(-erfzI(1/E48*F48^0.5,G48*F48^0.5)))+(COS(G48/E48*F48*2)*(-erfzI(1/E48*F48^0.5,G48*F48^0.5))+SIN(G48/E48*F48*2)*(1-erfzR(1/E48*F48^0.5,G48*F48^0.5)))/E48/G48)),1-((1/E48+G48)*EXP((1/E48+G48)^2*F48)*ERFC((1/E48+G48)*F48^0.5)-(1/E48-G48)*EXP((1/E48-G48)^2*F48)*ERFC((1/E48-G48)*F48^0.5))/2/G48),1)","v":0.93991383568202724}]
["PCB 13",5.29,4.9926299999999992,5.1549558269146356,0.15942180547619514,0.21898881393859759,5.7509731053677582,{"$f":"IFERROR(IF(E49>1,1-(EXP((1/E49^2-G49^2)*F49)*((COS(G49/E49*F49*2)*(1-erfzR(1/E49*F49^0.5,G49*F49^0.5))-SIN(G49/E49*F49*2)*(-erfzI(1/E49*F49^0.5,G49*F49^0.5)))+(COS(G49/E49*F49*2)*(-erfzI(1/E49*F49^0.5,G49*F49^0.5))+SIN(G49/E49*F49*2)*(1-erfzR(1/E49*F49^0.5,G49*F49^0.5)))/E49/G49)),1-((1/E49+G49)*EXP((1/E49+G49)^2*F49)*ERFC((1/E49+G49)*F49^0.5)-(1/E49-G49)*EXP((1/E49-G49)^2*F49)*ERFC((1/E49-G49)*F49^0.5))/2/G49),1)","v":0.93190228756044513}]
["PCB 14",5.28,4.9831599999999998,5.1492542562911048,0.15804446617339654,0.22188273068140354,5.8058429516337897,{"$f":"IFERROR(IF(E50>1,1-(EXP((1/E50^2-G50^2)*F50)*((COS(G50/E50*F50*2)*(1-erfzR(1/E50*F50^0.5,G50*F50^0.5))-SIN(G50/E50*F50*2)*(-erfzI(1/E50*F50^0.5,G50*F50^0.5)))+(COS(G50/E50*F50*2)*(-erfzI(1/E50*F50^0.5,G50*F50^0.5))+SIN(G50/E50*F50*2)*(1-erfzR(1/E50*F50^0.5,G50*F50^0.5)))/E50/G50)),1-((1/E50+G50)*EXP((1/E50+G50)^2*F50)*ERFC((1/E50+G50)*F50^0.5)-(1/E50-G50)*EXP((1/E50-G50)^2*F50)*ERFC((1/E50-G50)*F50^0.5))/2/G50),1)","v":0.93310449223805336}]
["PCB 15",5.3,5.0020999999999995,5.1606573975381664,0.16081114813223382,0.2161326412513504,5.6965734351421169,{"$f":"IFERROR(IF(E51>1,1-(EXP((1/E51^2-G51^2)*F51)*((COS(G51/E51*F51*2)*(1-erfzR(1/E51*F51^0.5,G51*F51^0.5))-SIN(G51/E51*F51*2)*(-erfzI(1/E51*F51^0.5,G51*F51^0.5)))+(COS(G51/E51*F51*2)*(-erfzI(1/E51*F51^0.5,G51*F51^0.5))+SIN(G51/E51*F51*2)*(1-erfzR(1/E51*F51^0.5,G51*F51^0.5)))/E51/G51)),1-((1/E51+G51)*EXP((1/E51+G51)^2*F51)*ERFC((1/E51+G51)*F51^0.5)-(1/E51-G51)*EXP((1/E51-G51)^2*F51)*ERFC((1/E51-G51)*F51^0.5))/2/G51),1)","v":0.93068011826472063}]
["PCB 16",5.16,4.8695199999999996,5.0808354088087366,0.14241578936946439,0.25974210123788333,6.5024982926608654,{"$f":"IFERROR(IF(E52>1,1-(EXP((1/E52^2-G52^2)*F52)*((COS(G52/E52*F52*2)*(1-erfzR(1/E52*F52^0.5,G52*F52^0.5))-SIN(G52/E52*F52*2)*(-erfzI(1/E52*F52^0.5,G52*F52^0.5)))+(COS(G52/E52*F52*2)*(-erfzI(1/E52*F52^0.5,G52*F52^0.5))+SIN(G52/E52*F52*2)*(1-erfzR(1/E52*F52^0.5,G52*F52^0.5)))/E52/G52)),1-((1/E52+G52)*EXP((1/E52+G52)^2*F52)*ERFC((1/E52+G52)*F52^0.5)-(1/E52-G52)*EXP((1/E52-G52)^2*F52)*ERFC((1/E52-G52)*F52^0.5))/2/G52),1)","v":0.94607248516080833}]
["PCB 17",5.25,4.9547499999999998,5.1321495444205123,0.15398343581579393,0.23079596612893147,5.9733151328274703,{"$f":"IFERROR(IF(E53>1,1-(EXP((1/E53^2-G53^2)*F53)*((COS(G53/E53*F53*2)*(1-erfzR(1/E53*F53^0.5,G53*F53^0.5))-SIN(G53/E53*F53*2)*(-erfzI(1/E53*F53^0.5,G53*F53^0.5)))+(COS(G53/E53*F53*2)*(-erfzI(1/E53*F53^0.5,G53*F53^0.5))+SIN(G53/E53*F53*2)*(1-erfzR(1/E53*F53^0.5,G53*F53^0.5)))/E53/G53)),1-((1/E53+G53)*EXP((1/E53+G53)^2*F53)*ERFC((1/E53+G53)*F53^0.5)-(1/E53-G53)*EXP((1/E53-G53)^2*F53)*ERFC((1/E53-G53)*F53^0.5))/2/G53),1)","v":0.93659407843461451}]
["PCB 18",5.24,4.9452799999999995,5.1264479737969824,0.15265308180621742,0.23384591328623131,6.0301074482430748,{"$f":"IFERROR(IF(E54>1,1-(EXP((1/E54^2-G54^2)*F54)*((COS(G54/E54*F54*2)*(1-erfzR(1/E54*F54^0.5,G54*F54^0.5))-SIN(G54/E54*F54*2)*(-erfzI(1/E54*F54^0.5,G54*F54^0.5)))+(COS(G54/E54*F54*2)*(-erfzI(1/E54*F54^0.5,G54*F54^0.5))+SIN(G54/E54*F54*2)*(1-erfzR(1/E54*F54^0.5,G54*F54^0.5)))/E54/G54)),1-((1/E54+G54)*EXP((1/E54+G54)^2*F54)*ERFC((1/E54+G54)*F54^0.5)-(1/E54-G54)*EXP((1/E54-G54)^2*F54)*ERFC((1/E54-G54)*F54^0.5))/2/G54),1)","v":0.93771917478489542}]
["PCB 19",5.0199999999999996,4.7369399999999988,5.0010134200793086,0.12612469531682982,0.31215071802602623,7.411815553680281,{"$f":"IFERROR(IF(E55>1,1-(EXP((1/E55^2-G55^2)*F55)*((COS(G55/E55*F55*2)*(1-erfzR(1/E55*F55^0.5,G55*F55^0.5))-SIN(G55/E55*F55*2)*(-erfzI(1/E55*F55^0.5,G55*F55^0.5)))+(COS(G55/E55*F55*2)*(-erfzI(1/E55*F55^0.5,G55*F55^0.5))+SIN(G55/E55*F55*2)*(1-erfzR(1/E55*F55^0.5,G55*F55^0.5)))/E55/G55)),1-((1/E55+G55)*EXP((1/E55+G55)^2*F55)*ERFC((1/E55+G55)*F55^0.5)-(1/E55-G55)*EXP((1/E55-G55)^2*F55)*ERFC((1/E55-G55)*F55^0.5))/2/G55),1)","v":0.95821688991753184}]
["PCB 20",5.57,5.25779,5.3145998043734934,0.20326553425195593,0.1516274928353788,4.3912994815196011,{"$f":"IFERROR(IF(E56>1,1-(EXP((1/E56^2-G56^2)*F56)*((COS(G56/E56*F56*2)*(1-erfzR(1/E56*F56^0.5,G56*F56^0.5))-SIN(G56/E56*F56*2)*(-erfzI(1/E56*F56^0.5,G56*F56^0.5)))+(COS(G56/E56*F56*2)*(-erfzI(1/E56*F56^0.5,G56*F56^0.5))+SIN(G56/E56*F56*2)*(1-erfzR(1/E56*F56^0.5,G56*F56^0.5)))/E56/G56)),1-((1/E56+G56)*EXP((1/E56+G56)^2*F56)*ERFC((1/E56+G56)*F56^0.5)-(1/E56-G56)*EXP((1/E56-G56)^2*F56)*ERFC((1/E56-G56)*F56^0.5))/2/G56),1)","v":0.88908959856720382}]
["PCB 21",5.51,5.200969999999999,5.2803903806323085,0.19295372608765474,0.16405420919349067,4.6558185766796889,{"$f":"IFERROR(IF(E57>1,1-(EXP((1/E57^2-G57^2)*F57)*((COS(G57/E57*F57*2)*(1-erfzR(1/E57*F57^0.5,G57*F57^0.5))-SIN(G57/E57*F57*2)*(-erfzI(1/E57*F57^0.5,G57*F57^0.5)))+(COS(G57/E57*F57*2)*(-erfzI(1/E57*F57^0.5,G57*F57^0.5))+SIN(G57/E57*F57*2)*(1-erfzR(1/E57*F57^0.5,G57*F57^0.5)))/E57/G57)),1-((1/E57+G57)*EXP((1/E57+G57)^2*F57)*ERFC((1/E57+G57)*F57^0.5)-(1/E57-G57)*EXP((1/E57-G57)^2*F57)*ERFC((1/E57-G57)*F57^0.5))/2/G57),1)","v":0.8998976477866899}]
["PCB 22",5.58,5.2672599999999994,5.3203013749970234,0.20503696994982129,0.14964988358729364,4.3485181880376391,{"$f":"IFERROR(IF(E58>1,1-(EXP((1/E58^2-G58^2)*F58)*((COS(G58/E58*F58*2)*(1-erfzR(1/E58*F58^0.5,G58*F58^0.5))-SIN(G58/E58*F58*2)*(-erfzI(1/E58*F58^0.5,G58*F58^0.5)))+(COS(G58/E58*F58*2)*(-erfzI(1/E58*F58^0.5,G58*F58^0.5))+SIN(G58/E58*F58*2)*(1-erfzR(1/E58*F58^0.5,G58*F58^0.5)))/E58/G58)),1-((1/E58+G58)*EXP((1/E58+G58)^2*F58)*ERFC((1/E58+G58)*F58^0.5)-(1/E58-G58)*EXP((1/E58-G58)^2*F58)*ERFC((1/E58-G58)*F58^0.5))/2/G58),1)","v":0.88719191437622991}]
["PCB 23",5.57,5.25779,5.3145998043734934,0.20326553425195593,0.1516274928353788,4.3912994815196011,{"$f":"IFERROR(IF(E59>1,1-(EXP((1/E59^2-G59^2)*F59)*((COS(G59/E59*F59*2)*(1-erfzR(1/E59*F59^0.5,G59*F59^0.5))-SIN(G59/E59*F59*2)*(-erfzI(1/E59*F59^0.5,G59*F59^0.5)))+(COS(G59/E59*F59*2)*(-erfzI(1/E59*F59^0.5,G59*F59^0.5))+SIN(G59/E59*F59*2)*(1-erfzR(1/E59*F59^0.5,G59*F59^0.5)))/E59/G59)),1-((1/E59+G59)*EXP((1/E59+G59)^2*F59)*ERFC((1/E59+G59)*F59^0.5)-(1/E59-G59)*EXP((1/E59-G59)^2*F59)*ERFC((1/E59-G59)*F59^0.5))/2/G59),1)","v":0.88908959856720382}]
["PCB 24",5.51,5.200969999999999,5.2803903806323085,0.19295372608765474,0.16405420919349067,4.6558185766796889,{"$f":"IFERROR(IF(E60>1,1-(EXP((1/E60^2-G60^2)*F60)*((COS(G60/E60*F60*2)*(1-erfzR(1/E60*F60^0.5,G60*F60^0.5))-SIN(G60/E60*F60*2)*(-erfzI(1/E60*F60^0.5,G60*F60^0.5)))+(COS(G60/E60*F60*2)*(-erfzI(1/E60*F60^0.5,G60*F60^0.5))+SIN(G60/E60*F60*2)*(1-erfzR(1/E60*F60^0.5,G60*F60^0.5)))/E60/G60)),1-((1/E60+G60)*EXP((1/E60+G60)^2*F60)*ERFC((1/E60+G60)*F60^0.5)-(1/E60-G60)*EXP((1/E60-G60)^2*F60)*ERFC((1/E60-G60)*F60^0.5))/2/G60),1)","v":0.8998976477866899}]
["PCB 25",5.58,5.2672599999999994,5.3203013749970234,0.20503696994982129,0.14964988358729364,4.3485181880376391,{"$f":"IFERROR(IF(E61>1,1-(EXP((1/E61^2-G61^2)*F61)*((COS(G61/E61*F61*2)*(1-erfzR(1/E61*F61^0.5,G61*F61^0.5))-SIN(G61/E61*F61*2)*(-erfzI(1/E61*F61^0.5,G61*F61^0.5)))+(COS(G61/E61*F61*2)*(-erfzI(1/E61*F61^0.5,G61*F61^0.5))+SIN(G61/E61*F61*2)*(1-erfzR(1/E61*F61^0.5,G61*F61^0.5)))/E61/G61)),1-((1/E61+G61)*EXP((1/E61+G61)^2*F61)*ERFC((1/E61+G61)*F61^0.5)-(1/E61-G61)*EXP((1/E61-G61)^2*F61)*ERFC((1/E61-G61)*F61^0.5))/2/G61),1)","v":0.88719191437622991}]
["PCB 26",5.57,5.25779,5.3145998043734934,0.20326553425195593,0.1516274928353788,4.3912994815196011,{"$f":"IFERROR(IF(E62>1,1-(EXP((1/E62^2-G62^2)*F62)*((COS(G62/E62*F62*2)*(1-erfzR(1/E62*F62^0.5,G62*F62^0.5))-SIN(G62/E62*F62*2)*(-erfzI(1/E62*F62^0.5,G62*F62^0.5)))+(COS(G62/E62*F62*2)*(-erfzI(1/E62*F62^0.5,G62*F62^0.5))+SIN(G62/E62*F62*2)*(1-erfzR(1/E62*F62^0.5,G62*F62^0.5)))/E62/G62)),1-((1/E62+G62)*EXP((1/E62+G62)^2*F62)*ERFC((1/E62+G62)*F62^0.5)-(1/E62-G62)*EXP((1/E62-G62)^2*F62)*ERFC((1/E62-G62)*F62^0.5))/2/G62),1)","v":0.88908959856720382}]
["PCB 27",5.35,5.0494499999999993,5.1891652506558188,0.16794160506032091,0.20240093186112787,5.4314852417533359,{"$f":"IFERROR(IF(E63>1,1-(EXP((1/E63^2-G63^2)*F63)*((COS(G63/E63*F63*2)*(1-erfzR(1/E63*F63^0.5,G63*F63^0.5))-SIN(G63/E63*F63*2)*(-erfzI(1/E63*F63^0.5,G63*F63^0.5)))+(COS(G63/E63*F63*2)*(-erfzI(1/E63*F63^0.5,G63*F63^0.5))+SIN(G63/E63*F63*2)*(1-erfzR(1/E63*F63^0.5,G63*F63^0.5)))/E63/G63)),1-((1/E63+G63)*EXP((1/E63+G63)^2*F63)*ERFC((1/E63+G63)*F63^0.5)-(1/E63-G63)*EXP((1/E63-G63)^2*F63)*ERFC((1/E63-G63)*F63^0.5))/2/G63),1)","v":0.92425998873998227}]
["PCB 28",5.67,5.3524899999999995,5.371615510608799,0.2216909883512016,0.1329726266901167,3.979495243060899,{"$f":"IFERROR(IF(E64>1,1-(EXP((1/E64^2-G64^2)*F64)*((COS(G64/E64*F64*2)*(1-erfzR(1/E64*F64^0.5,G64*F64^0.5))-SIN(G64/E64*F64*2)*(-erfzI(1/E64*F64^0.5,G64*F64^0.5)))+(COS(G64/E64*F64*2)*(-erfzI(1/E64*F64^0.5,G64*F64^0.5))+SIN(G64/E64*F64*2)*(1-erfzR(1/E64*F64^0.5,G64*F64^0.5)))/E64/G64)),1-((1/E64+G64)*EXP((1/E64+G64)^2*F64)*ERFC((1/E64+G64)*F64^0.5)-(1/E64-G64)*EXP((1/E64-G64)^2*F64)*ERFC((1/E64-G64)*F64^0.5))/2/G64),1)","v":0.86880973286601093}]
["PCB 29",5.66,5.3430199999999992,5.3659139399852691,0.21977566873466342,0.13472984754442599,4.0191122391204637,{"$f":"IFERROR(IF(E65>1,1-(EXP((1/E65^2-G65^2)*F65)*((COS(G65/E65*F65*2)*(1-erfzR(1/E65*F65^0.5,G65*F65^0.5))-SIN(G65/E65*F65*2)*(-erfzI(1/E65*F65^0.5,G65*F65^0.5)))+(COS(G65/E65*F65*2)*(-erfzI(1/E65*F65^0.5,G65*F65^0.5))+SIN(G65/E65*F65*2)*(1-erfzR(1/E65*F65^0.5,G65*F65^0.5)))/E65/G65)),1-((1/E65+G65)*EXP((1/E65+G65)^2*F65)*ERFC((1/E65+G65)*F65^0.5)-(1/E65-G65)*EXP((1/E65-G65)^2*F65)*ERFC((1/E65-G65)*F65^0.5))/2/G65),1)","v":0.87097106773532407}]
["PCB 30",5.44,5.1346799999999995,5.2404793862675945,0.18158257225621971,0.17984500160604688,4.9821095229762751,{"$f":"IFERROR(IF(E66>1,1-(EXP((1/E66^2-G66^2)*F66)*((COS(G66/E66*F66*2)*(1-erfzR(1/E66*F66^0.5,G66*F66^0.5))-SIN(G66/E66*F66*2)*(-erfzI(1/E66*F66^0.5,G66*F66^0.5)))+(COS(G66/E66*F66*2)*(-erfzI(1/E66*F66^0.5,G66*F66^0.5))+SIN(G66/E66*F66*2)*(1-erfzR(1/E66*F66^0.5,G66*F66^0.5)))/E66/G66)),1-((1/E66+G66)*EXP((1/E66+G66)^2*F66)*ERFC((1/E66+G66)*F66^0.5)-(1/E66-G66)*EXP((1/E66-G66)^2*F66)*ERFC((1/E66-G66)*F66^0.5))/2/G66),1)","v":0.91131470586037977}]
["PCB 31",5.67,5.3524899999999995,5.371615510608799,0.2216909883512016,0.1329726266901167,3.979495243060899,{"$f":"IFERROR(IF(E67>1,1-(EXP((1/E67^2-G67^2)*F67)*((COS(G67/E67*F67*2)*(1-erfzR(1/E67*F67^0.5,G67*F67^0.5))-SIN(G67/E67*F67*2)*(-erfzI(1/E67*F67^0.5,G67*F67^0.5)))+(COS(G67/E67*F67*2)*(-erfzI(1/E67*F67^0.5,G67*F67^0.5))+SIN(G67/E67*F67*2)*(1-erfzR(1/E67*F67^0.5,G67*F67^0.5)))/E67/G67)),1-((1/E67+G67)*EXP((1/E67+G67)^2*F67)*ERFC((1/E67+G67)*F67^0.5)-(1/E67-G67)*EXP((1/E67-G67)^2*F67)*ERFC((1/E67-G67)*F67^0.5))/2/G67),1)","v":0.86880973286601093}]
["PCB 32",5.44,5.1346799999999995,5.2404793862675945,0.18158257225621971,0.17984500160604688,4.9821095229762751,{"$f":"IFERROR(IF(E68>1,1-(EXP((1/E68^2-G68^2)*F68)*((COS(G68/E68*F68*2)*(1-erfzR(1/E68*F68^0.5,G68*F68^0.5))-SIN(G68/E68*F68*2)*(-erfzI(1/E68*F68^0.5,G68*F68^0.5)))+(COS(G68/E68*F68*2)*(-erfzI(1/E68*F68^0.5,G68*F68^0.5))+SIN(G68/E68*F68*2)*(1-erfzR(1/E68*F68^0.5,G68*F68^0.5)))/E68/G68)),1-((1/E68+G68)*EXP((1/E68+G68)^2*F68)*ERFC((1/E68+G68)*F68^0.5)-(1/E68-G68)*EXP((1/E68-G68)^2*F68)*ERFC((1/E68-G68)*F68^0.5))/2/G68),1)","v":0.91131470586037977}]
["PCB 33",5.6,5.2861999999999991,5.3317045162440841,0.20862628945837342,0.14577170788979199,4.2640449626419219,{"$f":"IFERROR(IF(E69>1,1-(EXP((1/E69^2-G69^2)*F69)*((COS(G69/E69*F69*2)*(1-erfzR(1/E69*F69^0.5,G69*F69^0.5))-SIN(G69/E69*F69*2)*(-erfzI(1/E69*F69^0.5,G69*F69^0.5)))+(COS(G69/E69*F69*2)*(-erfzI(1/E69*F69^0.5,G69*F69^0.5))+SIN(G69/E69*F69*2)*(1-erfzR(1/E69*F69^0.5,G69*F69^0.5)))/E69/G69)),1-((1/E69+G69)*EXP((1/E69+G69)^2*F69)*ERFC((1/E69+G69)*F69^0.5)-(1/E69-G69)*EXP((1/E69-G69)^2*F69)*ERFC((1/E69-G69)*F69^0.5))/2/G69),1)","v":0.88331149969031919}]
["PCB 34",5.66,5.3430199999999992,5.3659139399852691,0.21977566873466342,0.13472984754442599,4.0191122391204637,{"$f":"IFERROR(IF(E70>1,1-(EXP((1/E70^2-G70^2)*F70)*((COS(G70/E70*F70*2)*(1-erfzR(1/E70*F70^0.5,G70*F70^0.5))-SIN(G70/E70*F70*2)*(-erfzI(1/E70*F70^0.5,G70*F70^0.5)))+(COS(G70/E70*F70*2)*(-erfzI(1/E70*F70^0.5,G70*F70^0.5))+SIN(G70/E70*F70*2)*(1-erfzR(1/E70*F70^0.5,G70*F70^0.5)))/E70/G70)),1-((1/E70+G70)*EXP((1/E70+G70)^2*F70)*ERFC((1/E70+G70)*F70^0.5)-(1/E70-G70)*EXP((1/E70-G70)^2*F70)*ERFC((1/E70-G70)*F70^0.5))/2/G70),1)","v":0.87097106773532407}]
["PCB 35",5.82,5.4945399999999998,5.4571390699617588,0.25250761519474618,0.10920403572462682,3.4239617630172368,{"$f":"IFERROR(IF(E71>1,1-(EXP((1/E71^2-G71^2)*F71)*((COS(G71/E71*F71*2)*(1-erfzR(1/E71*F71^0.5,G71*F71^0.5))-SIN(G71/E71*F71*2)*(-erfzI(1/E71*F71^0.5,G71*F71^0.5)))+(COS(G71/E71*F71*2)*(-erfzI(1/E71*F71^0.5,G71*F71^0.5))+SIN(G71/E71*F71*2)*(1-erfzR(1/E71*F71^0.5,G71*F71^0.5)))/E71/G71)),1-((1/E71+G71)*EXP((1/E71+G71)^2*F71)*ERFC((1/E71+G71)*F71^0.5)-(1/E71-G71)*EXP((1/E71-G71)^2*F71)*ERFC((1/E71-G71)*F71^0.5))/2/G71),1)","v":0.83261386612820532}]
["PCB 36",5.88,5.551359999999999,5.491348493702942,0.26600209462620605,0.10093208961740778,3.220789589587659,{"$f":"IFERROR(IF(E72>1,1-(EXP((1/E72^2-G72^2)*F72)*((COS(G72/E72*F72*2)*(1-erfzR(1/E72*F72^0.5,G72*F72^0.5))-SIN(G72/E72*F72*2)*(-erfzI(1/E72*F72^0.5,G72*F72^0.5)))+(COS(G72/E72*F72*2)*(-erfzI(1/E72*F72^0.5,G72*F72^0.5))+SIN(G72/E72*F72*2)*(1-erfzR(1/E72*F72^0.5,G72*F72^0.5)))/E72/G72)),1-((1/E72+G72)*EXP((1/E72+G72)^2*F72)*ERFC((1/E72+G72)*F72^0.5)-(1/E72-G72)*EXP((1/E72-G72)^2*F72)*ERFC((1/E72-G72)*F72^0.5))/2/G72),1)","v":0.81607880376963193}]
["PCB 37",5.83,5.5040099999999992,5.4628406405852896,0.25470818995123329,0.10777973656265528,3.389380018442675,{"$f":"IFERROR(IF(E73>1,1-(EXP((1/E73^2-G73^2)*F73)*((COS(G73/E73*F73*2)*(1-erfzR(1/E73*F73^0.5,G73*F73^0.5))-SIN(G73/E73*F73*2)*(-erfzI(1/E73*F73^0.5,G73*F73^0.5)))+(COS(G73/E73*F73*2)*(-erfzI(1/E73*F73^0.5,G73*F73^0.5))+SIN(G73/E73*F73*2)*(1-erfzR(1/E73*F73^0.5,G73*F73^0.5)))/E73/G73)),1-((1/E73+G73)*EXP((1/E73+G73)^2*F73)*ERFC((1/E73+G73)*F73^0.5)-(1/E73-G73)*EXP((1/E73-G73)^2*F73)*ERFC((1/E73-G73)*F73^0.5))/2/G73),1)","v":0.82994125749316572}]
["PCB 38",5.76,5.4377199999999988,5.4229296462205747,0.2396977205045526,0.11815391382215863,3.6377197864796025,{"$f":"IFERROR(IF(E74>1,1-(EXP((1/E74^2-G74^2)*F74)*((COS(G74/E74*F74*2)*(1-erfzR(1/E74*F74^0.5,G74*F74^0.5))-SIN(G74/E74*F74*2)*(-erfzI(1/E74*F74^0.5,G74*F74^0.5)))+(COS(G74/E74*F74*2)*(-erfzI(1/E74*F74^0.5,G74*F74^0.5))+SIN(G74/E74*F74*2)*(1-erfzR(1/E74*F74^0.5,G74*F74^0.5)))/E74/G74)),1-((1/E74+G74)*EXP((1/E74+G74)^2*F74)*ERFC((1/E74+G74)*F74^0.5)-(1/E74-G74)*EXP((1/E74-G74)^2*F74)*ERFC((1/E74-G74)*F74^0.5))/2/G74),1)","v":0.84795865954826288}]
["PCB 39",5.89,5.5608299999999993,5.4970500643264728,0.2683202722152494,9.9615677731123523E-2,3.1879171446560099,{"$f":"IFERROR(IF(E75>1,1-(EXP((1/E75^2-G75^2)*F75)*((COS(G75/E75*F75*2)*(1-erfzR(1/E75*F75^0.5,G75*F75^0.5))-SIN(G75/E75*F75*2)*(-erfzI(1/E75*F75^0.5,G75*F75^0.5)))+(COS(G75/E75*F75*2)*(-erfzI(1/E75*F75^0.5,G75*F75^0.5))+SIN(G75/E75*F75*2)*(1-erfzR(1/E75*F75^0.5,G75*F75^0.5)))/E75/G75)),1-((1/E75+G75)*EXP((1/E75+G75)^2*F75)*ERFC((1/E75+G75)*F75^0.5)-(1/E75-G75)*EXP((1/E75-G75)^2*F75)*ERFC((1/E75-G75)*F75^0.5))/2/G75),1)","v":0.81320599742131394}]
["PCB 40",5.66,5.3430199999999992,5.3659139399852691,0.21977566873466342,0.13472984754442599,4.0191122391204637,{"$f":"IFERROR(IF(E76>1,1-(EXP((1/E76^2-G76^2)*F76)*((COS(G76/E76*F76*2)*(1-erfzR(1/E76*F76^0.5,G76*F76^0.5))-SIN(G76/E76*F76*2)*(-erfzI(1/E76*F76^0.5,G76*F76^0.5)))+(COS(G76/E76*F76*2)*(-erfzI(1/E76*F76^0.5,G76*F76^0.5))+SIN(G76/E76*F76*2)*(1-erfzR(1/E76*F76^0.5,G76*F76^0.5)))/E76/G76)),1-((1/E76+G76)*EXP((1/E76+G76)^2*F76)*ERFC((1/E76+G76)*F76^0.5)-(1/E76-G76)*EXP((1/E76-G76)^2*F76)*ERFC((1/E76-G76)*F76^0.5))/2/G76),1)","v":0.87097106773532407}]
["PCB 41",5.69,5.3714300000000001,5.3830186518558607,0.22557184842026129,0.129526641989689,3.9012669410362073,{"$f":"IFERROR(IF(E77>1,1-(EXP((1/E77^2-G77^2)*F77)*((COS(G77/E77*F77*2)*(1-erfzR(1/E77*F77^0.5,G77*F77^0.5))-SIN(G77/E77*F77*2)*(-erfzI(1/E77*F77^0.5,G77*F77^0.5)))+(COS(G77/E77*F77*2)*(-erfzI(1/E77*F77^0.5,G77*F77^0.5))+SIN(G77/E77*F77*2)*(1-erfzR(1/E77*F77^0.5,G77*F77^0.5)))/E77/G77)),1-((1/E77+G77)*EXP((1/E77+G77)^2*F77)*ERFC((1/E77+G77)*F77^0.5)-(1/E77-G77)*EXP((1/E77-G77)^2*F77)*ERFC((1/E77-G77)*F77^0.5))/2/G77),1)","v":0.86439527802281924}]
["PCB 42",5.76,5.4377199999999988,5.4229296462205747,0.2396977205045526,0.11815391382215863,3.6377197864796025,{"$f":"IFERROR(IF(E78>1,1-(EXP((1/E78^2-G78^2)*F78)*((COS(G78/E78*F78*2)*(1-erfzR(1/E78*F78^0.5,G78*F78^0.5))-SIN(G78/E78*F78*2)*(-erfzI(1/E78*F78^0.5,G78*F78^0.5)))+(COS(G78/E78*F78*2)*(-erfzI(1/E78*F78^0.5,G78*F78^0.5))+SIN(G78/E78*F78*2)*(1-erfzR(1/E78*F78^0.5,G78*F78^0.5)))/E78/G78)),1-((1/E78+G78)*EXP((1/E78+G78)^2*F78)*ERFC((1/E78+G78)*F78^0.5)-(1/E78-G78)*EXP((1/E78-G78)^2*F78)*ERFC((1/E78-G78)*F78^0.5))/2/G78),1)","v":0.84795865954826288}]
["PCB 43",5.75,5.4282499999999994,5.4172280755970448,0.23762683007487692,0.1197153067686211,3.6744160322457624,{"$f":"IFERROR(IF(E79>1,1-(EXP((1/E79^2-G79^2)*F79)*((COS(G79/E79*F79*2)*(1-erfzR(1/E79*F79^0.5,G79*F79^0.5))-SIN(G79/E79*F79*2)*(-erfzI(1/E79*F79^0.5,G79*F79^0.5)))+(COS(G79/E79*F79*2)*(-erfzI(1/E79*F79^0.5,G79*F79^0.5))+SIN(G79/E79*F79*2)*(1-erfzR(1/E79*F79^0.5,G79*F79^0.5)))/E79/G79)),1-((1/E79+G79)*EXP((1/E79+G79)^2*F79)*ERFC((1/E79+G79)*F79^0.5)-(1/E79-G79)*EXP((1/E79-G79)^2*F79)*ERFC((1/E79-G79)*F79^0.5))/2/G79),1)","v":0.8504022248312274}]
["PCB 44",5.75,5.4282499999999994,5.4172280755970448,0.23762683007487692,0.1197153067686211,3.6744160322457624,{"$f":"IFERROR(IF(E80>1,1-(EXP((1/E80^2-G80^2)*F80)*((COS(G80/E80*F80*2)*(1-erfzR(1/E80*F80^0.5,G80*F80^0.5))-SIN(G80/E80*F80*2)*(-erfzI(1/E80*F80^0.5,G80*F80^0.5)))+(COS(G80/E80*F80*2)*(-erfzI(1/E80*F80^0.5,G80*F80^0.5))+SIN(G80/E80*F80*2)*(1-erfzR(1/E80*F80^0.5,G80*F80^0.5)))/E80/G80)),1-((1/E80+G80)*EXP((1/E80+G80)^2*F80)*ERFC((1/E80+G80)*F80^0.5)-(1/E80-G80)*EXP((1/E80-G80)^2*F80)*ERFC((1/E80-G80)*F80^0.5))/2/G80),1)","v":0.8504022248312274}]
["PCB 45",5.53,5.2199099999999996,5.2917935218793701,0.19633151972879084,0.15980274549759035,4.5661317625239182,{"$f":"IFERROR(IF(E81>1,1-(EXP((1/E81^2-G81^2)*F81)*((COS(G81/E81*F81*2)*(1-erfzR(1/E81*F81^0.5,G81*F81^0.5))-SIN(G81/E81*F81*2)*(-erfzI(1/E81*F81^0.5,G81*F81^0.5)))+(COS(G81/E81*F81*2)*(-erfzI(1/E81*F81^0.5,G81*F81^0.5))+SIN(G81/E81*F81*2)*(1-erfzR(1/E81*F81^0.5,G81*F81^0.5)))/E81/G81)),1-((1/E81+G81)*EXP((1/E81+G81)^2*F81)*ERFC((1/E81+G81)*F81^0.5)-(1/E81-G81)*EXP((1/E81-G81)^2*F81)*ERFC((1/E81-G81)*F81^0.5))/2/G81),1)","v":0.89640321175956439}]
["PCB 46",5.53,5.2199099999999996,5.2917935218793701,0.19633151972879084,0.15980274549759035,4.5661317625239182,{"$f":"IFERROR(IF(E82>1,1-(EXP((1/E82^2-G82^2)*F82)*((COS(G82/E82*F82*2)*(1-erfzR(1/E82*F82^0.5,G82*F82^0.5))-SIN(G82/E82*F82*2)*(-erfzI(1/E82*F82^0.5,G82*F82^0.5)))+(COS(G82/E82*F82*2)*(-erfzI(1/E82*F82^0.5,G82*F82^0.5))+SIN(G82/E82*F82*2)*(1-erfzR(1/E82*F82^0.5,G82*F82^0.5)))/E82/G82)),1-((1/E82+G82)*EXP((1/E82+G82)^2*F82)*ERFC((1/E82+G82)*F82^0.5)-(1/E82-G82)*EXP((1/E82-G82)^2*F82)*ERFC((1/E82-G82)*F82^0.5))/2/G82),1)","v":0.89640321175956439}]
["PCB 47",5.85,5.5229499999999989,5.4742437818323504,0.25916703986207479,0.10498662543553172,3.3210879718462682,{"$f":"IFERROR(IF(E83>1,1-(EXP((1/E83^2-G83^2)*F83)*((COS(G83/E83*F83*2)*(1-erfzR(1/E83*F83^0.5,G83*F83^0.5))-SIN(G83/E83*F83*2)*(-erfzI(1/E83*F83^0.5,G83*F83^0.5)))+(COS(G83/E83*F83*2)*(-erfzI(1/E83*F83^0.5,G83*F83^0.5))+SIN(G83/E83*F83*2)*(1-erfzR(1/E83*F83^0.5,G83*F83^0.5)))/E83/G83)),1-((1/E83+G83)*EXP((1/E83+G83)^2*F83)*ERFC((1/E83+G83)*F83^0.5)-(1/E83-G83)*EXP((1/E83-G83)^2*F83)*ERFC((1/E83-G83)*F83^0.5))/2/G83),1)","v":0.82449637981967794}]
["PCB 48",5.78,5.4566599999999994,5.4343327874676364,0.24389380136047348,0.11509195596314989,3.5652553193071874,{"$f":"IFERROR(IF(E84>1,1-(EXP((1/E84^2-G84^2)*F84)*((COS(G84/E84*F84*2)*(1-erfzR(1/E84*F84^0.5,G84*F84^0.5))-SIN(G84/E84*F84*2)*(-erfzI(1/E84*F84^0.5,G84*F84^0.5)))+(COS(G84/E84*F84*2)*(-erfzI(1/E84*F84^0.5,G84*F84^0.5))+SIN(G84/E84*F84*2)*(1-erfzR(1/E84*F84^0.5,G84*F84^0.5)))/E84/G84)),1-((1/E84+G84)*EXP((1/E84+G84)^2*F84)*ERFC((1/E84+G84)*F84^0.5)-(1/E84-G84)*EXP((1/E84-G84)^2*F84)*ERFC((1/E84-G84)*F84^0.5))/2/G84),1)","v":0.84297448204086634}]
["PCB 49",5.85,5.5229499999999989,5.4742437818323504,0.25916703986207479,0.10498662543553172,3.3210879718462682,{"$f":"IFERROR(IF(E85>1,1-(EXP((1/E85^2-G85^2)*F85)*((COS(G85/E85*F85*2)*(1-erfzR(1/E85*F85^0.5,G85*F85^0.5))-SIN(G85/E85*F85*2)*(-erfzI(1/E85*F85^0.5,G85*F85^0.5)))+(COS(G85/E85*F85*2)*(-erfzI(1/E85*F85^0.5,G85*F85^0.5))+SIN(G85/E85*F85*2)*(1-erfzR(1/E85*F85^0.5,G85*F85^0.5)))/E85/G85)),1-((1/E85+G85)*EXP((1/E85+G85)^2*F85)*ERFC((1/E85+G85)*F85^0.5)-(1/E85-G85)*EXP((1/E85-G85)^2*F85)*ERFC((1/E85-G85)*F85^0.5))/2/G85),1)","v":0.82449637981967794}]
["PCB 50",5.63,5.3146099999999992,5.3488092281146766,0.21412842473932683,0.14014207070070814,4.1400107451272943,{"$f":"IFERROR(IF(E86>1,1-(EXP((1/E86^2-G86^2)*F86)*((COS(G86/E86*F86*2)*(1-erfzR(1/E86*F86^0.5,G86*F86^0.5))-SIN(G86/E86*F86*2)*(-erfzI(1/E86*F86^0.5,G86*F86^0.5)))+(COS(G86/E86*F86*2)*(-erfzI(1/E86*F86^0.5,G86*F86^0.5))+SIN(G86/E86*F86*2)*(1-erfzR(1/E86*F86^0.5,G86*F86^0.5)))/E86/G86)),1-((1/E86+G86)*EXP((1/E86+G86)^2*F86)*ERFC((1/E86+G86)*F86^0.5)-(1/E86-G86)*EXP((1/E86-G86)^2*F86)*ERFC((1/E86-G86)*F86^0.5))/2/G86),1)","v":0.87727429585030992}]
["PCB 51",5.63,5.3146099999999992,5.3488092281146766,0.21412842473932683,0.14014207070070814,4.1400107451272943,{"$f":"IFERROR(IF(E87>1,1-(EXP((1/E87^2-G87^2)*F87)*((COS(G87/E87*F87*2)*(1-erfzR(1/E87*F87^0.5,G87*F87^0.5))-SIN(G87/E87*F87*2)*(-erfzI(1/E87*F87^0.5,G87*F87^0.5)))+(COS(G87/E87*F87*2)*(-erfzI(1/E87*F87^0.5,G87*F87^0.5))+SIN(G87/E87*F87*2)*(1-erfzR(1/E87*F87^0.5,G87*F87^0.5)))/E87/G87)),1-((1/E87+G87)*EXP((1/E87+G87)^2*F87)*ERFC((1/E87+G87)*F87^0.5)-(1/E87-G87)*EXP((1/E87-G87)^2*F87)*ERFC((1/E87-G87)*F87^0.5))/2/G87),1)","v":0.87727429585030992}]
["PCB 52",5.84,5.5134799999999995,5.4685422112088196,0.25692794246303441,0.10637401389457753,3.3550896265158303,{"$f":"IFERROR(IF(E88>1,1-(EXP((1/E88^2-G88^2)*F88)*((COS(G88/E88*F88*2)*(1-erfzR(1/E88*F88^0.5,G88*F88^0.5))-SIN(G88/E88*F88*2)*(-erfzI(1/E88*F88^0.5,G88*F88^0.5)))+(COS(G88/E88*F88*2)*(-erfzI(1/E88*F88^0.5,G88*F88^0.5))+SIN(G88/E88*F88*2)*(1-erfzR(1/E88*F88^0.5,G88*F88^0.5)))/E88/G88)),1-((1/E88+G88)*EXP((1/E88+G88)^2*F88)*ERFC((1/E88+G88)*F88^0.5)-(1/E88-G88)*EXP((1/E88-G88)^2*F88)*ERFC((1/E88-G88)*F88^0.5))/2/G88),1)","v":0.82723545724655878}]
["PCB 53",5.62,5.3051399999999997,5.3431076574911458,0.21227844258438341,0.14199403508865166,4.1810029381328846,{"$f":"IFERROR(IF(E89>1,1-(EXP((1/E89^2-G89^2)*F89)*((COS(G89/E89*F89*2)*(1-erfzR(1/E89*F89^0.5,G89*F89^0.5))-SIN(G89/E89*F89*2)*(-erfzI(1/E89*F89^0.5,G89*F89^0.5)))+(COS(G89/E89*F89*2)*(-erfzI(1/E89*F89^0.5,G89*F89^0.5))+SIN(G89/E89*F89*2)*(1-erfzR(1/E89*F89^0.5,G89*F89^0.5)))/E89/G89)),1-((1/E89+G89)*EXP((1/E89+G89)^2*F89)*ERFC((1/E89+G89)*F89^0.5)-(1/E89-G89)*EXP((1/E89-G89)^2*F89)*ERFC((1/E89-G89)*F89^0.5))/2/G89),1)","v":0.87931592085124533}]
["PCB 54",5.21,4.9168699999999994,5.1093432619263908,0.14873058572390258,0.24323972089424706,6.2034491489953725,{"$f":"IFERROR(IF(E90>1,1-(EXP((1/E90^2-G90^2)*F90)*((COS(G90/E90*F90*2)*(1-erfzR(1/E90*F90^0.5,G90*F90^0.5))-SIN(G90/E90*F90*2)*(-erfzI(1/E90*F90^0.5,G90*F90^0.5)))+(COS(G90/E90*F90*2)*(-erfzI(1/E90*F90^0.5,G90*F90^0.5))+SIN(G90/E90*F90*2)*(1-erfzR(1/E90*F90^0.5,G90*F90^0.5)))/E90/G90)),1-((1/E90+G90)*EXP((1/E90+G90)^2*F90)*ERFC((1/E90+G90)*F90^0.5)-(1/E90-G90)*EXP((1/E90-G90)^2*F90)*ERFC((1/E90-G90)*F90^0.5))/2/G90),1)","v":0.94098393157019999}]
["PCB 55",6.11,5.7691699999999999,5.6224846180441475,0.32475730753480164,7.4626511462066045E-2,2.5302941669045969,{"$f":"IFERROR(IF(E91>1,1-(EXP((1/E91^2-G91^2)*F91)*((COS(G91/E91*F91*2)*(1-erfzR(1/E91*F91^0.5,G91*F91^0.5))-SIN(G91/E91*F91*2)*(-erfzI(1/E91*F91^0.5,G91*F91^0.5)))+(COS(G91/E91*F91*2)*(-erfzI(1/E91*F91^0.5,G91*F91^0.5))+SIN(G91/E91*F91*2)*(1-erfzR(1/E91*F91^0.5,G91*F91^0.5)))/E91/G91)),1-((1/E91+G91)*EXP((1/E91+G91)^2*F91)*ERFC((1/E91+G91)*F91^0.5)-(1/E91-G91)*EXP((1/E91-G91)^2*F91)*ERFC((1/E91-G91)*F91^0.5))/2/G91),1)","v":0.74162711572387008}]
["PCB 56",6.11,5.7691699999999999,5.6224846180441475,0.32475730753480164,7.4626511462066045E-2,2.5302941669045969,{"$f":"IFERROR(IF(E92>1,1-(EXP((1/E92^2-G92^2)*F92)*((COS(G92/E92*F92*2)*(1-erfzR(1/E92*F92^0.5,G92*F92^0.5))-SIN(G92/E92*F92*2)*(-erfzI(1/E92*F92^0.5,G92*F92^0.5)))+(COS(G92/E92*F92*2)*(-erfzI(1/E92*F92^0.5,G92*F92^0.5))+SIN(G92/E92*F92*2)*(1-erfzR(1/E92*F92^0.5,G92*F92^0.5)))/E92/G92)),1-((1/E92+G92)*EXP((1/E92+G92)^2*F92)*ERFC((1/E92+G92)*F92^0.5)-(1/E92-G92)*EXP((1/E92-G92)^2*F92)*ERFC((1/E92-G92)*F92^0.5))/2/G92),1)","v":0.74162711572387008}]
["PCB 57",6.17,5.8259899999999991,5.6566940417853306,0.34211294571373285,6.8973730620334281E-2,2.370861377672647,{"$f":"IFERROR(IF(E93>1,1-(EXP((1/E93^2-G93^2)*F93)*((COS(G93/E93*F93*2)*(1-erfzR(1/E93*F93^0.5,G93*F93^0.5))-SIN(G93/E93*F93*2)*(-erfzI(1/E93*F93^0.5,G93*F93^0.5)))+(COS(G93/E93*F93*2)*(-erfzI(1/E93*F93^0.5,G93*F93^0.5))+SIN(G93/E93*F93*2)*(1-erfzR(1/E93*F93^0.5,G93*F93^0.5)))/E93/G93)),1-((1/E93+G93)*EXP((1/E93+G93)^2*F93)*ERFC((1/E93+G93)*F93^0.5)-(1/E93-G93)*EXP((1/E93-G93)^2*F93)*ERFC((1/E93-G93)*F93^0.5))/2/G93),1)","v":0.71945519585503348}]
["PCB 58",6.17,5.8259899999999991,5.6566940417853306,0.34211294571373285,6.8973730620334281E-2,2.370861377672647,{"$f":"IFERROR(IF(E94>1,1-(EXP((1/E94^2-G94^2)*F94)*((COS(G94/E94*F94*2)*(1-erfzR(1/E94*F94^0.5,G94*F94^0.5))-SIN(G94/E94*F94*2)*(-erfzI(1/E94*F94^0.5,G94*F94^0.5)))+(COS(G94/E94*F94*2)*(-erfzI(1/E94*F94^0.5,G94*F94^0.5))+SIN(G94/E94*F94*2)*(1-erfzR(1/E94*F94^0.5,G94*F94^0.5)))/E94/G94)),1-((1/E94+G94)*EXP((1/E94+G94)^2*F94)*ERFC((1/E94+G94)*F94^0.5)-(1/E94-G94)*EXP((1/E94-G94)^2*F94)*ERFC((1/E94-G94)*F94^0.5))/2/G94),1)","v":0.71945519585503348}]
["PCB 59",5.95,5.6176499999999994,5.5312594880676569,0.28265980962547693,9.2070026948547656E-2,2.9963912469004699,{"$f":"IFERROR(IF(E95>1,1-(EXP((1/E95^2-G95^2)*F95)*((COS(G95/E95*F95*2)*(1-erfzR(1/E95*F95^0.5,G95*F95^0.5))-SIN(G95/E95*F95*2)*(-erfzI(1/E95*F95^0.5,G95*F95^0.5)))+(COS(G95/E95*F95*2)*(-erfzI(1/E95*F95^0.5,G95*F95^0.5))+SIN(G95/E95*F95*2)*(1-erfzR(1/E95*F95^0.5,G95*F95^0.5)))/E95/G95)),1-((1/E95+G95)*EXP((1/E95+G95)^2*F95)*ERFC((1/E95+G95)*F95^0.5)-(1/E95-G95)*EXP((1/E95-G95)^2*F95)*ERFC((1/E95-G95)*F95^0.5))/2/G95),1)","v":0.79526517834413091}]
["PCB 60",6.11,5.7691699999999999,5.6224846180441475,0.32475730753480164,7.4626511462066045E-2,2.5302941669045969,{"$f":"IFERROR(IF(E96>1,1-(EXP((1/E96^2-G96^2)*F96)*((COS(G96/E96*F96*2)*(1-erfzR(1/E96*F96^0.5,G96*F96^0.5))-SIN(G96/E96*F96*2)*(-erfzI(1/E96*F96^0.5,G96*F96^0.5)))+(COS(G96/E96*F96*2)*(-erfzI(1/E96*F96^0.5,G96*F96^0.5))+SIN(G96/E96*F96*2)*(1-erfzR(1/E96*F96^0.5,G96*F96^0.5)))/E96/G96)),1-((1/E96+G96)*EXP((1/E96+G96)^2*F96)*ERFC((1/E96+G96)*F96^0.5)-(1/E96-G96)*EXP((1/E96-G96)^2*F96)*ERFC((1/E96-G96)*F96^0.5))/2/G96),1)","v":0.74162711572387008}]
["PCB 61",6.04,5.7028799999999995,5.5825736236794326,0.30561870173154643,8.180957465053261E-2,2.7265852516393916,{"$f":"IFERROR(IF(E97>1,1-(EXP((1/E97^2-G97^2)*F97)*((COS(G97/E97*F97*2)*(1-erfzR(1/E97*F97^0.5,G97*F97^0.5))-SIN(G97/E97*F97*2)*(-erfzI(1/E97*F97^0.5,G97*F97^0.5)))+(COS(G97/E97*F97*2)*(-erfzI(1/E97*F97^0.5,G97*F97^0.5))+SIN(G97/E97*F97*2)*(1-erfzR(1/E97*F97^0.5,G97*F97^0.5)))/E97/G97)),1-((1/E97+G97)*EXP((1/E97+G97)^2*F97)*ERFC((1/E97+G97)*F97^0.5)-(1/E97-G97)*EXP((1/E97-G97)^2*F97)*ERFC((1/E97-G97)*F97^0.5))/2/G97),1)","v":0.76610953135933602}]
["PCB 62",5.89,5.5608299999999993,5.4970500643264728,0.2683202722152494,9.9615677731123523E-2,3.1879171446560099,{"$f":"IFERROR(IF(E98>1,1-(EXP((1/E98^2-G98^2)*F98)*((COS(G98/E98*F98*2)*(1-erfzR(1/E98*F98^0.5,G98*F98^0.5))-SIN(G98/E98*F98*2)*(-erfzI(1/E98*F98^0.5,G98*F98^0.5)))+(COS(G98/E98*F98*2)*(-erfzI(1/E98*F98^0.5,G98*F98^0.5))+SIN(G98/E98*F98*2)*(1-erfzR(1/E98*F98^0.5,G98*F98^0.5)))/E98/G98)),1-((1/E98+G98)*EXP((1/E98+G98)^2*F98)*ERFC((1/E98+G98)*F98^0.5)-(1/E98-G98)*EXP((1/E98-G98)^2*F98)*ERFC((1/E98-G98)*F98^0.5))/2/G98),1)","v":0.81320599742131394}]
["PCB 63",6.17,5.8259899999999991,5.6566940417853306,0.34211294571373285,6.8973730620334281E-2,2.370861377672647,{"$f":"IFERROR(IF(E99>1,1-(EXP((1/E99^2-G99^2)*F99)*((COS(G99/E99*F99*2)*(1-erfzR(1/E99*F99^0.5,G99*F99^0.5))-SIN(G99/E99*F99*2)*(-erfzI(1/E99*F99^0.5,G99*F99^0.5)))+(COS(G99/E99*F99*2)*(-erfzI(1/E99*F99^0.5,G99*F99^0.5))+SIN(G99/E99*F99*2)*(1-erfzR(1/E99*F99^0.5,G99*F99^0.5)))/E99/G99)),1-((1/E99+G99)*EXP((1/E99+G99)^2*F99)*ERFC((1/E99+G99)*F99^0.5)-(1/E99-G99)*EXP((1/E99-G99)^2*F99)*ERFC((1/E99-G99)*F99^0.5))/2/G99),1)","v":0.71945519585503348}]
["PCB 64",5.95,5.6176499999999994,5.5312594880676569,0.28265980962547693,9.2070026948547656E-2,2.9963912469004699,{"$f":"IFERROR(IF(E100>1,1-(EXP((1/E100^2-G100^2)*F100)*((COS(G100/E100*F100*2)*(1-erfzR(1/E100*F100^0.5,G100*F100^0.5))-SIN(G100/E100*F100*2)*(-erfzI(1/E100*F100^0.5,G100*F100^0.5)))+(COS(G100/E100*F100*2)*(-erfzI(1/E100*F100^0.5,G100*F100^0.5))+SIN(G100/E100*F100*2)*(1-erfzR(1/E100*F100^0.5,G100*F100^0.5)))/E100/G100)),1-((1/E100+G100)*EXP((1/E100+G100)^2*F100)*ERFC((1/E100+G100)*F100^0.5)-(1/E100-G100)*EXP((1/E100-G100)^2*F100)*ERFC((1/E100-G100)*F100^0.5))/2/G100),1)","v":0.79526517834413091}]
["PCB 65",5.86,5.5324200000000001,5.4799453524558812,0.261425650736818,0.1036173320606686,3.2873724599387488,{"$f":"IFERROR(IF(E101>1,1-(EXP((1/E101^2-G101^2)*F101)*((COS(G101/E101*F101*2)*(1-erfzR(1/E101*F101^0.5,G101*F101^0.5))-SIN(G101/E101*F101*2)*(-erfzI(1/E101*F101^0.5,G101*F101^0.5)))+(COS(G101/E101*F101*2)*(-erfzI(1/E101*F101^0.5,G101*F101^0.5))+SIN(G101/E101*F101*2)*(1-erfzR(1/E101*F101^0.5,G101*F101^0.5)))/E101/G101)),1-((1/E101+G101)*EXP((1/E101+G101)^2*F101)*ERFC((1/E101+G101)*F101^0.5)-(1/E101-G101)*EXP((1/E101-G101)^2*F101)*ERFC((1/E101-G101)*F101^0.5))/2/G101),1)","v":0.8217239511861294}]
["PCB 66",6.2,{"$f":"B102*0.947-0.017","v":5.8543999999999992},{"$f":"B102*$B$30+$B$31","v":5.6737987536559231},{"$f":"10^C102*($C$8^2-$C$7^2)/10^D102/$C$8^2","v":0.35113554642991807},{"$f":"$B$29*$C$9*86400/10^D102/$C$8^2","v":6.6309996452770914E-2},{"$f":"IF(E102>1,(1/E102-1/E102^2)^0.5,(1/E102^2-1/E102)^0.5)","v":2.2940463851537691},{"$f":"IFERROR(IF(E102>1,1-(EXP((1/E102^2-G102^2)*F102)*((COS(G102/E102*F102*2)*(1-erfzR(1/E102*F102^0.5,G102*F102^0.5))-SIN(G102/E102*F102*2)*(-erfzI(1/E102*F102^0.5,G102*F102^0.5)))+(COS(G102/E102*F102*2)*(-erfzI(1/E102*F102^0.5,G102*F102^0.5))+SIN(G102/E102*F102*2)*(1-erfzR(1/E102*F102^0.5,G102*F102^0.5)))/E102/G102)),1-((1/E102+G102)*EXP((1/E102+G102)^2*F102)*ERFC((1/E102+G102)*F102^0.5)-(1/E102-G102)*EXP((1/E102-G102)^2*F102)*ERFC((1/E102-G102)*F102^0.5))/2/G102),1)","v":0.70798332897601512}]
["PCB 67",6.2,5.8543999999999992,5.6737987536559231,0.35113554642991807,6.6309996452770914E-2,2.2940463851537691,{"$f":"IFERROR(IF(E103>1,1-(EXP((1/E103^2-G103^2)*F103)*((COS(G103/E103*F103*2)*(1-erfzR(1/E103*F103^0.5,G103*F103^0.5))-SIN(G103/E103*F103*2)*(-erfzI(1/E103*F103^0.5,G103*F103^0.5)))+(COS(G103/E103*F103*2)*(-erfzI(1/E103*F103^0.5,G103*F103^0.5))+SIN(G103/E103*F103*2)*(1-erfzR(1/E103*F103^0.5,G103*F103^0.5)))/E103/G103)),1-((1/E103+G103)*EXP((1/E103+G103)^2*F103)*ERFC((1/E103+G103)*F103^0.5)-(1/E103-G103)*EXP((1/E103-G103)^2*F103)*ERFC((1/E103-G103)*F103^0.5))/2/G103),1)","v":0.70798332897601512}]
["PCB 68",6.26,5.9112199999999993,5.7080081773971063,0.36990088705261093,6.1287171853043242E-2,2.1459473441037478,{"$f":"IFERROR(IF(E104>1,1-(EXP((1/E104^2-G104^2)*F104)*((COS(G104/E104*F104*2)*(1-erfzR(1/E104*F104^0.5,G104*F104^0.5))-SIN(G104/E104*F104*2)*(-erfzI(1/E104*F104^0.5,G104*F104^0.5)))+(COS(G104/E104*F104*2)*(-erfzI(1/E104*F104^0.5,G104*F104^0.5))+SIN(G104/E104*F104*2)*(1-erfzR(1/E104*F104^0.5,G104*F104^0.5)))/E104/G104)),1-((1/E104+G104)*EXP((1/E104+G104)^2*F104)*ERFC((1/E104+G104)*F104^0.5)-(1/E104-G104)*EXP((1/E104-G104)^2*F104)*ERFC((1/E104-G104)*F104^0.5))/2/G104),1)","v":0.6843261727516019}]
["PCB 69",6.04,5.7028799999999995,5.5825736236794326,0.30561870173154643,8.180957465053261E-2,2.7265852516393916,{"$f":"IFERROR(IF(E105>1,1-(EXP((1/E105^2-G105^2)*F105)*((COS(G105/E105*F105*2)*(1-erfzR(1/E105*F105^0.5,G105*F105^0.5))-SIN(G105/E105*F105*2)*(-erfzI(1/E105*F105^0.5,G105*F105^0.5)))+(COS(G105/E105*F105*2)*(-erfzI(1/E105*F105^0.5,G105*F105^0.5))+SIN(G105/E105*F105*2)*(1-erfzR(1/E105*F105^0.5,G105*F105^0.5)))/E105/G105)),1-((1/E105+G105)*EXP((1/E105+G105)^2*F105)*ERFC((1/E105+G105)*F105^0.5)-(1/E105-G105)*EXP((1/E105-G105)^2*F105)*ERFC((1/E105-G105)*F105^0.5))/2/G105),1)","v":0.76610953135933602}]
["PCB 70",6.2,5.8543999999999992,5.6737987536559231,0.35113554642991807,6.6309996452770914E-2,2.2940463851537691,{"$f":"IFERROR(IF(E106>1,1-(EXP((1/E106^2-G106^2)*F106)*((COS(G106/E106*F106*2)*(1-erfzR(1/E106*F106^0.5,G106*F106^0.5))-SIN(G106/E106*F106*2)*(-erfzI(1/E106*F106^0.5,G106*F106^0.5)))+(COS(G106/E106*F106*2)*(-erfzI(1/E106*F106^0.5,G106*F106^0.5))+SIN(G106/E106*F106*2)*(1-erfzR(1/E106*F106^0.5,G106*F106^0.5)))/E106/G106)),1-((1/E106+G106)*EXP((1/E106+G106)^2*F106)*ERFC((1/E106+G106)*F106^0.5)-(1/E106-G106)*EXP((1/E106-G106)^2*F106)*ERFC((1/E106-G106)*F106^0.5))/2/G106),1)","v":0.70798332897601512}]
["PCB 71",5.98,5.6460599999999994,5.5483641999382485,0.29011444305200029,8.8514324300806579E-2,2.904188623840243,{"$f":"IFERROR(IF(E107>1,1-(EXP((1/E107^2-G107^2)*F107)*((COS(G107/E107*F107*2)*(1-erfzR(1/E107*F107^0.5,G107*F107^0.5))-SIN(G107/E107*F107*2)*(-erfzI(1/E107*F107^0.5,G107*F107^0.5)))+(COS(G107/E107*F107*2)*(-erfzI(1/E107*F107^0.5,G107*F107^0.5))+SIN(G107/E107*F107*2)*(1-erfzR(1/E107*F107^0.5,G107*F107^0.5)))/E107/G107)),1-((1/E107+G107)*EXP((1/E107+G107)^2*F107)*ERFC((1/E107+G107)*F107^0.5)-(1/E107-G107)*EXP((1/E107-G107)^2*F107)*ERFC((1/E107-G107)*F107^0.5))/2/G107),1)","v":0.78584353052361344}]
["PCB 72",6.26,5.9112199999999993,5.7080081773971063,0.36990088705261093,6.1287171853043242E-2,2.1459473441037478,{"$f":"IFERROR(IF(E108>1,1-(EXP((1/E108^2-G108^2)*F108)*((COS(G108/E108*F108*2)*(1-erfzR(1/E108*F108^0.5,G108*F108^0.5))-SIN(G108/E108*F108*2)*(-erfzI(1/E108*F108^0.5,G108*F108^0.5)))+(COS(G108/E108*F108*2)*(-erfzI(1/E108*F108^0.5,G108*F108^0.5))+SIN(G108/E108*F108*2)*(1-erfzR(1/E108*F108^0.5,G108*F108^0.5)))/E108/G108)),1-((1/E108+G108)*EXP((1/E108+G108)^2*F108)*ERFC((1/E108+G108)*F108^0.5)-(1/E108-G108)*EXP((1/E108-G108)^2*F108)*ERFC((1/E108-G108)*F108^0.5))/2/G108),1)","v":0.6843261727516019}]
["PCB 73",6.04,5.7028799999999995,5.5825736236794326,0.30561870173154643,8.180957465053261E-2,2.7265852516393916,{"$f":"IFERROR(IF(E109>1,1-(EXP((1/E109^2-G109^2)*F109)*((COS(G109/E109*F109*2)*(1-erfzR(1/E109*F109^0.5,G109*F109^0.5))-SIN(G109/E109*F109*2)*(-erfzI(1/E109*F109^0.5,G109*F109^0.5)))+(COS(G109/E109*F109*2)*(-erfzI(1/E109*F109^0.5,G109*F109^0.5))+SIN(G109/E109*F109*2)*(1-erfzR(1/E109*F109^0.5,G109*F109^0.5)))/E109/G109)),1-((1/E109+G109)*EXP((1/E109+G109)^2*F109)*ERFC((1/E109+G109)*F109^0.5)-(1/E109-G109)*EXP((1/E109-G109)^2*F109)*ERFC((1/E109-G109)*F109^0.5))/2/G109),1)","v":0.76610953135933602}]
["PCB 74",6.2,5.8543999999999992,5.6737987536559231,0.35113554642991807,6.6309996452770914E-2,2.2940463851537691,{"$f":"IFERROR(IF(E110>1,1-(EXP((1/E110^2-G110^2)*F110)*((COS(G110/E110*F110*2)*(1-erfzR(1/E110*F110^0.5,G110*F110^0.5))-SIN(G110/E110*F110*2)*(-erfzI(1/E110*F110^0.5,G110*F110^0.5)))+(COS(G110/E110*F110*2)*(-erfzI(1/E110*F110^0.5,G110*F110^0.5))+SIN(G110/E110*F110*2)*(1-erfzR(1/E110*F110^0.5,G110*F110^0.5)))/E110/G110)),1-((1/E110+G110)*EXP((1/E110+G110)^2*F110)*ERFC((1/E110+G110)*F110^0.5)-(1/E110-G110)*EXP((1/E110-G110)^2*F110)*ERFC((1/E110-G110)*F110^0.5))/2/G110),1)","v":0.70798332897601512}]
["PCB 75",6.05,5.7123499999999989,5.5882751943029625,0.30828213348437655,8.0742569133357436E-2,2.6978396971064407,{"$f":"IFERROR(IF(E111>1,1-(EXP((1/E111^2-G111^2)*F111)*((COS(G111/E111*F111*2)*(1-erfzR(1/E111*F111^0.5,G111*F111^0.5))-SIN(G111/E111*F111*2)*(-erfzI(1/E111*F111^0.5,G111*F111^0.5)))+(COS(G111/E111*F111*2)*(-erfzI(1/E111*F111^0.5,G111*F111^0.5))+SIN(G111/E111*F111*2)*(1-erfzR(1/E111*F111^0.5,G111*F111^0.5)))/E111/G111)),1-((1/E111+G111)*EXP((1/E111+G111)^2*F111)*ERFC((1/E111+G111)*F111^0.5)-(1/E111-G111)*EXP((1/E111-G111)^2*F111)*ERFC((1/E111-G111)*F111^0.5))/2/G111),1)","v":0.76270679348247017}]
["PCB 76",6.13,5.7881099999999996,5.6338877592912082,0.33044241758966109,7.269256593398489E-2,2.4762710216579693,{"$f":"IFERROR(IF(E112>1,1-(EXP((1/E112^2-G112^2)*F112)*((COS(G112/E112*F112*2)*(1-erfzR(1/E112*F112^0.5,G112*F112^0.5))-SIN(G112/E112*F112*2)*(-erfzI(1/E112*F112^0.5,G112*F112^0.5)))+(COS(G112/E112*F112*2)*(-erfzI(1/E112*F112^0.5,G112*F112^0.5))+SIN(G112/E112*F112*2)*(1-erfzR(1/E112*F112^0.5,G112*F112^0.5)))/E112/G112)),1-((1/E112+G112)*EXP((1/E112+G112)^2*F112)*ERFC((1/E112+G112)*F112^0.5)-(1/E112-G112)*EXP((1/E112-G112)^2*F112)*ERFC((1/E112-G112)*F112^0.5))/2/G112),1)","v":0.73435438990312751}]
["PCB 77",6.36,6.0059199999999997,5.7650238836324128,0.40343137140521124,5.3746956249917162E-2,1.9145227847809412,{"$f":"IFERROR(IF(E113>1,1-(EXP((1/E113^2-G113^2)*F113)*((COS(G113/E113*F113*2)*(1-erfzR(1/E113*F113^0.5,G113*F113^0.5))-SIN(G113/E113*F113*2)*(-erfzI(1/E113*F113^0.5,G113*F113^0.5)))+(COS(G113/E113*F113*2)*(-erfzI(1/E113*F113^0.5,G113*F113^0.5))+SIN(G113/E113*F113*2)*(1-erfzR(1/E113*F113^0.5,G113*F113^0.5)))/E113/G113)),1-((1/E113+G113)*EXP((1/E113+G113)^2*F113)*ERFC((1/E113+G113)*F113^0.5)-(1/E113-G113)*EXP((1/E113-G113)^2*F113)*ERFC((1/E113-G113)*F113^0.5))/2/G113),1)","v":0.64304822028708597}]
["PCB 78",6.35,5.9964499999999994,5.759322313008882,0.39994588908892037,5.4457217261742664E-2,1.9368410028205092,{"$f":"IFERROR(IF(E114>1,1-(EXP((1/E114^2-G114^2)*F114)*((COS(G114/E114*F114*2)*(1-erfzR(1/E114*F114^0.5,G114*F114^0.5))-SIN(G114/E114*F114*2)*(-erfzI(1/E114*F114^0.5,G114*F114^0.5)))+(COS(G114/E114*F114*2)*(-erfzI(1/E114*F114^0.5,G114*F114^0.5))+SIN(G114/E114*F114*2)*(1-erfzR(1/E114*F114^0.5,G114*F114^0.5)))/E114/G114)),1-((1/E114+G114)*EXP((1/E114+G114)^2*F114)*ERFC((1/E114+G114)*F114^0.5)-(1/E114-G114)*EXP((1/E114-G114)^2*F114)*ERFC((1/E114-G114)*F114^0.5))/2/G114),1)","v":0.64726698761092227}]
["PCB 79",6.42,6.0627399999999989,5.799233307373596,0.42499149876705156,4.9675752080801334E-2,1.7842548665828288,{"$f":"IFERROR(IF(E115>1,1-(EXP((1/E115^2-G115^2)*F115)*((COS(G115/E115*F115*2)*(1-erfzR(1/E115*F115^0.5,G115*F115^0.5))-SIN(G115/E115*F115*2)*(-erfzI(1/E115*F115^0.5,G115*F115^0.5)))+(COS(G115/E115*F115*2)*(-erfzI(1/E115*F115^0.5,G115*F115^0.5))+SIN(G115/E115*F115*2)*(1-erfzR(1/E115*F115^0.5,G115*F115^0.5)))/E115/G115)),1-((1/E115+G115)*EXP((1/E115+G115)^2*F115)*ERFC((1/E115+G115)*F115^0.5)-(1/E115-G115)*EXP((1/E115-G115)^2*F115)*ERFC((1/E115-G115)*F115^0.5))/2/G115),1)","v":0.61738288356980708}]
["PCB 80",6.48,6.1195599999999999,5.833442731114781,0.44770383967698463,4.5912931949463331E-2,1.6599507117198116,{"$f":"IFERROR(IF(E116>1,1-(EXP((1/E116^2-G116^2)*F116)*((COS(G116/E116*F116*2)*(1-erfzR(1/E116*F116^0.5,G116*F116^0.5))-SIN(G116/E116*F116*2)*(-erfzI(1/E116*F116^0.5,G116*F116^0.5)))+(COS(G116/E116*F116*2)*(-erfzI(1/E116*F116^0.5,G116*F116^0.5))+SIN(G116/E116*F116*2)*(1-erfzR(1/E116*F116^0.5,G116*F116^0.5)))/E116/G116)),1-((1/E116+G116)*EXP((1/E116+G116)^2*F116)*ERFC((1/E116+G116)*F116^0.5)-(1/E116-G116)*EXP((1/E116-G116)^2*F116)*ERFC((1/E116-G116)*F116^0.5))/2/G116),1)","v":0.59122027583105075}]
["PCB 81",6.36,6.0059199999999997,5.7650238836324128,0.40343137140521124,5.3746956249917162E-2,1.9145227847809412,{"$f":"IFERROR(IF(E117>1,1-(EXP((1/E117^2-G117^2)*F117)*((COS(G117/E117*F117*2)*(1-erfzR(1/E117*F117^0.5,G117*F117^0.5))-SIN(G117/E117*F117*2)*(-erfzI(1/E117*F117^0.5,G117*F117^0.5)))+(COS(G117/E117*F117*2)*(-erfzI(1/E117*F117^0.5,G117*F117^0.5))+SIN(G117/E117*F117*2)*(1-erfzR(1/E117*F117^0.5,G117*F117^0.5)))/E117/G117)),1-((1/E117+G117)*EXP((1/E117+G117)^2*F117)*ERFC((1/E117+G117)*F117^0.5)-(1/E117-G117)*EXP((1/E117-G117)^2*F117)*ERFC((1/E117-G117)*F117^0.5))/2/G117),1)","v":0.64304822028708597}]
["PCB 82",6.2,5.8543999999999992,5.6737987536559231,0.35113554642991807,6.6309996452770914E-2,2.2940463851537691,{"$f":"IFERROR(IF(E118>1,1-(EXP((1/E118^2-G118^2)*F118)*((COS(G118/E118*F118*2)*(1-erfzR(1/E118*F118^0.5,G118*F118^0.5))-SIN(G118/E118*F118*2)*(-erfzI(1/E118*F118^0.5,G118*F118^0.5)))+(COS(G118/E118*F118*2)*(-erfzI(1/E118*F118^0.5,G118*F118^0.5))+SIN(G118/E118*F118*2)*(1-erfzR(1/E118*F118^0.5,G118*F118^0.5)))/E118/G118)),1-((1/E118+G118)*EXP((1/E118+G118)^2*F118)*ERFC((1/E118+G118)*F118^0.5)-(1/E118-G118)*EXP((1/E118-G118)^2*F118)*ERFC((1/E118-G118)*F118^0.5))/2/G118),1)","v":0.70798332897601512}]
["PCB 83",6.26,5.9112199999999993,5.7080081773971063,0.36990088705261093,6.1287171853043242E-2,2.1459473441037478,{"$f":"IFERROR(IF(E119>1,1-(EXP((1/E119^2-G119^2)*F119)*((COS(G119/E119*F119*2)*(1-erfzR(1/E119*F119^0.5,G119*F119^0.5))-SIN(G119/E119*F119*2)*(-erfzI(1/E119*F119^0.5,G119*F119^0.5)))+(COS(G119/E119*F119*2)*(-erfzI(1/E119*F119^0.5,G119*F119^0.5))+SIN(G119/E119*F119*2)*(1-erfzR(1/E119*F119^0.5,G119*F119^0.5)))/E119/G119)),1-((1/E119+G119)*EXP((1/E119+G119)^2*F119)*ERFC((1/E119+G119)*F119^0.5)-(1/E119-G119)*EXP((1/E119-G119)^2*F119)*ERFC((1/E119-G119)*F119^0.5))/2/G119),1)","v":0.6843261727516019}]
["PCB 84",6.04,5.7028799999999995,5.5825736236794326,0.30561870173154643,8.180957465053261E-2,2.7265852516393916,{"$f":"IFERROR(IF(E120>1,1-(EXP((1/E120^2-G120^2)*F120)*((COS(G120/E120*F120*2)*(1-erfzR(1/E120*F120^0.5,G120*F120^0.5))-SIN(G120/E120*F120*2)*(-erfzI(1/E120*F120^0.5,G120*F120^0.5)))+(COS(G120/E120*F120*2)*(-erfzI(1/E120*F120^0.5,G120*F120^0.5))+SIN(G120/E120*F120*2)*(1-erfzR(1/E120*F120^0.5,G120*F120^0.5)))/E120/G120)),1-((1/E120+G120)*EXP((1/E120+G120)^2*F120)*ERFC((1/E120+G120)*F120^0.5)-(1/E120-G120)*EXP((1/E120-G120)^2*F120)*ERFC((1/E120-G120)*F120^0.5))/2/G120),1)","v":0.76610953135933602}]
["PCB 85",6.3,5.9490999999999996,5.7308144598912287,0.38296500496143082,5.8151818243874207E-2,2.0511423780344655,{"$f":"IFERROR(IF(E121>1,1-(EXP((1/E121^2-G121^2)*F121)*((COS(G121/E121*F121*2)*(1-erfzR(1/E121*F121^0.5,G121*F121^0.5))-SIN(G121/E121*F121*2)*(-erfzI(1/E121*F121^0.5,G121*F121^0.5)))+(COS(G121/E121*F121*2)*(-erfzI(1/E121*F121^0.5,G121*F121^0.5))+SIN(G121/E121*F121*2)*(1-erfzR(1/E121*F121^0.5,G121*F121^0.5)))/E121/G121)),1-((1/E121+G121)*EXP((1/E121+G121)^2*F121)*ERFC((1/E121+G121)*F121^0.5)-(1/E121-G121)*EXP((1/E121-G121)^2*F121)*ERFC((1/E121-G121)*F121^0.5))/2/G121),1)","v":0.66806978984693655}]
["PCB 86",6.23,5.8828100000000001,5.6909034655265147,0.36039610167166192,6.3749134489620066E-2,2.2190928104631604,{"$f":"IFERROR(IF(E122>1,1-(EXP((1/E122^2-G122^2)*F122)*((COS(G122/E122*F122*2)*(1-erfzR(1/E122*F122^0.5,G122*F122^0.5))-SIN(G122/E122*F122*2)*(-erfzI(1/E122*F122^0.5,G122*F122^0.5)))+(COS(G122/E122*F122*2)*(-erfzI(1/E122*F122^0.5,G122*F122^0.5))+SIN(G122/E122*F122*2)*(1-erfzR(1/E122*F122^0.5,G122*F122^0.5)))/E122/G122)),1-((1/E122+G122)*EXP((1/E122+G122)^2*F122)*ERFC((1/E122+G122)*F122^0.5)-(1/E122-G122)*EXP((1/E122-G122)^2*F122)*ERFC((1/E122-G122)*F122^0.5))/2/G122),1)","v":0.69626935739688811}]
["PCB 87",6.29,5.9396299999999993,5.7251128892676988,0.37965634369420592,5.8920289095941193E-2,2.0745576683346312,{"$f":"IFERROR(IF(E123>1,1-(EXP((1/E123^2-G123^2)*F123)*((COS(G123/E123*F123*2)*(1-erfzR(1/E123*F123^0.5,G123*F123^0.5))-SIN(G123/E123*F123*2)*(-erfzI(1/E123*F123^0.5,G123*F123^0.5)))+(COS(G123/E123*F123*2)*(-erfzI(1/E123*F123^0.5,G123*F123^0.5))+SIN(G123/E123*F123*2)*(1-erfzR(1/E123*F123^0.5,G123*F123^0.5)))/E123/G123)),1-((1/E123+G123)*EXP((1/E123+G123)^2*F123)*ERFC((1/E123+G123)*F123^0.5)-(1/E123-G123)*EXP((1/E123-G123)^2*F123)*ERFC((1/E123-G123)*F123^0.5))/2/G123),1)","v":0.67216781167694362}]
["PCB 88",6.07,5.7312899999999996,5.5996783355500241,0.31367883377761746,7.865012601305113E-2,2.6410613018167219,{"$f":"IFERROR(IF(E124>1,1-(EXP((1/E124^2-G124^2)*F124)*((COS(G124/E124*F124*2)*(1-erfzR(1/E124*F124^0.5,G124*F124^0.5))-SIN(G124/E124*F124*2)*(-erfzI(1/E124*F124^0.5,G124*F124^0.5)))+(COS(G124/E124*F124*2)*(-erfzI(1/E124*F124^0.5,G124*F124^0.5))+SIN(G124/E124*F124*2)*(1-erfzR(1/E124*F124^0.5,G124*F124^0.5)))/E124/G124)),1-((1/E124+G124)*EXP((1/E124+G124)^2*F124)*ERFC((1/E124+G124)*F124^0.5)-(1/E124-G124)*EXP((1/E124-G124)^2*F124)*ERFC((1/E124-G124)*F124^0.5))/2/G124),1)","v":0.75580558089067018}]
["PCB 89",6.07,5.7312899999999996,5.5996783355500241,0.31367883377761746,7.865012601305113E-2,2.6410613018167219,{"$f":"IFERROR(IF(E125>1,1-(EXP((1/E125^2-G125^2)*F125)*((COS(G125/E125*F125*2)*(1-erfzR(1/E125*F125^0.5,G125*F125^0.5))-SIN(G125/E125*F125*2)*(-erfzI(1/E125*F125^0.5,G125*F125^0.5)))+(COS(G125/E125*F125*2)*(-erfzI(1/E125*F125^0.5,G125*F125^0.5))+SIN(G125/E125*F125*2)*(1-erfzR(1/E125*F125^0.5,G125*F125^0.5)))/E125/G125)),1-((1/E125+G125)*EXP((1/E125+G125)^2*F125)*ERFC((1/E125+G125)*F125^0.5)-(1/E125-G125)*EXP((1/E125-G125)^2*F125)*ERFC((1/E125-G125)*F125^0.5))/2/G125),1)","v":0.75580558089067018}]
["PCB 90",6.36,6.0059199999999997,5.7650238836324128,0.40343137140521124,5.3746956249917162E-2,1.9145227847809412,{"$f":"IFERROR(IF(E126>1,1-(EXP((1/E126^2-G126^2)*F126)*((COS(G126/E126*F126*2)*(1-erfzR(1/E126*F126^0.5,G126*F126^0.5))-SIN(G126/E126*F126*2)*(-erfzI(1/E126*F126^0.5,G126*F126^0.5)))+(COS(G126/E126*F126*2)*(-erfzI(1/E126*F126^0.5,G126*F126^0.5))+SIN(G126/E126*F126*2)*(1-erfzR(1/E126*F126^0.5,G126*F126^0.5)))/E126/G126)),1-((1/E126+G126)*EXP((1/E126+G126)^2*F126)*ERFC((1/E126+G126)*F126^0.5)-(1/E126-G126)*EXP((1/E126-G126)^2*F126)*ERFC((1/E126-G126)*F126^0.5))/2/G126),1)","v":0.64304822028708597}]
["PCB 91",6.13,5.7881099999999996,5.6338877592912082,0.33044241758966109,7.269256593398489E-2,2.4762710216579693,{"$f":"IFERROR(IF(E127>1,1-(EXP((1/E127^2-G127^2)*F127)*((COS(G127/E127*F127*2)*(1-erfzR(1/E127*F127^0.5,G127*F127^0.5))-SIN(G127/E127*F127*2)*(-erfzI(1/E127*F127^0.5,G127*F127^0.5)))+(COS(G127/E127*F127*2)*(-erfzI(1/E127*F127^0.5,G127*F127^0.5))+SIN(G127/E127*F127*2)*(1-erfzR(1/E127*F127^0.5,G127*F127^0.5)))/E127/G127)),1-((1/E127+G127)*EXP((1/E127+G127)^2*F127)*ERFC((1/E127+G127)*F127^0.5)-(1/E127-G127)*EXP((1/E127-G127)^2*F127)*ERFC((1/E127-G127)*F127^0.5))/2/G127),1)","v":0.73435438990312751}]
["PCB 92",6.35,5.9964499999999994,5.759322313008882,0.39994588908892037,5.4457217261742664E-2,1.9368410028205092,{"$f":"IFERROR(IF(E128>1,1-(EXP((1/E128^2-G128^2)*F128)*((COS(G128/E128*F128*2)*(1-erfzR(1/E128*F128^0.5,G128*F128^0.5))-SIN(G128/E128*F128*2)*(-erfzI(1/E128*F128^0.5,G128*F128^0.5)))+(COS(G128/E128*F128*2)*(-erfzI(1/E128*F128^0.5,G128*F128^0.5))+SIN(G128/E128*F128*2)*(1-erfzR(1/E128*F128^0.5,G128*F128^0.5)))/E128/G128)),1-((1/E128+G128)*EXP((1/E128+G128)^2*F128)*ERFC((1/E128+G128)*F128^0.5)-(1/E128-G128)*EXP((1/E128-G128)^2*F128)*ERFC((1/E128-G128)*F128^0.5))/2/G128),1)","v":0.64726698761092227}]
["PCB 93",6.04,5.7028799999999995,5.5825736236794326,0.30561870173154643,8.180957465053261E-2,2.7265852516393916,{"$f":"IFERROR(IF(E129>1,1-(EXP((1/E129^2-G129^2)*F129)*((COS(G129/E129*F129*2)*(1-erfzR(1/E129*F129^0.5,G129*F129^0.5))-SIN(G129/E129*F129*2)*(-erfzI(1/E129*F129^0.5,G129*F129^0.5)))+(COS(G129/E129*F129*2)*(-erfzI(1/E129*F129^0.5,G129*F129^0.5))+SIN(G129/E129*F129*2)*(1-erfzR(1/E129*F129^0.5,G129*F129^0.5)))/E129/G129)),1-((1/E129+G129)*EXP((1/E129+G129)^2*F129)*ERFC((1/E129+G129)*F129^0.5)-(1/E129-G129)*EXP((1/E129-G129)^2*F129)*ERFC((1/E129-G129)*F129^0.5))/2/G129),1)","v":0.76610953135933602}]
["PCB 94",6.13,5.7881099999999996,5.6338877592912082,0.33044241758966109,7.269256593398489E-2,2.4762710216579693,{"$f":"IFERROR(IF(E130>1,1-(EXP((1/E130^2-G130^2)*F130)*((COS(G130/E130*F130*2)*(1-erfzR(1/E130*F130^0.5,G130*F130^0.5))-SIN(G130/E130*F130*2)*(-erfzI(1/E130*F130^0.5,G130*F130^0.5)))+(COS(G130/E130*F130*2)*(-erfzI(1/E130*F130^0.5,G130*F130^0.5))+SIN(G130/E130*F130*2)*(1-erfzR(1/E130*F130^0.5,G130*F130^0.5)))/E130/G130)),1-((1/E130+G130)*EXP((1/E130+G130)^2*F130)*ERFC((1/E130+G130)*F130^0.5)-(1/E130-G130)*EXP((1/E130-G130)^2*F130)*ERFC((1/E130-G130)*F130^0.5))/2/G130),1)","v":0.73435438990312751}]
["PCB 95",6.13,5.7881099999999996,5.6338877592912082,0.33044241758966109,7.269256593398489E-2,2.4762710216579693,{"$f":"IFERROR(IF(E131>1,1-(EXP((1/E131^2-G131^2)*F131)*((COS(G131/E131*F131*2)*(1-erfzR(1/E131*F131^0.5,G131*F131^0.5))-SIN(G131/E131*F131*2)*(-erfzI(1/E131*F131^0.5,G131*F131^0.5)))+(COS(G131/E131*F131*2)*(-erfzI(1/E131*F131^0.5,G131*F131^0.5))+SIN(G131/E131*F131*2)*(1-erfzR(1/E131*F131^0.5,G131*F131^0.5)))/E131/G131)),1-((1/E131+G131)*EXP((1/E131+G131)^2*F131)*ERFC((1/E131+G131)*F131^0.5)-(1/E131-G131)*EXP((1/E131-G131)^2*F131)*ERFC((1/E131-G131)*F131^0.5))/2/G131),1)","v":0.73435438990312751}]
["PCB 96",5.71,5.390369999999999,5.3944217931029215,0.22952064573380468,0.12616995995892488,3.8243598125084395,{"$f":"IFERROR(IF(E132>1,1-(EXP((1/E132^2-G132^2)*F132)*((COS(G132/E132*F132*2)*(1-erfzR(1/E132*F132^0.5,G132*F132^0.5))-SIN(G132/E132*F132*2)*(-erfzI(1/E132*F132^0.5,G132*F132^0.5)))+(COS(G132/E132*F132*2)*(-erfzI(1/E132*F132^0.5,G132*F132^0.5))+SIN(G132/E132*F132*2)*(1-erfzR(1/E132*F132^0.5,G132*F132^0.5)))/E132/G132)),1-((1/E132+G132)*EXP((1/E132+G132)^2*F132)*ERFC((1/E132+G132)*F132^0.5)-(1/E132-G132)*EXP((1/E132-G132)^2*F132)*ERFC((1/E132-G132)*F132^0.5))/2/G132),1)","v":0.85985697113847892}]
["PCB 97",6.29,5.9396299999999993,5.7251128892676988,0.37965634369420592,5.8920289095941193E-2,2.0745576683346312,{"$f":"IFERROR(IF(E133>1,1-(EXP((1/E133^2-G133^2)*F133)*((COS(G133/E133*F133*2)*(1-erfzR(1/E133*F133^0.5,G133*F133^0.5))-SIN(G133/E133*F133*2)*(-erfzI(1/E133*F133^0.5,G133*F133^0.5)))+(COS(G133/E133*F133*2)*(-erfzI(1/E133*F133^0.5,G133*F133^0.5))+SIN(G133/E133*F133*2)*(1-erfzR(1/E133*F133^0.5,G133*F133^0.5)))/E133/G133)),1-((1/E133+G133)*EXP((1/E133+G133)^2*F133)*ERFC((1/E133+G133)*F133^0.5)-(1/E133-G133)*EXP((1/E133-G133)^2*F133)*ERFC((1/E133-G133)*F133^0.5))/2/G133),1)","v":0.67216781167694362}]
["PCB 98",6.13,5.7881099999999996,5.6338877592912082,0.33044241758966109,7.269256593398489E-2,2.4762710216579693,{"$f":"IFERROR(IF(E134>1,1-(EXP((1/E134^2-G134^2)*F134)*((COS(G134/E134*F134*2)*(1-erfzR(1/E134*F134^0.5,G134*F134^0.5))-SIN(G134/E134*F134*2)*(-erfzI(1/E134*F134^0.5,G134*F134^0.5)))+(COS(G134/E134*F134*2)*(-erfzI(1/E134*F134^0.5,G134*F134^0.5))+SIN(G134/E134*F134*2)*(1-erfzR(1/E134*F134^0.5,G134*F134^0.5)))/E134/G134)),1-((1/E134+G134)*EXP((1/E134+G134)^2*F134)*ERFC((1/E134+G134)*F134^0.5)-(1/E134-G134)*EXP((1/E134-G134)^2*F134)*ERFC((1/E134-G134)*F134^0.5))/2/G134),1)","v":0.73435438990312751}]
["PCB 99",6.39,6.0343299999999989,5.7821285955030044,0.41407113299908643,5.167127319670535E-2,1.8486193422937096,{"$f":"IFERROR(IF(E135>1,1-(EXP((1/E135^2-G135^2)*F135)*((COS(G135/E135*F135*2)*(1-erfzR(1/E135*F135^0.5,G135*F135^0.5))-SIN(G135/E135*F135*2)*(-erfzI(1/E135*F135^0.5,G135*F135^0.5)))+(COS(G135/E135*F135*2)*(-erfzI(1/E135*F135^0.5,G135*F135^0.5))+SIN(G135/E135*F135*2)*(1-erfzR(1/E135*F135^0.5,G135*F135^0.5)))/E135/G135)),1-((1/E135+G135)*EXP((1/E135+G135)^2*F135)*ERFC((1/E135+G135)*F135^0.5)-(1/E135-G135)*EXP((1/E135-G135)^2*F135)*ERFC((1/E135-G135)*F135^0.5))/2/G135),1)","v":0.63028710615227568}]
["PCB 100",6.23,5.8828100000000001,5.6909034655265147,0.36039610167166192,6.3749134489620066E-2,2.2190928104631604,{"$f":"IFERROR(IF(E136>1,1-(EXP((1/E136^2-G136^2)*F136)*((COS(G136/E136*F136*2)*(1-erfzR(1/E136*F136^0.5,G136*F136^0.5))-SIN(G136/E136*F136*2)*(-erfzI(1/E136*F136^0.5,G136*F136^0.5)))+(COS(G136/E136*F136*2)*(-erfzI(1/E136*F136^0.5,G136*F136^0.5))+SIN(G136/E136*F136*2)*(1-erfzR(1/E136*F136^0.5,G136*F136^0.5)))/E136/G136)),1-((1/E136+G136)*EXP((1/E136+G136)^2*F136)*ERFC((1/E136+G136)*F136^0.5)-(1/E136-G136)*EXP((1/E136-G136)^2*F136)*ERFC((1/E136-G136)*F136^0.5))/2/G136),1)","v":0.69626935739688811}]
["PCB 101",6.38,6.0248599999999994,5.7764270248794736,0.41049372748714635,5.2354104250660345E-2,1.8704137649135135,{"$f":"IFERROR(IF(E137>1,1-(EXP((1/E137^2-G137^2)*F137)*((COS(G137/E137*F137*2)*(1-erfzR(1/E137*F137^0.5,G137*F137^0.5))-SIN(G137/E137*F137*2)*(-erfzI(1/E137*F137^0.5,G137*F137^0.5)))+(COS(G137/E137*F137*2)*(-erfzI(1/E137*F137^0.5,G137*F137^0.5))+SIN(G137/E137*F137*2)*(1-erfzR(1/E137*F137^0.5,G137*F137^0.5)))/E137/G137)),1-((1/E137+G137)*EXP((1/E137+G137)^2*F137)*ERFC((1/E137+G137)*F137^0.5)-(1/E137-G137)*EXP((1/E137-G137)^2*F137)*ERFC((1/E137-G137)*F137^0.5))/2/G137),1)","v":0.63455761604186622}]
["PCB 102",6.16,5.8165199999999997,5.6509924711617998,0.33915722955733685,6.9885212034685937E-2,2.3968893878514956,{"$f":"IFERROR(IF(E138>1,1-(EXP((1/E138^2-G138^2)*F138)*((COS(G138/E138*F138*2)*(1-erfzR(1/E138*F138^0.5,G138*F138^0.5))-SIN(G138/E138*F138*2)*(-erfzI(1/E138*F138^0.5,G138*F138^0.5)))+(COS(G138/E138*F138*2)*(-erfzI(1/E138*F138^0.5,G138*F138^0.5))+SIN(G138/E138*F138*2)*(1-erfzR(1/E138*F138^0.5,G138*F138^0.5)))/E138/G138)),1-((1/E138+G138)*EXP((1/E138+G138)^2*F138)*ERFC((1/E138+G138)*F138^0.5)-(1/E138-G138)*EXP((1/E138-G138)^2*F138)*ERFC((1/E138-G138)*F138^0.5))/2/G138),1)","v":0.72322329474752656}]
["PCB 103",6.22,5.8733399999999989,5.685201894902983,0.35728242651332798,6.4591573353600717E-2,2.2438738228520965,{"$f":"IFERROR(IF(E139>1,1-(EXP((1/E139^2-G139^2)*F139)*((COS(G139/E139*F139*2)*(1-erfzR(1/E139*F139^0.5,G139*F139^0.5))-SIN(G139/E139*F139*2)*(-erfzI(1/E139*F139^0.5,G139*F139^0.5)))+(COS(G139/E139*F139*2)*(-erfzI(1/E139*F139^0.5,G139*F139^0.5))+SIN(G139/E139*F139*2)*(1-erfzR(1/E139*F139^0.5,G139*F139^0.5)))/E139/G139)),1-((1/E139+G139)*EXP((1/E139+G139)^2*F139)*ERFC((1/E139+G139)*F139^0.5)-(1/E139-G139)*EXP((1/E139-G139)^2*F139)*ERFC((1/E139-G139)*F139^0.5))/2/G139),1)","v":0.70020014351690429}]
["PCB 104",5.81,5.4850699999999994,5.451437499338228,0.2503260525055962,0.11064715686712522,3.4588374967457431,{"$f":"IFERROR(IF(E140>1,1-(EXP((1/E140^2-G140^2)*F140)*((COS(G140/E140*F140*2)*(1-erfzR(1/E140*F140^0.5,G140*F140^0.5))-SIN(G140/E140*F140*2)*(-erfzI(1/E140*F140^0.5,G140*F140^0.5)))+(COS(G140/E140*F140*2)*(-erfzI(1/E140*F140^0.5,G140*F140^0.5))+SIN(G140/E140*F140*2)*(1-erfzR(1/E140*F140^0.5,G140*F140^0.5)))/E140/G140)),1-((1/E140+G140)*EXP((1/E140+G140)^2*F140)*ERFC((1/E140+G140)*F140^0.5)-(1/E140-G140)*EXP((1/E140-G140)^2*F140)*ERFC((1/E140-G140)*F140^0.5))/2/G140),1)","v":0.8352533799458105}]
["PCB 105",6.65,6.2805499999999999,5.9303694317148015,0.51886469186912454,3.6728934237831433E-2,1.3368401975664934,{"$f":"IFERROR(IF(E141>1,1-(EXP((1/E141^2-G141^2)*F141)*((COS(G141/E141*F141*2)*(1-erfzR(1/E141*F141^0.5,G141*F141^0.5))-SIN(G141/E141*F141*2)*(-erfzI(1/E141*F141^0.5,G141*F141^0.5)))+(COS(G141/E141*F141*2)*(-erfzI(1/E141*F141^0.5,G141*F141^0.5))+SIN(G141/E141*F141*2)*(1-erfzR(1/E141*F141^0.5,G141*F141^0.5)))/E141/G141)),1-((1/E141+G141)*EXP((1/E141+G141)^2*F141)*ERFC((1/E141+G141)*F141^0.5)-(1/E141-G141)*EXP((1/E141-G141)^2*F141)*ERFC((1/E141-G141)*F141^0.5))/2/G141),1)","v":0.51576111774108302}]
["PCB 106",6.64,6.2710799999999987,5.9246678610912697,0.51438191279877443,3.7214303676683672E-2,1.3547580425670724,{"$f":"IFERROR(IF(E142>1,1-(EXP((1/E142^2-G142^2)*F142)*((COS(G142/E142*F142*2)*(1-erfzR(1/E142*F142^0.5,G142*F142^0.5))-SIN(G142/E142*F142*2)*(-erfzI(1/E142*F142^0.5,G142*F142^0.5)))+(COS(G142/E142*F142*2)*(-erfzI(1/E142*F142^0.5,G142*F142^0.5))+SIN(G142/E142*F142*2)*(1-erfzR(1/E142*F142^0.5,G142*F142^0.5)))/E142/G142)),1-((1/E142+G142)*EXP((1/E142+G142)^2*F142)*ERFC((1/E142+G142)*F142^0.5)-(1/E142-G142)*EXP((1/E142-G142)^2*F142)*ERFC((1/E142-G142)*F142^0.5))/2/G142),1)","v":0.52021117116610793}]
["PCB 107",6.71,6.3373699999999991,5.9645788554559847,0.54659379186770574,3.3946804781031334E-2,1.231910158274804,{"$f":"IFERROR(IF(E143>1,1-(EXP((1/E143^2-G143^2)*F143)*((COS(G143/E143*F143*2)*(1-erfzR(1/E143*F143^0.5,G143*F143^0.5))-SIN(G143/E143*F143*2)*(-erfzI(1/E143*F143^0.5,G143*F143^0.5)))+(COS(G143/E143*F143*2)*(-erfzI(1/E143*F143^0.5,G143*F143^0.5))+SIN(G143/E143*F143*2)*(1-erfzR(1/E143*F143^0.5,G143*F143^0.5)))/E143/G143)),1-((1/E143+G143)*EXP((1/E143+G143)^2*F143)*ERFC((1/E143+G143)*F143^0.5)-(1/E143-G143)*EXP((1/E143-G143)^2*F143)*ERFC((1/E143-G143)*F143^0.5))/2/G143),1)","v":0.48914775935249366}]
["PCB 108",6.71,6.3373699999999991,5.9645788554559847,0.54659379186770574,3.3946804781031334E-2,1.231910158274804,{"$f":"IFERROR(IF(E144>1,1-(EXP((1/E144^2-G144^2)*F144)*((COS(G144/E144*F144*2)*(1-erfzR(1/E144*F144^0.5,G144*F144^0.5))-SIN(G144/E144*F144*2)*(-erfzI(1/E144*F144^0.5,G144*F144^0.5)))+(COS(G144/E144*F144*2)*(-erfzI(1/E144*F144^0.5,G144*F144^0.5))+SIN(G144/E144*F144*2)*(1-erfzR(1/E144*F144^0.5,G144*F144^0.5)))/E144/G144)),1-((1/E144+G144)*EXP((1/E144+G144)^2*F144)*ERFC((1/E144+G144)*F144^0.5)-(1/E144-G144)*EXP((1/E144-G144)^2*F144)*ERFC((1/E144-G144)*F144^0.5))/2/G144),1)","v":0.48914775935249366}]
["PCB 109",6.48,6.1195599999999999,5.833442731114781,0.44770383967698463,4.5912931949463331E-2,1.6599507117198116,{"$f":"IFERROR(IF(E145>1,1-(EXP((1/E145^2-G145^2)*F145)*((COS(G145/E145*F145*2)*(1-erfzR(1/E145*F145^0.5,G145*F145^0.5))-SIN(G145/E145*F145*2)*(-erfzI(1/E145*F145^0.5,G145*F145^0.5)))+(COS(G145/E145*F145*2)*(-erfzI(1/E145*F145^0.5,G145*F145^0.5))+SIN(G145/E145*F145*2)*(1-erfzR(1/E145*F145^0.5,G145*F145^0.5)))/E145/G145)),1-((1/E145+G145)*EXP((1/E145+G145)^2*F145)*ERFC((1/E145+G145)*F145^0.5)-(1/E145-G145)*EXP((1/E145-G145)^2*F145)*ERFC((1/E145-G145)*F145^0.5))/2/G145),1)","v":0.59122027583105075}]
["PCB 110",6.48,6.1195599999999999,5.833442731114781,0.44770383967698463,4.5912931949463331E-2,1.6599507117198116,{"$f":"IFERROR(IF(E146>1,1-(EXP((1/E146^2-G146^2)*F146)*((COS(G146/E146*F146*2)*(1-erfzR(1/E146*F146^0.5,G146*F146^0.5))-SIN(G146/E146*F146*2)*(-erfzI(1/E146*F146^0.5,G146*F146^0.5)))+(COS(G146/E146*F146*2)*(-erfzI(1/E146*F146^0.5,G146*F146^0.5))+SIN(G146/E146*F146*2)*(1-erfzR(1/E146*F146^0.5,G146*F146^0.5)))/E146/G146)),1-((1/E146+G146)*EXP((1/E146+G146)^2*F146)*ERFC((1/E146+G146)*F146^0.5)-(1/E146-G146)*EXP((1/E146-G146)^2*F146)*ERFC((1/E146-G146)*F146^0.5))/2/G146),1)","v":0.59122027583105075}]
["PCB 111",6.76,6.3847199999999988,5.993086708573637,0.57083006861431407,3.1790038198802682E-2,1.1476456152596965,{"$f":"IFERROR(IF(E147>1,1-(EXP((1/E147^2-G147^2)*F147)*((COS(G147/E147*F147*2)*(1-erfzR(1/E147*F147^0.5,G147*F147^0.5))-SIN(G147/E147*F147*2)*(-erfzI(1/E147*F147^0.5,G147*F147^0.5)))+(COS(G147/E147*F147*2)*(-erfzI(1/E147*F147^0.5,G147*F147^0.5))+SIN(G147/E147*F147*2)*(1-erfzR(1/E147*F147^0.5,G147*F147^0.5)))/E147/G147)),1-((1/E147+G147)*EXP((1/E147+G147)^2*F147)*ERFC((1/E147+G147)*F147^0.5)-(1/E147-G147)*EXP((1/E147-G147)^2*F147)*ERFC((1/E147-G147)*F147^0.5))/2/G147),1)","v":0.46715972370008707}]
["PCB 112",6.45,6.0911499999999998,5.8163380192441885,0.43619986912891828,4.7757297084573817E-2,1.7213811988296259,{"$f":"IFERROR(IF(E148>1,1-(EXP((1/E148^2-G148^2)*F148)*((COS(G148/E148*F148*2)*(1-erfzR(1/E148*F148^0.5,G148*F148^0.5))-SIN(G148/E148*F148*2)*(-erfzI(1/E148*F148^0.5,G148*F148^0.5)))+(COS(G148/E148*F148*2)*(-erfzI(1/E148*F148^0.5,G148*F148^0.5))+SIN(G148/E148*F148*2)*(1-erfzR(1/E148*F148^0.5,G148*F148^0.5)))/E148/G148)),1-((1/E148+G148)*EXP((1/E148+G148)^2*F148)*ERFC((1/E148+G148)*F148^0.5)-(1/E148-G148)*EXP((1/E148-G148)^2*F148)*ERFC((1/E148-G148)*F148^0.5))/2/G148),1)","v":0.60435421344673301}]
["PCB 113",6.54,6.1763799999999991,5.8676521548559641,0.47162997058296519,4.2435136498129751E-2,1.5412308458752437,{"$f":"IFERROR(IF(E149>1,1-(EXP((1/E149^2-G149^2)*F149)*((COS(G149/E149*F149*2)*(1-erfzR(1/E149*F149^0.5,G149*F149^0.5))-SIN(G149/E149*F149*2)*(-erfzI(1/E149*F149^0.5,G149*F149^0.5)))+(COS(G149/E149*F149*2)*(-erfzI(1/E149*F149^0.5,G149*F149^0.5))+SIN(G149/E149*F149*2)*(1-erfzR(1/E149*F149^0.5,G149*F149^0.5)))/E149/G149)),1-((1/E149+G149)*EXP((1/E149+G149)^2*F149)*ERFC((1/E149+G149)*F149^0.5)-(1/E149-G149)*EXP((1/E149-G149)^2*F149)*ERFC((1/E149-G149)*F149^0.5))/2/G149),1)","v":0.56471516786041676}]
["PCB 114",6.65,6.2805499999999999,5.9303694317148015,0.51886469186912454,3.6728934237831433E-2,1.3368401975664934,{"$f":"IFERROR(IF(E150>1,1-(EXP((1/E150^2-G150^2)*F150)*((COS(G150/E150*F150*2)*(1-erfzR(1/E150*F150^0.5,G150*F150^0.5))-SIN(G150/E150*F150*2)*(-erfzI(1/E150*F150^0.5,G150*F150^0.5)))+(COS(G150/E150*F150*2)*(-erfzI(1/E150*F150^0.5,G150*F150^0.5))+SIN(G150/E150*F150*2)*(1-erfzR(1/E150*F150^0.5,G150*F150^0.5)))/E150/G150)),1-((1/E150+G150)*EXP((1/E150+G150)^2*F150)*ERFC((1/E150+G150)*F150^0.5)-(1/E150-G150)*EXP((1/E150-G150)^2*F150)*ERFC((1/E150-G150)*F150^0.5))/2/G150),1)","v":0.51576111774108302}]
["PCB 115",6.49,6.1290299999999993,5.8391443017383109,0.45160552702695189,4.5314110211188321E-2,1.6397864224026173,{"$f":"IFERROR(IF(E151>1,1-(EXP((1/E151^2-G151^2)*F151)*((COS(G151/E151*F151*2)*(1-erfzR(1/E151*F151^0.5,G151*F151^0.5))-SIN(G151/E151*F151*2)*(-erfzI(1/E151*F151^0.5,G151*F151^0.5)))+(COS(G151/E151*F151*2)*(-erfzI(1/E151*F151^0.5,G151*F151^0.5))+SIN(G151/E151*F151*2)*(1-erfzR(1/E151*F151^0.5,G151*F151^0.5)))/E151/G151)),1-((1/E151+G151)*EXP((1/E151+G151)^2*F151)*ERFC((1/E151+G151)*F151^0.5)-(1/E151-G151)*EXP((1/E151-G151)^2*F151)*ERFC((1/E151-G151)*F151^0.5))/2/G151),1)","v":0.58682227825105615}]
["PCB 116",6.33,5.9775099999999997,5.7479191717618203,0.39306500372304048,5.590602141993873E-2,1.9820139713696689,{"$f":"IFERROR(IF(E152>1,1-(EXP((1/E152^2-G152^2)*F152)*((COS(G152/E152*F152*2)*(1-erfzR(1/E152*F152^0.5,G152*F152^0.5))-SIN(G152/E152*F152*2)*(-erfzI(1/E152*F152^0.5,G152*F152^0.5)))+(COS(G152/E152*F152*2)*(-erfzI(1/E152*F152^0.5,G152*F152^0.5))+SIN(G152/E152*F152*2)*(1-erfzR(1/E152*F152^0.5,G152*F152^0.5)))/E152/G152)),1-((1/E152+G152)*EXP((1/E152+G152)^2*F152)*ERFC((1/E152+G152)*F152^0.5)-(1/E152-G152)*EXP((1/E152-G152)^2*F152)*ERFC((1/E152-G152)*F152^0.5))/2/G152),1)","v":0.65564820425030668}]
["PCB 117",6.46,6.1006199999999993,5.8220395898677193,0.44000130070177507,4.7134420120693951E-2,1.700746354823981,{"$f":"IFERROR(IF(E153>1,1-(EXP((1/E153^2-G153^2)*F153)*((COS(G153/E153*F153*2)*(1-erfzR(1/E153*F153^0.5,G153*F153^0.5))-SIN(G153/E153*F153*2)*(-erfzI(1/E153*F153^0.5,G153*F153^0.5)))+(COS(G153/E153*F153*2)*(-erfzI(1/E153*F153^0.5,G153*F153^0.5))+SIN(G153/E153*F153*2)*(1-erfzR(1/E153*F153^0.5,G153*F153^0.5)))/E153/G153)),1-((1/E153+G153)*EXP((1/E153+G153)^2*F153)*ERFC((1/E153+G153)*F153^0.5)-(1/E153-G153)*EXP((1/E153-G153)^2*F153)*ERFC((1/E153-G153)*F153^0.5))/2/G153),1)","v":0.59998697087804076}]
["PCB 118",6.74,6.3657799999999991,5.9816835673265771,0.56100919941003036,3.2635794589737234E-2,1.1810212905419628,{"$f":"IFERROR(IF(E154>1,1-(EXP((1/E154^2-G154^2)*F154)*((COS(G154/E154*F154*2)*(1-erfzR(1/E154*F154^0.5,G154*F154^0.5))-SIN(G154/E154*F154*2)*(-erfzI(1/E154*F154^0.5,G154*F154^0.5)))+(COS(G154/E154*F154*2)*(-erfzI(1/E154*F154^0.5,G154*F154^0.5))+SIN(G154/E154*F154*2)*(1-erfzR(1/E154*F154^0.5,G154*F154^0.5)))/E154/G154)),1-((1/E154+G154)*EXP((1/E154+G154)^2*F154)*ERFC((1/E154+G154)*F154^0.5)-(1/E154-G154)*EXP((1/E154-G154)^2*F154)*ERFC((1/E154-G154)*F154^0.5))/2/G154),1)","v":0.47592818610825816}]
["PCB 119",6.58,6.2142599999999995,5.8904584373500866,0.48828694481766904,4.0264222841124693E-2,1.4650017238921387,{"$f":"IFERROR(IF(E155>1,1-(EXP((1/E155^2-G155^2)*F155)*((COS(G155/E155*F155*2)*(1-erfzR(1/E155*F155^0.5,G155*F155^0.5))-SIN(G155/E155*F155*2)*(-erfzI(1/E155*F155^0.5,G155*F155^0.5)))+(COS(G155/E155*F155*2)*(-erfzI(1/E155*F155^0.5,G155*F155^0.5))+SIN(G155/E155*F155*2)*(1-erfzR(1/E155*F155^0.5,G155*F155^0.5)))/E155/G155)),1-((1/E155+G155)*EXP((1/E155+G155)^2*F155)*ERFC((1/E155+G155)*F155^0.5)-(1/E155-G155)*EXP((1/E155-G155)^2*F155)*ERFC((1/E155-G155)*F155^0.5))/2/G155),1)","v":0.54693331608289819}]
["PCB 120",6.79,6.4131299999999998,6.0101914204442295,0.58588466345040047,3.0562321353901054E-2,1.0983696590164087,{"$f":"IFERROR(IF(E156>1,1-(EXP((1/E156^2-G156^2)*F156)*((COS(G156/E156*F156*2)*(1-erfzR(1/E156*F156^0.5,G156*F156^0.5))-SIN(G156/E156*F156*2)*(-erfzI(1/E156*F156^0.5,G156*F156^0.5)))+(COS(G156/E156*F156*2)*(-erfzI(1/E156*F156^0.5,G156*F156^0.5))+SIN(G156/E156*F156*2)*(1-erfzR(1/E156*F156^0.5,G156*F156^0.5)))/E156/G156)),1-((1/E156+G156)*EXP((1/E156+G156)^2*F156)*ERFC((1/E156+G156)*F156^0.5)-(1/E156-G156)*EXP((1/E156-G156)^2*F156)*ERFC((1/E156-G156)*F156^0.5))/2/G156),1)","v":0.45408678840388694}]
["PCB 121",6.64,6.2710799999999987,5.9246678610912697,0.51438191279877443,3.7214303676683672E-2,1.3547580425670724,{"$f":"IFERROR(IF(E157>1,1-(EXP((1/E157^2-G157^2)*F157)*((COS(G157/E157*F157*2)*(1-erfzR(1/E157*F157^0.5,G157*F157^0.5))-SIN(G157/E157*F157*2)*(-erfzI(1/E157*F157^0.5,G157*F157^0.5)))+(COS(G157/E157*F157*2)*(-erfzI(1/E157*F157^0.5,G157*F157^0.5))+SIN(G157/E157*F157*2)*(1-erfzR(1/E157*F157^0.5,G157*F157^0.5)))/E157/G157)),1-((1/E157+G157)*EXP((1/E157+G157)^2*F157)*ERFC((1/E157+G157)*F157^0.5)-(1/E157-G157)*EXP((1/E157-G157)^2*F157)*ERFC((1/E157-G157)*F157^0.5))/2/G157),1)","v":0.52021117116610793}]
["PCB 122",6.64,6.2710799999999987,5.9246678610912697,0.51438191279877443,3.7214303676683672E-2,1.3547580425670724,{"$f":"IFERROR(IF(E158>1,1-(EXP((1/E158^2-G158^2)*F158)*((COS(G158/E158*F158*2)*(1-erfzR(1/E158*F158^0.5,G158*F158^0.5))-SIN(G158/E158*F158*2)*(-erfzI(1/E158*F158^0.5,G158*F158^0.5)))+(COS(G158/E158*F158*2)*(-erfzI(1/E158*F158^0.5,G158*F158^0.5))+SIN(G158/E158*F158*2)*(1-erfzR(1/E158*F158^0.5,G158*F158^0.5)))/E158/G158)),1-((1/E158+G158)*EXP((1/E158+G158)^2*F158)*ERFC((1/E158+G158)*F158^0.5)-(1/E158-G158)*EXP((1/E158-G158)^2*F158)*ERFC((1/E158-G158)*F158^0.5))/2/G158),1)","v":0.52021117116610793}]
["PCB 123",6.74,6.3657799999999991,5.9816835673265771,0.56100919941003036,3.2635794589737234E-2,1.1810212905419628,{"$f":"IFERROR(IF(E159>1,1-(EXP((1/E159^2-G159^2)*F159)*((COS(G159/E159*F159*2)*(1-erfzR(1/E159*F159^0.5,G159*F159^0.5))-SIN(G159/E159*F159*2)*(-erfzI(1/E159*F159^0.5,G159*F159^0.5)))+(COS(G159/E159*F159*2)*(-erfzI(1/E159*F159^0.5,G159*F159^0.5))+SIN(G159/E159*F159*2)*(1-erfzR(1/E159*F159^0.5,G159*F159^0.5)))/E159/G159)),1-((1/E159+G159)*EXP((1/E159+G159)^2*F159)*ERFC((1/E159+G159)*F159^0.5)-(1/E159-G159)*EXP((1/E159-G159)^2*F159)*ERFC((1/E159-G159)*F159^0.5))/2/G159),1)","v":0.47592818610825816}]
["PCB 124",6.73,6.3563099999999997,5.9759819967030463,0.55616230900334518,3.3067073570062222E-2,1.1978723393813013,{"$f":"IFERROR(IF(E160>1,1-(EXP((1/E160^2-G160^2)*F160)*((COS(G160/E160*F160*2)*(1-erfzR(1/E160*F160^0.5,G160*F160^0.5))-SIN(G160/E160*F160*2)*(-erfzI(1/E160*F160^0.5,G160*F160^0.5)))+(COS(G160/E160*F160*2)*(-erfzI(1/E160*F160^0.5,G160*F160^0.5))+SIN(G160/E160*F160*2)*(1-erfzR(1/E160*F160^0.5,G160*F160^0.5)))/E160/G160)),1-((1/E160+G160)*EXP((1/E160+G160)^2*F160)*ERFC((1/E160+G160)*F160^0.5)-(1/E160-G160)*EXP((1/E160-G160)^2*F160)*ERFC((1/E160-G160)*F160^0.5))/2/G160),1)","v":0.48032645012152531}]
["PCB 125",6.51,6.147969999999999,5.8505474429853717,0.45951120632334652,4.4139795358665017E-2,1.5999162141478795,{"$f":"IFERROR(IF(E161>1,1-(EXP((1/E161^2-G161^2)*F161)*((COS(G161/E161*F161*2)*(1-erfzR(1/E161*F161^0.5,G161*F161^0.5))-SIN(G161/E161*F161*2)*(-erfzI(1/E161*F161^0.5,G161*F161^0.5)))+(COS(G161/E161*F161*2)*(-erfzI(1/E161*F161^0.5,G161*F161^0.5))+SIN(G161/E161*F161*2)*(1-erfzR(1/E161*F161^0.5,G161*F161^0.5)))/E161/G161)),1-((1/E161+G161)*EXP((1/E161+G161)^2*F161)*ERFC((1/E161+G161)*F161^0.5)-(1/E161-G161)*EXP((1/E161-G161)^2*F161)*ERFC((1/E161-G161)*F161^0.5))/2/G161),1)","v":0.57800064591618272}]
["PCB 126",6.89,6.5078299999999993,6.067207126679536,0.63899347510204052,2.68022116054367E-2,0.94028845159992769,{"$f":"IFERROR(IF(E162>1,1-(EXP((1/E162^2-G162^2)*F162)*((COS(G162/E162*F162*2)*(1-erfzR(1/E162*F162^0.5,G162*F162^0.5))-SIN(G162/E162*F162*2)*(-erfzI(1/E162*F162^0.5,G162*F162^0.5)))+(COS(G162/E162*F162*2)*(-erfzI(1/E162*F162^0.5,G162*F162^0.5))+SIN(G162/E162*F162*2)*(1-erfzR(1/E162*F162^0.5,G162*F162^0.5)))/E162/G162)),1-((1/E162+G162)*EXP((1/E162+G162)^2*F162)*ERFC((1/E162+G162)*F162^0.5)-(1/E162-G162)*EXP((1/E162-G162)^2*F162)*ERFC((1/E162-G162)*F162^0.5))/2/G162),1)","v":0.41139691014000113}]
["PCB 127",6.95,6.5646499999999994,6.1014165504207192,0.67314248205357929,2.4772007790318393E-2,0.84932173737765326,{"$f":"IFERROR(IF(E163>1,1-(EXP((1/E163^2-G163^2)*F163)*((COS(G163/E163*F163*2)*(1-erfzR(1/E163*F163^0.5,G163*F163^0.5))-SIN(G163/E163*F163*2)*(-erfzI(1/E163*F163^0.5,G163*F163^0.5)))+(COS(G163/E163*F163*2)*(-erfzI(1/E163*F163^0.5,G163*F163^0.5))+SIN(G163/E163*F163*2)*(1-erfzR(1/E163*F163^0.5,G163*F163^0.5)))/E163/G163)),1-((1/E163+G163)*EXP((1/E163+G163)^2*F163)*ERFC((1/E163+G163)*F163^0.5)-(1/E163-G163)*EXP((1/E163-G163)^2*F163)*ERFC((1/E163-G163)*F163^0.5))/2/G163),1)","v":0.38660340067936849}]
["PCB 128",6.74,6.3657799999999991,5.9816835673265771,0.56100919941003036,3.2635794589737234E-2,1.1810212905419628,{"$f":"IFERROR(IF(E164>1,1-(EXP((1/E164^2-G164^2)*F164)*((COS(G164/E164*F164*2)*(1-erfzR(1/E164*F164^0.5,G164*F164^0.5))-SIN(G164/E164*F164*2)*(-erfzI(1/E164*F164^0.5,G164*F164^0.5)))+(COS(G164/E164*F164*2)*(-erfzI(1/E164*F164^0.5,G164*F164^0.5))+SIN(G164/E164*F164*2)*(1-erfzR(1/E164*F164^0.5,G164*F164^0.5)))/E164/G164)),1-((1/E164+G164)*EXP((1/E164+G164)^2*F164)*ERFC((1/E164+G164)*F164^0.5)-(1/E164-G164)*EXP((1/E164-G164)^2*F164)*ERFC((1/E164-G164)*F164^0.5))/2/G164),1)","v":0.47592818610825816}]
["PCB 129",6.73,6.3563099999999997,5.9759819967030463,0.55616230900334518,3.3067073570062222E-2,1.1978723393813013,{"$f":"IFERROR(IF(E165>1,1-(EXP((1/E165^2-G165^2)*F165)*((COS(G165/E165*F165*2)*(1-erfzR(1/E165*F165^0.5,G165*F165^0.5))-SIN(G165/E165*F165*2)*(-erfzI(1/E165*F165^0.5,G165*F165^0.5)))+(COS(G165/E165*F165*2)*(-erfzI(1/E165*F165^0.5,G165*F165^0.5))+SIN(G165/E165*F165*2)*(1-erfzR(1/E165*F165^0.5,G165*F165^0.5)))/E165/G165)),1-((1/E165+G165)*EXP((1/E165+G165)^2*F165)*ERFC((1/E165+G165)*F165^0.5)-(1/E165-G165)*EXP((1/E165-G165)^2*F165)*ERFC((1/E165-G165)*F165^0.5))/2/G165),1)","v":0.48032645012152531}]
["PCB 130",6.8,{"$f":"B166*0.947-0.017","v":6.4225999999999992},{"$f":"B166*$B$30+$B$31","v":6.0158929910677603},{"$f":"10^C166*($C$8^2-$C$7^2)/10^D166/$C$8^2","v":0.59099058074959776},{"$f":"$B$29*$C$9*86400/10^D166/$C$8^2","v":3.01637107311029E-2},{"$f":"IF(E166>1,(1/E166-1/E166^2)^0.5,(1/E166^2-1/E166)^0.5)","v":1.0821465911423656},{"$f":"IFERROR(IF(E166>1,1-(EXP((1/E166^2-G166^2)*F166)*((COS(G166/E166*F166*2)*(1-erfzR(1/E166*F166^0.5,G166*F166^0.5))-SIN(G166/E166*F166*2)*(-erfzI(1/E166*F166^0.5,G166*F166^0.5)))+(COS(G166/E166*F166*2)*(-erfzI(1/E166*F166^0.5,G166*F166^0.5))+SIN(G166/E166*F166*2)*(1-erfzR(1/E166*F166^0.5,G166*F166^0.5)))/E166/G166)),1-((1/E166+G166)*EXP((1/E166+G166)^2*F166)*ERFC((1/E166+G166)*F166^0.5)-(1/E166-G166)*EXP((1/E166-G166)^2*F166)*ERFC((1/E166-G166)*F166^0.5))/2/G166),1)","v":0.44975290642501864}]
["PCB 131",6.58,6.2142599999999995,5.8904584373500866,0.48828694481766904,4.0264222841124693E-2,1.4650017238921387,{"$f":"IFERROR(IF(E167>1,1-(EXP((1/E167^2-G167^2)*F167)*((COS(G167/E167*F167*2)*(1-erfzR(1/E167*F167^0.5,G167*F167^0.5))-SIN(G167/E167*F167*2)*(-erfzI(1/E167*F167^0.5,G167*F167^0.5)))+(COS(G167/E167*F167*2)*(-erfzI(1/E167*F167^0.5,G167*F167^0.5))+SIN(G167/E167*F167*2)*(1-erfzR(1/E167*F167^0.5,G167*F167^0.5)))/E167/G167)),1-((1/E167+G167)*EXP((1/E167+G167)^2*F167)*ERFC((1/E167+G167)*F167^0.5)-(1/E167-G167)*EXP((1/E167-G167)^2*F167)*ERFC((1/E167-G167)*F167^0.5))/2/G167),1)","v":0.54693331608289819}]
["PCB 132",6.58,6.2142599999999995,5.8904584373500866,0.48828694481766904,4.0264222841124693E-2,1.4650017238921387,{"$f":"IFERROR(IF(E168>1,1-(EXP((1/E168^2-G168^2)*F168)*((COS(G168/E168*F168*2)*(1-erfzR(1/E168*F168^0.5,G168*F168^0.5))-SIN(G168/E168*F168*2)*(-erfzI(1/E168*F168^0.5,G168*F168^0.5)))+(COS(G168/E168*F168*2)*(-erfzI(1/E168*F168^0.5,G168*F168^0.5))+SIN(G168/E168*F168*2)*(1-erfzR(1/E168*F168^0.5,G168*F168^0.5)))/E168/G168)),1-((1/E168+G168)*EXP((1/E168+G168)^2*F168)*ERFC((1/E168+G168)*F168^0.5)-(1/E168-G168)*EXP((1/E168-G168)^2*F168)*ERFC((1/E168-G168)*F168^0.5))/2/G168),1)","v":0.54693331608289819}]
["PCB 133",6.86,6.4794199999999993,6.0501024148089435,0.62257422320711908,2.7878881348143019E-2,0.98678978106229409,{"$f":"IFERROR(IF(E169>1,1-(EXP((1/E169^2-G169^2)*F169)*((COS(G169/E169*F169*2)*(1-erfzR(1/E169*F169^0.5,G169*F169^0.5))-SIN(G169/E169*F169*2)*(-erfzI(1/E169*F169^0.5,G169*F169^0.5)))+(COS(G169/E169*F169*2)*(-erfzI(1/E169*F169^0.5,G169*F169^0.5))+SIN(G169/E169*F169*2)*(1-erfzR(1/E169*F169^0.5,G169*F169^0.5)))/E169/G169)),1-((1/E169+G169)*EXP((1/E169+G169)^2*F169)*ERFC((1/E169+G169)*F169^0.5)-(1/E169-G169)*EXP((1/E169-G169)^2*F169)*ERFC((1/E169-G169)*F169^0.5))/2/G169),1)","v":0.42404070274362526}]
["PCB 134",6.55,6.1858499999999994,5.873353725479495,0.47574017140549252,4.1881674083014971E-2,1.5219607968404911,{"$f":"IFERROR(IF(E170>1,1-(EXP((1/E170^2-G170^2)*F170)*((COS(G170/E170*F170*2)*(1-erfzR(1/E170*F170^0.5,G170*F170^0.5))-SIN(G170/E170*F170*2)*(-erfzI(1/E170*F170^0.5,G170*F170^0.5)))+(COS(G170/E170*F170*2)*(-erfzI(1/E170*F170^0.5,G170*F170^0.5))+SIN(G170/E170*F170*2)*(1-erfzR(1/E170*F170^0.5,G170*F170^0.5)))/E170/G170)),1-((1/E170+G170)*EXP((1/E170+G170)^2*F170)*ERFC((1/E170+G170)*F170^0.5)-(1/E170-G170)*EXP((1/E170-G170)^2*F170)*ERFC((1/E170-G170)*F170^0.5))/2/G170),1)","v":0.56027549503215568}]
["PCB 135",6.64,6.2710799999999987,5.9246678610912697,0.51438191279877443,3.7214303676683672E-2,1.3547580425670724,{"$f":"IFERROR(IF(E171>1,1-(EXP((1/E171^2-G171^2)*F171)*((COS(G171/E171*F171*2)*(1-erfzR(1/E171*F171^0.5,G171*F171^0.5))-SIN(G171/E171*F171*2)*(-erfzI(1/E171*F171^0.5,G171*F171^0.5)))+(COS(G171/E171*F171*2)*(-erfzI(1/E171*F171^0.5,G171*F171^0.5))+SIN(G171/E171*F171*2)*(1-erfzR(1/E171*F171^0.5,G171*F171^0.5)))/E171/G171)),1-((1/E171+G171)*EXP((1/E171+G171)^2*F171)*ERFC((1/E171+G171)*F171^0.5)-(1/E171-G171)*EXP((1/E171-G171)^2*F171)*ERFC((1/E171-G171)*F171^0.5))/2/G171),1)","v":0.52021117116610793}]
["PCB 136",6.22,5.8733399999999989,5.685201894902983,0.35728242651332798,6.4591573353600717E-2,2.2438738228520965,{"$f":"IFERROR(IF(E172>1,1-(EXP((1/E172^2-G172^2)*F172)*((COS(G172/E172*F172*2)*(1-erfzR(1/E172*F172^0.5,G172*F172^0.5))-SIN(G172/E172*F172*2)*(-erfzI(1/E172*F172^0.5,G172*F172^0.5)))+(COS(G172/E172*F172*2)*(-erfzI(1/E172*F172^0.5,G172*F172^0.5))+SIN(G172/E172*F172*2)*(1-erfzR(1/E172*F172^0.5,G172*F172^0.5)))/E172/G172)),1-((1/E172+G172)*EXP((1/E172+G172)^2*F172)*ERFC((1/E172+G172)*F172^0.5)-(1/E172-G172)*EXP((1/E172-G172)^2*F172)*ERFC((1/E172-G172)*F172^0.5))/2/G172),1)","v":0.70020014351690429}]
["PCB 137",6.83,6.4510099999999992,6.0329977029383519,0.60657687207220945,2.8998801914770989E-2,1.034056088849761,{"$f":"IFERROR(IF(E173>1,1-(EXP((1/E173^2-G173^2)*F173)*((COS(G173/E173*F173*2)*(1-erfzR(1/E173*F173^0.5,G173*F173^0.5))-SIN(G173/E173*F173*2)*(-erfzI(1/E173*F173^0.5,G173*F173^0.5)))+(COS(G173/E173*F173*2)*(-erfzI(1/E173*F173^0.5,G173*F173^0.5))+SIN(G173/E173*F173*2)*(1-erfzR(1/E173*F173^0.5,G173*F173^0.5)))/E173/G173)),1-((1/E173+G173)*EXP((1/E173+G173)^2*F173)*ERFC((1/E173+G173)*F173^0.5)-(1/E173-G173)*EXP((1/E173-G173)^2*F173)*ERFC((1/E173-G173)*F173^0.5))/2/G173),1)","v":0.43683097326266418}]
["PCB 138",6.83,6.4510099999999992,6.0329977029383519,0.60657687207220945,2.8998801914770989E-2,1.034056088849761,{"$f":"IFERROR(IF(E174>1,1-(EXP((1/E174^2-G174^2)*F174)*((COS(G174/E174*F174*2)*(1-erfzR(1/E174*F174^0.5,G174*F174^0.5))-SIN(G174/E174*F174*2)*(-erfzI(1/E174*F174^0.5,G174*F174^0.5)))+(COS(G174/E174*F174*2)*(-erfzI(1/E174*F174^0.5,G174*F174^0.5))+SIN(G174/E174*F174*2)*(1-erfzR(1/E174*F174^0.5,G174*F174^0.5)))/E174/G174)),1-((1/E174+G174)*EXP((1/E174+G174)^2*F174)*ERFC((1/E174+G174)*F174^0.5)-(1/E174-G174)*EXP((1/E174-G174)^2*F174)*ERFC((1/E174-G174)*F174^0.5))/2/G174),1)","v":0.43683097326266418}]
["PCB 139",6.67,6.2994899999999996,5.9417725729618613,0.52794779118180313,3.5777104161243398E-2,1.3013797355615921,{"$f":"IFERROR(IF(E175>1,1-(EXP((1/E175^2-G175^2)*F175)*((COS(G175/E175*F175*2)*(1-erfzR(1/E175*F175^0.5,G175*F175^0.5))-SIN(G175/E175*F175*2)*(-erfzI(1/E175*F175^0.5,G175*F175^0.5)))+(COS(G175/E175*F175*2)*(-erfzI(1/E175*F175^0.5,G175*F175^0.5))+SIN(G175/E175*F175*2)*(1-erfzR(1/E175*F175^0.5,G175*F175^0.5)))/E175/G175)),1-((1/E175+G175)*EXP((1/E175+G175)^2*F175)*ERFC((1/E175+G175)*F175^0.5)-(1/E175-G175)*EXP((1/E175-G175)^2*F175)*ERFC((1/E175-G175)*F175^0.5))/2/G175),1)","v":0.5068706161126777}]
["PCB 140",6.67,6.2994899999999996,5.9417725729618613,0.52794779118180313,3.5777104161243398E-2,1.3013797355615921,{"$f":"IFERROR(IF(E176>1,1-(EXP((1/E176^2-G176^2)*F176)*((COS(G176/E176*F176*2)*(1-erfzR(1/E176*F176^0.5,G176*F176^0.5))-SIN(G176/E176*F176*2)*(-erfzI(1/E176*F176^0.5,G176*F176^0.5)))+(COS(G176/E176*F176*2)*(-erfzI(1/E176*F176^0.5,G176*F176^0.5))+SIN(G176/E176*F176*2)*(1-erfzR(1/E176*F176^0.5,G176*F176^0.5)))/E176/G176)),1-((1/E176+G176)*EXP((1/E176+G176)^2*F176)*ERFC((1/E176+G176)*F176^0.5)-(1/E176-G176)*EXP((1/E176-G176)^2*F176)*ERFC((1/E176-G176)*F176^0.5))/2/G176),1)","v":0.5068706161126777}]
["PCB 141",6.82,6.4415399999999998,6.027296132314822,0.60133629558031565,2.9382018376256501E-2,1.0499918572424012,{"$f":"IFERROR(IF(E177>1,1-(EXP((1/E177^2-G177^2)*F177)*((COS(G177/E177*F177*2)*(1-erfzR(1/E177*F177^0.5,G177*F177^0.5))-SIN(G177/E177*F177*2)*(-erfzI(1/E177*F177^0.5,G177*F177^0.5)))+(COS(G177/E177*F177*2)*(-erfzI(1/E177*F177^0.5,G177*F177^0.5))+SIN(G177/E177*F177*2)*(1-erfzR(1/E177*F177^0.5,G177*F177^0.5)))/E177/G177)),1-((1/E177+G177)*EXP((1/E177+G177)^2*F177)*ERFC((1/E177+G177)*F177^0.5)-(1/E177-G177)*EXP((1/E177-G177)^2*F177)*ERFC((1/E177-G177)*F177^0.5))/2/G177),1)","v":0.44112441238450684}]
["PCB 142",6.51,6.147969999999999,5.8505474429853717,0.45951120632334652,4.4139795358665017E-2,1.5999162141478795,{"$f":"IFERROR(IF(E178>1,1-(EXP((1/E178^2-G178^2)*F178)*((COS(G178/E178*F178*2)*(1-erfzR(1/E178*F178^0.5,G178*F178^0.5))-SIN(G178/E178*F178*2)*(-erfzI(1/E178*F178^0.5,G178*F178^0.5)))+(COS(G178/E178*F178*2)*(-erfzI(1/E178*F178^0.5,G178*F178^0.5))+SIN(G178/E178*F178*2)*(1-erfzR(1/E178*F178^0.5,G178*F178^0.5)))/E178/G178)),1-((1/E178+G178)*EXP((1/E178+G178)^2*F178)*ERFC((1/E178+G178)*F178^0.5)-(1/E178-G178)*EXP((1/E178-G178)^2*F178)*ERFC((1/E178-G178)*F178^0.5))/2/G178),1)","v":0.57800064591618272}]
["PCB 143",6.6,6.2331999999999992,5.9018615785971473,0.49683475869354765,3.9220775784848408E-2,1.427720990470543,{"$f":"IFERROR(IF(E179>1,1-(EXP((1/E179^2-G179^2)*F179)*((COS(G179/E179*F179*2)*(1-erfzR(1/E179*F179^0.5,G179*F179^0.5))-SIN(G179/E179*F179*2)*(-erfzI(1/E179*F179^0.5,G179*F179^0.5)))+(COS(G179/E179*F179*2)*(-erfzI(1/E179*F179^0.5,G179*F179^0.5))+SIN(G179/E179*F179*2)*(1-erfzR(1/E179*F179^0.5,G179*F179^0.5)))/E179/G179)),1-((1/E179+G179)*EXP((1/E179+G179)^2*F179)*ERFC((1/E179+G179)*F179^0.5)-(1/E179-G179)*EXP((1/E179-G179)^2*F179)*ERFC((1/E179-G179)*F179^0.5))/2/G179),1)","v":0.53802663036251808}]
["PCB 144",6.67,6.2994899999999996,5.9417725729618613,0.52794779118180313,3.5777104161243398E-2,1.3013797355615921,{"$f":"IFERROR(IF(E180>1,1-(EXP((1/E180^2-G180^2)*F180)*((COS(G180/E180*F180*2)*(1-erfzR(1/E180*F180^0.5,G180*F180^0.5))-SIN(G180/E180*F180*2)*(-erfzI(1/E180*F180^0.5,G180*F180^0.5)))+(COS(G180/E180*F180*2)*(-erfzI(1/E180*F180^0.5,G180*F180^0.5))+SIN(G180/E180*F180*2)*(1-erfzR(1/E180*F180^0.5,G180*F180^0.5)))/E180/G180)),1-((1/E180+G180)*EXP((1/E180+G180)^2*F180)*ERFC((1/E180+G180)*F180^0.5)-(1/E180-G180)*EXP((1/E180-G180)^2*F180)*ERFC((1/E180-G180)*F180^0.5))/2/G180),1)","v":0.5068706161126777}]
["PCB 145",6.25,5.9017499999999989,5.7023066067735755,0.36670509442966331,6.2097076110502046E-2,2.1701315145283453,{"$f":"IFERROR(IF(E181>1,1-(EXP((1/E181^2-G181^2)*F181)*((COS(G181/E181*F181*2)*(1-erfzR(1/E181*F181^0.5,G181*F181^0.5))-SIN(G181/E181*F181*2)*(-erfzI(1/E181*F181^0.5,G181*F181^0.5)))+(COS(G181/E181*F181*2)*(-erfzI(1/E181*F181^0.5,G181*F181^0.5))+SIN(G181/E181*F181*2)*(1-erfzR(1/E181*F181^0.5,G181*F181^0.5)))/E181/G181)),1-((1/E181+G181)*EXP((1/E181+G181)^2*F181)*ERFC((1/E181+G181)*F181^0.5)-(1/E181-G181)*EXP((1/E181-G181)^2*F181)*ERFC((1/E181-G181)*F181^0.5))/2/G181),1)","v":0.68833185878152259}]
["PCB 146",6.89,6.5078299999999993,6.067207126679536,0.63899347510204052,2.68022116054367E-2,0.94028845159992769,{"$f":"IFERROR(IF(E182>1,1-(EXP((1/E182^2-G182^2)*F182)*((COS(G182/E182*F182*2)*(1-erfzR(1/E182*F182^0.5,G182*F182^0.5))-SIN(G182/E182*F182*2)*(-erfzI(1/E182*F182^0.5,G182*F182^0.5)))+(COS(G182/E182*F182*2)*(-erfzI(1/E182*F182^0.5,G182*F182^0.5))+SIN(G182/E182*F182*2)*(1-erfzR(1/E182*F182^0.5,G182*F182^0.5)))/E182/G182)),1-((1/E182+G182)*EXP((1/E182+G182)^2*F182)*ERFC((1/E182+G182)*F182^0.5)-(1/E182-G182)*EXP((1/E182-G182)^2*F182)*ERFC((1/E182-G182)*F182^0.5))/2/G182),1)","v":0.41139691014000113}]
["PCB 147",6.64,6.2710799999999987,5.9246678610912697,0.51438191279877443,3.7214303676683672E-2,1.3547580425670724,{"$f":"IFERROR(IF(E183>1,1-(EXP((1/E183^2-G183^2)*F183)*((COS(G183/E183*F183*2)*(1-erfzR(1/E183*F183^0.5,G183*F183^0.5))-SIN(G183/E183*F183*2)*(-erfzI(1/E183*F183^0.5,G183*F183^0.5)))+(COS(G183/E183*F183*2)*(-erfzI(1/E183*F183^0.5,G183*F183^0.5))+SIN(G183/E183*F183*2)*(1-erfzR(1/E183*F183^0.5,G183*F183^0.5)))/E183/G183)),1-((1/E183+G183)*EXP((1/E183+G183)^2*F183)*ERFC((1/E183+G183)*F183^0.5)-(1/E183-G183)*EXP((1/E183-G183)^2*F183)*ERFC((1/E183-G183)*F183^0.5))/2/G183),1)","v":0.52021117116610793}]
["PCB 148",6.73,6.3563099999999997,5.9759819967030463,0.55616230900334518,3.3067073570062222E-2,1.1978723393813013,{"$f":"IFERROR(IF(E184>1,1-(EXP((1/E184^2-G184^2)*F184)*((COS(G184/E184*F184*2)*(1-erfzR(1/E184*F184^0.5,G184*F184^0.5))-SIN(G184/E184*F184*2)*(-erfzI(1/E184*F184^0.5,G184*F184^0.5)))+(COS(G184/E184*F184*2)*(-erfzI(1/E184*F184^0.5,G184*F184^0.5))+SIN(G184/E184*F184*2)*(1-erfzR(1/E184*F184^0.5,G184*F184^0.5)))/E184/G184)),1-((1/E184+G184)*EXP((1/E184+G184)^2*F184)*ERFC((1/E184+G184)*F184^0.5)-(1/E184-G184)*EXP((1/E184-G184)^2*F184)*ERFC((1/E184-G184)*F184^0.5))/2/G184),1)","v":0.48032645012152531}]
["PCB 149",6.67,6.2994899999999996,5.9417725729618613,0.52794779118180313,3.5777104161243398E-2,1.3013797355615921,{"$f":"IFERROR(IF(E185>1,1-(EXP((1/E185^2-G185^2)*F185)*((COS(G185/E185*F185*2)*(1-erfzR(1/E185*F185^0.5,G185*F185^0.5))-SIN(G185/E185*F185*2)*(-erfzI(1/E185*F185^0.5,G185*F185^0.5)))+(COS(G185/E185*F185*2)*(-erfzI(1/E185*F185^0.5,G185*F185^0.5))+SIN(G185/E185*F185*2)*(1-erfzR(1/E185*F185^0.5,G185*F185^0.5)))/E185/G185)),1-((1/E185+G185)*EXP((1/E185+G185)^2*F185)*ERFC((1/E185+G185)*F185^0.5)-(1/E185-G185)*EXP((1/E185-G185)^2*F185)*ERFC((1/E185-G185)*F185^0.5))/2/G185),1)","v":0.5068706161126777}]
["PCB 150",6.32,5.9680399999999993,5.7422176011382904,0.38966908259063643,5.6644814276528066E-2,2.0048723954088539,{"$f":"IFERROR(IF(E186>1,1-(EXP((1/E186^2-G186^2)*F186)*((COS(G186/E186*F186*2)*(1-erfzR(1/E186*F186^0.5,G186*F186^0.5))-SIN(G186/E186*F186*2)*(-erfzI(1/E186*F186^0.5,G186*F186^0.5)))+(COS(G186/E186*F186*2)*(-erfzI(1/E186*F186^0.5,G186*F186^0.5))+SIN(G186/E186*F186*2)*(1-erfzR(1/E186*F186^0.5,G186*F186^0.5)))/E186/G186)),1-((1/E186+G186)*EXP((1/E186+G186)^2*F186)*ERFC((1/E186+G186)*F186^0.5)-(1/E186-G186)*EXP((1/E186-G186)^2*F186)*ERFC((1/E186-G186)*F186^0.5))/2/G186),1)","v":0.65980938376800435}]
["PCB 151",6.64,6.2710799999999987,5.9246678610912697,0.51438191279877443,3.7214303676683672E-2,1.3547580425670724,{"$f":"IFERROR(IF(E187>1,1-(EXP((1/E187^2-G187^2)*F187)*((COS(G187/E187*F187*2)*(1-erfzR(1/E187*F187^0.5,G187*F187^0.5))-SIN(G187/E187*F187*2)*(-erfzI(1/E187*F187^0.5,G187*F187^0.5)))+(COS(G187/E187*F187*2)*(-erfzI(1/E187*F187^0.5,G187*F187^0.5))+SIN(G187/E187*F187*2)*(1-erfzR(1/E187*F187^0.5,G187*F187^0.5)))/E187/G187)),1-((1/E187+G187)*EXP((1/E187+G187)^2*F187)*ERFC((1/E187+G187)*F187^0.5)-(1/E187-G187)*EXP((1/E187-G187)^2*F187)*ERFC((1/E187-G187)*F187^0.5))/2/G187),1)","v":0.52021117116610793}]
["PCB 152",6.22,5.8733399999999989,5.685201894902983,0.35728242651332798,6.4591573353600717E-2,2.2438738228520965,{"$f":"IFERROR(IF(E188>1,1-(EXP((1/E188^2-G188^2)*F188)*((COS(G188/E188*F188*2)*(1-erfzR(1/E188*F188^0.5,G188*F188^0.5))-SIN(G188/E188*F188*2)*(-erfzI(1/E188*F188^0.5,G188*F188^0.5)))+(COS(G188/E188*F188*2)*(-erfzI(1/E188*F188^0.5,G188*F188^0.5))+SIN(G188/E188*F188*2)*(1-erfzR(1/E188*F188^0.5,G188*F188^0.5)))/E188/G188)),1-((1/E188+G188)*EXP((1/E188+G188)^2*F188)*ERFC((1/E188+G188)*F188^0.5)-(1/E188-G188)*EXP((1/E188-G188)^2*F188)*ERFC((1/E188-G188)*F188^0.5))/2/G188),1)","v":0.70020014351690429}]
["PCB 153",6.92,6.5362399999999994,6.0843118385501276,0.65584575461478012,2.5767122359464975E-2,0.89448869064041425,{"$f":"IFERROR(IF(E189>1,1-(EXP((1/E189^2-G189^2)*F189)*((COS(G189/E189*F189*2)*(1-erfzR(1/E189*F189^0.5,G189*F189^0.5))-SIN(G189/E189*F189*2)*(-erfzI(1/E189*F189^0.5,G189*F189^0.5)))+(COS(G189/E189*F189*2)*(-erfzI(1/E189*F189^0.5,G189*F189^0.5))+SIN(G189/E189*F189*2)*(1-erfzR(1/E189*F189^0.5,G189*F189^0.5)))/E189/G189)),1-((1/E189+G189)*EXP((1/E189+G189)^2*F189)*ERFC((1/E189+G189)*F189^0.5)-(1/E189-G189)*EXP((1/E189-G189)^2*F189)*ERFC((1/E189-G189)*F189^0.5))/2/G189),1)","v":0.39891349367741136}]
["PCB 154",6.76,6.3847199999999988,5.993086708573637,0.57083006861431407,3.1790038198802682E-2,1.1476456152596965,{"$f":"IFERROR(IF(E190>1,1-(EXP((1/E190^2-G190^2)*F190)*((COS(G190/E190*F190*2)*(1-erfzR(1/E190*F190^0.5,G190*F190^0.5))-SIN(G190/E190*F190*2)*(-erfzI(1/E190*F190^0.5,G190*F190^0.5)))+(COS(G190/E190*F190*2)*(-erfzI(1/E190*F190^0.5,G190*F190^0.5))+SIN(G190/E190*F190*2)*(1-erfzR(1/E190*F190^0.5,G190*F190^0.5)))/E190/G190)),1-((1/E190+G190)*EXP((1/E190+G190)^2*F190)*ERFC((1/E190+G190)*F190^0.5)-(1/E190-G190)*EXP((1/E190-G190)^2*F190)*ERFC((1/E190-G190)*F190^0.5))/2/G190),1)","v":0.46715972370008707}]
["PCB 155",6.41,6.0532699999999995,5.7935317367500652,0.42131974575397613,5.0332212509407601E-2,1.805541680081814,{"$f":"IFERROR(IF(E191>1,1-(EXP((1/E191^2-G191^2)*F191)*((COS(G191/E191*F191*2)*(1-erfzR(1/E191*F191^0.5,G191*F191^0.5))-SIN(G191/E191*F191*2)*(-erfzI(1/E191*F191^0.5,G191*F191^0.5)))+(COS(G191/E191*F191*2)*(-erfzI(1/E191*F191^0.5,G191*F191^0.5))+SIN(G191/E191*F191*2)*(1-erfzR(1/E191*F191^0.5,G191*F191^0.5)))/E191/G191)),1-((1/E191+G191)*EXP((1/E191+G191)^2*F191)*ERFC((1/E191+G191)*F191^0.5)-(1/E191-G191)*EXP((1/E191-G191)^2*F191)*ERFC((1/E191-G191)*F191^0.5))/2/G191),1)","v":0.62169905198311926}]
["PCB 156",7.18,6.7824599999999986,6.2325526747619238,0.8218278896119543,1.8315765880901318E-2,0.51361652314315465,{"$f":"IFERROR(IF(E192>1,1-(EXP((1/E192^2-G192^2)*F192)*((COS(G192/E192*F192*2)*(1-erfzR(1/E192*F192^0.5,G192*F192^0.5))-SIN(G192/E192*F192*2)*(-erfzI(1/E192*F192^0.5,G192*F192^0.5)))+(COS(G192/E192*F192*2)*(-erfzI(1/E192*F192^0.5,G192*F192^0.5))+SIN(G192/E192*F192*2)*(1-erfzR(1/E192*F192^0.5,G192*F192^0.5)))/E192/G192)),1-((1/E192+G192)*EXP((1/E192+G192)^2*F192)*ERFC((1/E192+G192)*F192^0.5)-(1/E192-G192)*EXP((1/E192-G192)^2*F192)*ERFC((1/E192-G192)*F192^0.5))/2/G192),1)","v":0.29908889326566157}]
["PCB 157",7.18,6.7824599999999986,6.2325526747619238,0.8218278896119543,1.8315765880901318E-2,0.51361652314315465,{"$f":"IFERROR(IF(E193>1,1-(EXP((1/E193^2-G193^2)*F193)*((COS(G193/E193*F193*2)*(1-erfzR(1/E193*F193^0.5,G193*F193^0.5))-SIN(G193/E193*F193*2)*(-erfzI(1/E193*F193^0.5,G193*F193^0.5)))+(COS(G193/E193*F193*2)*(-erfzI(1/E193*F193^0.5,G193*F193^0.5))+SIN(G193/E193*F193*2)*(1-erfzR(1/E193*F193^0.5,G193*F193^0.5)))/E193/G193)),1-((1/E193+G193)*EXP((1/E193+G193)^2*F193)*ERFC((1/E193+G193)*F193^0.5)-(1/E193-G193)*EXP((1/E193-G193)^2*F193)*ERFC((1/E193-G193)*F193^0.5))/2/G193),1)","v":0.29908889326566157}]
["PCB 158",7.02,6.6309399999999989,6.1413275447854341,0.7152963441714969,2.2596970234834892E-2,0.74595137108637488,{"$f":"IFERROR(IF(E194>1,1-(EXP((1/E194^2-G194^2)*F194)*((COS(G194/E194*F194*2)*(1-erfzR(1/E194*F194^0.5,G194*F194^0.5))-SIN(G194/E194*F194*2)*(-erfzI(1/E194*F194^0.5,G194*F194^0.5)))+(COS(G194/E194*F194*2)*(-erfzI(1/E194*F194^0.5,G194*F194^0.5))+SIN(G194/E194*F194*2)*(1-erfzR(1/E194*F194^0.5,G194*F194^0.5)))/E194/G194)),1-((1/E194+G194)*EXP((1/E194+G194)^2*F194)*ERFC((1/E194+G194)*F194^0.5)-(1/E194-G194)*EXP((1/E194-G194)^2*F194)*ERFC((1/E194-G194)*F194^0.5))/2/G194),1)","v":0.35861928054030912}]
["PCB 159",7.24,6.8392799999999996,6.2667620985031078,0.86574790978249594,1.6928390155508656E-2,0.42322281973764775,{"$f":"IFERROR(IF(E195>1,1-(EXP((1/E195^2-G195^2)*F195)*((COS(G195/E195*F195*2)*(1-erfzR(1/E195*F195^0.5,G195*F195^0.5))-SIN(G195/E195*F195*2)*(-erfzI(1/E195*F195^0.5,G195*F195^0.5)))+(COS(G195/E195*F195*2)*(-erfzI(1/E195*F195^0.5,G195*F195^0.5))+SIN(G195/E195*F195*2)*(1-erfzR(1/E195*F195^0.5,G195*F195^0.5)))/E195/G195)),1-((1/E195+G195)*EXP((1/E195+G195)^2*F195)*ERFC((1/E195+G195)*F195^0.5)-(1/E195-G195)*EXP((1/E195-G195)^2*F195)*ERFC((1/E195-G195)*F195^0.5))/2/G195),1)","v":0.27851258576175342}]
["PCB 160",6.93,6.5457099999999988,6.0900134091736584,0.66156137475812415,2.543105336220243E-2,0.87936630404794913,{"$f":"IFERROR(IF(E196>1,1-(EXP((1/E196^2-G196^2)*F196)*((COS(G196/E196*F196*2)*(1-erfzR(1/E196*F196^0.5,G196*F196^0.5))-SIN(G196/E196*F196*2)*(-erfzI(1/E196*F196^0.5,G196*F196^0.5)))+(COS(G196/E196*F196*2)*(-erfzI(1/E196*F196^0.5,G196*F196^0.5))+SIN(G196/E196*F196*2)*(1-erfzR(1/E196*F196^0.5,G196*F196^0.5)))/E196/G196)),1-((1/E196+G196)*EXP((1/E196+G196)^2*F196)*ERFC((1/E196+G196)*F196^0.5)-(1/E196-G196)*EXP((1/E196-G196)^2*F196)*ERFC((1/E196-G196)*F196^0.5))/2/G196),1)","v":0.39479025971780923}]
["PCB 161",7.08,6.687759999999999,6.1755369685266182,0.75352311921895765,2.088530345687498E-2,0.65885752873525683,{"$f":"IFERROR(IF(E197>1,1-(EXP((1/E197^2-G197^2)*F197)*((COS(G197/E197*F197*2)*(1-erfzR(1/E197*F197^0.5,G197*F197^0.5))-SIN(G197/E197*F197*2)*(-erfzI(1/E197*F197^0.5,G197*F197^0.5)))+(COS(G197/E197*F197*2)*(-erfzI(1/E197*F197^0.5,G197*F197^0.5))+SIN(G197/E197*F197*2)*(1-erfzR(1/E197*F197^0.5,G197*F197^0.5)))/E197/G197)),1-((1/E197+G197)*EXP((1/E197+G197)^2*F197)*ERFC((1/E197+G197)*F197^0.5)-(1/E197-G197)*EXP((1/E197-G197)^2*F197)*ERFC((1/E197-G197)*F197^0.5))/2/G197),1)","v":0.33553438554257531}]
["PCB 162",7.24,6.8392799999999996,6.2667620985031078,0.86574790978249594,1.6928390155508656E-2,0.42322281973764775,{"$f":"IFERROR(IF(E198>1,1-(EXP((1/E198^2-G198^2)*F198)*((COS(G198/E198*F198*2)*(1-erfzR(1/E198*F198^0.5,G198*F198^0.5))-SIN(G198/E198*F198*2)*(-erfzI(1/E198*F198^0.5,G198*F198^0.5)))+(COS(G198/E198*F198*2)*(-erfzI(1/E198*F198^0.5,G198*F198^0.5))+SIN(G198/E198*F198*2)*(1-erfzR(1/E198*F198^0.5,G198*F198^0.5)))/E198/G198)),1-((1/E198+G198)*EXP((1/E198+G198)^2*F198)*ERFC((1/E198+G198)*F198^0.5)-(1/E198-G198)*EXP((1/E198-G198)^2*F198)*ERFC((1/E198-G198)*F198^0.5))/2/G198),1)","v":0.27851258576175342}]
["PCB 163",6.99,6.6025299999999998,6.1242228329148425,0.69691645249483669,2.3504711524503154E-2,0.78995156473081785,{"$f":"IFERROR(IF(E199>1,1-(EXP((1/E199^2-G199^2)*F199)*((COS(G199/E199*F199*2)*(1-erfzR(1/E199*F199^0.5,G199*F199^0.5))-SIN(G199/E199*F199*2)*(-erfzI(1/E199*F199^0.5,G199*F199^0.5)))+(COS(G199/E199*F199*2)*(-erfzI(1/E199*F199^0.5,G199*F199^0.5))+SIN(G199/E199*F199*2)*(1-erfzR(1/E199*F199^0.5,G199*F199^0.5)))/E199/G199)),1-((1/E199+G199)*EXP((1/E199+G199)^2*F199)*ERFC((1/E199+G199)*F199^0.5)-(1/E199-G199)*EXP((1/E199-G199)^2*F199)*ERFC((1/E199-G199)*F199^0.5))/2/G199),1)","v":0.37048010752574756}]
["PCB 164",7.02,6.6309399999999989,6.1413275447854341,0.7152963441714969,2.2596970234834892E-2,0.74595137108637488,{"$f":"IFERROR(IF(E200>1,1-(EXP((1/E200^2-G200^2)*F200)*((COS(G200/E200*F200*2)*(1-erfzR(1/E200*F200^0.5,G200*F200^0.5))-SIN(G200/E200*F200*2)*(-erfzI(1/E200*F200^0.5,G200*F200^0.5)))+(COS(G200/E200*F200*2)*(-erfzI(1/E200*F200^0.5,G200*F200^0.5))+SIN(G200/E200*F200*2)*(1-erfzR(1/E200*F200^0.5,G200*F200^0.5)))/E200/G200)),1-((1/E200+G200)*EXP((1/E200+G200)^2*F200)*ERFC((1/E200+G200)*F200^0.5)-(1/E200-G200)*EXP((1/E200-G200)^2*F200)*ERFC((1/E200-G200)*F200^0.5))/2/G200),1)","v":0.35861928054030912}]
["PCB 165",7.05,6.659349999999999,6.1584322566560257,0.73416097173986594,2.1724285501725917E-2,0.70229257499523878,{"$f":"IFERROR(IF(E201>1,1-(EXP((1/E201^2-G201^2)*F201)*((COS(G201/E201*F201*2)*(1-erfzR(1/E201*F201^0.5,G201*F201^0.5))-SIN(G201/E201*F201*2)*(-erfzI(1/E201*F201^0.5,G201*F201^0.5)))+(COS(G201/E201*F201*2)*(-erfzI(1/E201*F201^0.5,G201*F201^0.5))+SIN(G201/E201*F201*2)*(1-erfzR(1/E201*F201^0.5,G201*F201^0.5)))/E201/G201)),1-((1/E201+G201)*EXP((1/E201+G201)^2*F201)*ERFC((1/E201+G201)*F201^0.5)-(1/E201-G201)*EXP((1/E201-G201)^2*F201)*ERFC((1/E201-G201)*F201^0.5))/2/G201),1)","v":0.34696782080640287}]
["PCB 166",6.93,6.5457099999999988,6.0900134091736584,0.66156137475812415,2.543105336220243E-2,0.87936630404794913,{"$f":"IFERROR(IF(E202>1,1-(EXP((1/E202^2-G202^2)*F202)*((COS(G202/E202*F202*2)*(1-erfzR(1/E202*F202^0.5,G202*F202^0.5))-SIN(G202/E202*F202*2)*(-erfzI(1/E202*F202^0.5,G202*F202^0.5)))+(COS(G202/E202*F202*2)*(-erfzI(1/E202*F202^0.5,G202*F202^0.5))+SIN(G202/E202*F202*2)*(1-erfzR(1/E202*F202^0.5,G202*F202^0.5)))/E202/G202)),1-((1/E202+G202)*EXP((1/E202+G202)^2*F202)*ERFC((1/E202+G202)*F202^0.5)-(1/E202-G202)*EXP((1/E202-G202)^2*F202)*ERFC((1/E202-G202)*F202^0.5))/2/G202),1)","v":0.39479025971780923}]
["PCB 167",7.27,6.8676899999999987,6.2838668103736994,0.8885804211174414,1.6274623411945365E-2,0.37565053917855262,{"$f":"IFERROR(IF(E203>1,1-(EXP((1/E203^2-G203^2)*F203)*((COS(G203/E203*F203*2)*(1-erfzR(1/E203*F203^0.5,G203*F203^0.5))-SIN(G203/E203*F203*2)*(-erfzI(1/E203*F203^0.5,G203*F203^0.5)))+(COS(G203/E203*F203*2)*(-erfzI(1/E203*F203^0.5,G203*F203^0.5))+SIN(G203/E203*F203*2)*(1-erfzR(1/E203*F203^0.5,G203*F203^0.5)))/E203/G203)),1-((1/E203+G203)*EXP((1/E203+G203)^2*F203)*ERFC((1/E203+G203)*F203^0.5)-(1/E203-G203)*EXP((1/E203-G203)^2*F203)*ERFC((1/E203-G203)*F203^0.5))/2/G203),1)","v":0.26859945060085089}]
["PCB 168",7.11,6.71617,6.1926416803972097,0.77339590778281941,2.0078722517760154E-2,0.61550559412910899,{"$f":"IFERROR(IF(E204>1,1-(EXP((1/E204^2-G204^2)*F204)*((COS(G204/E204*F204*2)*(1-erfzR(1/E204*F204^0.5,G204*F204^0.5))-SIN(G204/E204*F204*2)*(-erfzI(1/E204*F204^0.5,G204*F204^0.5)))+(COS(G204/E204*F204*2)*(-erfzI(1/E204*F204^0.5,G204*F204^0.5))+SIN(G204/E204*F204*2)*(1-erfzR(1/E204*F204^0.5,G204*F204^0.5)))/E204/G204)),1-((1/E204+G204)*EXP((1/E204+G204)^2*F204)*ERFC((1/E204+G204)*F204^0.5)-(1/E204-G204)*EXP((1/E204-G204)^2*F204)*ERFC((1/E204-G204)*F204^0.5))/2/G204),1)","v":0.3243266485527051}]
["PCB 169",7.42,7.009739999999999,6.3693903697266592,1.0120994304453037,1.3365567039784004E-2,0.10868241575450166,{"$f":"IFERROR(IF(E205>1,1-(EXP((1/E205^2-G205^2)*F205)*((COS(G205/E205*F205*2)*(1-erfzR(1/E205*F205^0.5,G205*F205^0.5))-SIN(G205/E205*F205*2)*(-erfzI(1/E205*F205^0.5,G205*F205^0.5)))+(COS(G205/E205*F205*2)*(-erfzI(1/E205*F205^0.5,G205*F205^0.5))+SIN(G205/E205*F205*2)*(1-erfzR(1/E205*F205^0.5,G205*F205^0.5)))/E205/G205)),1-((1/E205+G205)*EXP((1/E205+G205)^2*F205)*ERFC((1/E205+G205)*F205^0.5)-(1/E205-G205)*EXP((1/E205-G205)^2*F205)*ERFC((1/E205-G205)*F205^0.5))/2/G205),1)","v":0.22284444246442436}]
["PCB 170",7.27,6.8676899999999987,6.2838668103736994,0.8885804211174414,1.6274623411945365E-2,0.37565053917855262,{"$f":"IFERROR(IF(E206>1,1-(EXP((1/E206^2-G206^2)*F206)*((COS(G206/E206*F206*2)*(1-erfzR(1/E206*F206^0.5,G206*F206^0.5))-SIN(G206/E206*F206*2)*(-erfzI(1/E206*F206^0.5,G206*F206^0.5)))+(COS(G206/E206*F206*2)*(-erfzI(1/E206*F206^0.5,G206*F206^0.5))+SIN(G206/E206*F206*2)*(1-erfzR(1/E206*F206^0.5,G206*F206^0.5)))/E206/G206)),1-((1/E206+G206)*EXP((1/E206+G206)^2*F206)*ERFC((1/E206+G206)*F206^0.5)-(1/E206-G206)*EXP((1/E206-G206)^2*F206)*ERFC((1/E206-G206)*F206^0.5))/2/G206),1)","v":0.26859945060085089}]
["PCB 171",7.11,6.71617,6.1926416803972097,0.77339590778281941,2.0078722517760154E-2,0.61550559412910899,{"$f":"IFERROR(IF(E207>1,1-(EXP((1/E207^2-G207^2)*F207)*((COS(G207/E207*F207*2)*(1-erfzR(1/E207*F207^0.5,G207*F207^0.5))-SIN(G207/E207*F207*2)*(-erfzI(1/E207*F207^0.5,G207*F207^0.5)))+(COS(G207/E207*F207*2)*(-erfzI(1/E207*F207^0.5,G207*F207^0.5))+SIN(G207/E207*F207*2)*(1-erfzR(1/E207*F207^0.5,G207*F207^0.5)))/E207/G207)),1-((1/E207+G207)*EXP((1/E207+G207)^2*F207)*ERFC((1/E207+G207)*F207^0.5)-(1/E207-G207)*EXP((1/E207-G207)^2*F207)*ERFC((1/E207-G207)*F207^0.5))/2/G207),1)","v":0.3243266485527051}]
["PCB 172",7.33,6.9245099999999997,6.3180762341148835,0.93606782147453271,1.5041859376389294E-2,0.27011732218908502,{"$f":"IFERROR(IF(E208>1,1-(EXP((1/E208^2-G208^2)*F208)*((COS(G208/E208*F208*2)*(1-erfzR(1/E208*F208^0.5,G208*F208^0.5))-SIN(G208/E208*F208*2)*(-erfzI(1/E208*F208^0.5,G208*F208^0.5)))+(COS(G208/E208*F208*2)*(-erfzI(1/E208*F208^0.5,G208*F208^0.5))+SIN(G208/E208*F208*2)*(1-erfzR(1/E208*F208^0.5,G208*F208^0.5)))/E208/G208)),1-((1/E208+G208)*EXP((1/E208+G208)^2*F208)*ERFC((1/E208+G208)*F208^0.5)-(1/E208-G208)*EXP((1/E208-G208)^2*F208)*ERFC((1/E208-G208)*F208^0.5))/2/G208),1)","v":0.24953350426614063}]
["PCB 173",7.02,6.6309399999999989,6.1413275447854341,0.7152963441714969,2.2596970234834892E-2,0.74595137108637488,{"$f":"IFERROR(IF(E209>1,1-(EXP((1/E209^2-G209^2)*F209)*((COS(G209/E209*F209*2)*(1-erfzR(1/E209*F209^0.5,G209*F209^0.5))-SIN(G209/E209*F209*2)*(-erfzI(1/E209*F209^0.5,G209*F209^0.5)))+(COS(G209/E209*F209*2)*(-erfzI(1/E209*F209^0.5,G209*F209^0.5))+SIN(G209/E209*F209*2)*(1-erfzR(1/E209*F209^0.5,G209*F209^0.5)))/E209/G209)),1-((1/E209+G209)*EXP((1/E209+G209)^2*F209)*ERFC((1/E209+G209)*F209^0.5)-(1/E209-G209)*EXP((1/E209-G209)^2*F209)*ERFC((1/E209-G209)*F209^0.5))/2/G209),1)","v":0.35861928054030912}]
["PCB 174",7.11,6.71617,6.1926416803972097,0.77339590778281941,2.0078722517760154E-2,0.61550559412910899,{"$f":"IFERROR(IF(E210>1,1-(EXP((1/E210^2-G210^2)*F210)*((COS(G210/E210*F210*2)*(1-erfzR(1/E210*F210^0.5,G210*F210^0.5))-SIN(G210/E210*F210*2)*(-erfzI(1/E210*F210^0.5,G210*F210^0.5)))+(COS(G210/E210*F210*2)*(-erfzI(1/E210*F210^0.5,G210*F210^0.5))+SIN(G210/E210*F210*2)*(1-erfzR(1/E210*F210^0.5,G210*F210^0.5)))/E210/G210)),1-((1/E210+G210)*EXP((1/E210+G210)^2*F210)*ERFC((1/E210+G210)*F210^0.5)-(1/E210-G210)*EXP((1/E210-G210)^2*F210)*ERFC((1/E210-G210)*F210^0.5))/2/G210),1)","v":0.3243266485527051}]
["PCB 175",7.17,6.7729899999999992,6.2268511041383938,0.81472763222170652,1.855780701801122E-2,0.52831492512170186,{"$f":"IFERROR(IF(E211>1,1-(EXP((1/E211^2-G211^2)*F211)*((COS(G211/E211*F211*2)*(1-erfzR(1/E211*F211^0.5,G211*F211^0.5))-SIN(G211/E211*F211*2)*(-erfzI(1/E211*F211^0.5,G211*F211^0.5)))+(COS(G211/E211*F211*2)*(-erfzI(1/E211*F211^0.5,G211*F211^0.5))+SIN(G211/E211*F211*2)*(1-erfzR(1/E211*F211^0.5,G211*F211^0.5)))/E211/G211)),1-((1/E211+G211)*EXP((1/E211+G211)^2*F211)*ERFC((1/E211+G211)*F211^0.5)-(1/E211-G211)*EXP((1/E211-G211)^2*F211)*ERFC((1/E211-G211)*F211^0.5))/2/G211),1)","v":0.30261415640203726}]
["PCB 176",6.76,6.3847199999999988,5.993086708573637,0.57083006861431407,3.1790038198802682E-2,1.1476456152596965,{"$f":"IFERROR(IF(E212>1,1-(EXP((1/E212^2-G212^2)*F212)*((COS(G212/E212*F212*2)*(1-erfzR(1/E212*F212^0.5,G212*F212^0.5))-SIN(G212/E212*F212*2)*(-erfzI(1/E212*F212^0.5,G212*F212^0.5)))+(COS(G212/E212*F212*2)*(-erfzI(1/E212*F212^0.5,G212*F212^0.5))+SIN(G212/E212*F212*2)*(1-erfzR(1/E212*F212^0.5,G212*F212^0.5)))/E212/G212)),1-((1/E212+G212)*EXP((1/E212+G212)^2*F212)*ERFC((1/E212+G212)*F212^0.5)-(1/E212-G212)*EXP((1/E212-G212)^2*F212)*ERFC((1/E212-G212)*F212^0.5))/2/G212),1)","v":0.46715972370008707}]
["PCB 177",7.08,6.687759999999999,6.1755369685266182,0.75352311921895765,2.088530345687498E-2,0.65885752873525683,{"$f":"IFERROR(IF(E213>1,1-(EXP((1/E213^2-G213^2)*F213)*((COS(G213/E213*F213*2)*(1-erfzR(1/E213*F213^0.5,G213*F213^0.5))-SIN(G213/E213*F213*2)*(-erfzI(1/E213*F213^0.5,G213*F213^0.5)))+(COS(G213/E213*F213*2)*(-erfzI(1/E213*F213^0.5,G213*F213^0.5))+SIN(G213/E213*F213*2)*(1-erfzR(1/E213*F213^0.5,G213*F213^0.5)))/E213/G213)),1-((1/E213+G213)*EXP((1/E213+G213)^2*F213)*ERFC((1/E213+G213)*F213^0.5)-(1/E213-G213)*EXP((1/E213-G213)^2*F213)*ERFC((1/E213-G213)*F213^0.5))/2/G213),1)","v":0.33553438554257531}]
["PCB 178",7.14,6.7445799999999991,6.2097463922678013,0.79379280465235635,1.93032913683856E-2,0.57206417296374523,{"$f":"IFERROR(IF(E214>1,1-(EXP((1/E214^2-G214^2)*F214)*((COS(G214/E214*F214*2)*(1-erfzR(1/E214*F214^0.5,G214*F214^0.5))-SIN(G214/E214*F214*2)*(-erfzI(1/E214*F214^0.5,G214*F214^0.5)))+(COS(G214/E214*F214*2)*(-erfzI(1/E214*F214^0.5,G214*F214^0.5))+SIN(G214/E214*F214*2)*(1-erfzR(1/E214*F214^0.5,G214*F214^0.5)))/E214/G214)),1-((1/E214+G214)*EXP((1/E214+G214)^2*F214)*ERFC((1/E214+G214)*F214^0.5)-(1/E214-G214)*EXP((1/E214-G214)^2*F214)*ERFC((1/E214-G214)*F214^0.5))/2/G214),1)","v":0.31335131741894517}]
["PCB 179",6.73,6.3563099999999997,5.9759819967030463,0.55616230900334518,3.3067073570062222E-2,1.1978723393813013,{"$f":"IFERROR(IF(E215>1,1-(EXP((1/E215^2-G215^2)*F215)*((COS(G215/E215*F215*2)*(1-erfzR(1/E215*F215^0.5,G215*F215^0.5))-SIN(G215/E215*F215*2)*(-erfzI(1/E215*F215^0.5,G215*F215^0.5)))+(COS(G215/E215*F215*2)*(-erfzI(1/E215*F215^0.5,G215*F215^0.5))+SIN(G215/E215*F215*2)*(1-erfzR(1/E215*F215^0.5,G215*F215^0.5)))/E215/G215)),1-((1/E215+G215)*EXP((1/E215+G215)^2*F215)*ERFC((1/E215+G215)*F215^0.5)-(1/E215-G215)*EXP((1/E215-G215)^2*F215)*ERFC((1/E215-G215)*F215^0.5))/2/G215),1)","v":0.48032645012152531}]
["PCB 180",7.36,6.9529199999999998,6.335180945985476,0.96075489135087033,1.4460949595169524E-2,0.20619596559374317,{"$f":"IFERROR(IF(E216>1,1-(EXP((1/E216^2-G216^2)*F216)*((COS(G216/E216*F216*2)*(1-erfzR(1/E216*F216^0.5,G216*F216^0.5))-SIN(G216/E216*F216*2)*(-erfzI(1/E216*F216^0.5,G216*F216^0.5)))+(COS(G216/E216*F216*2)*(-erfzI(1/E216*F216^0.5,G216*F216^0.5))+SIN(G216/E216*F216*2)*(1-erfzR(1/E216*F216^0.5,G216*F216^0.5)))/E216/G216)),1-((1/E216+G216)*EXP((1/E216+G216)^2*F216)*ERFC((1/E216+G216)*F216^0.5)-(1/E216-G216)*EXP((1/E216-G216)^2*F216)*ERFC((1/E216-G216)*F216^0.5))/2/G216),1)","v":0.24038257406798957}]
["PCB 181",7.11,6.71617,6.1926416803972097,0.77339590778281941,2.0078722517760154E-2,0.61550559412910899,{"$f":"IFERROR(IF(E217>1,1-(EXP((1/E217^2-G217^2)*F217)*((COS(G217/E217*F217*2)*(1-erfzR(1/E217*F217^0.5,G217*F217^0.5))-SIN(G217/E217*F217*2)*(-erfzI(1/E217*F217^0.5,G217*F217^0.5)))+(COS(G217/E217*F217*2)*(-erfzI(1/E217*F217^0.5,G217*F217^0.5))+SIN(G217/E217*F217*2)*(1-erfzR(1/E217*F217^0.5,G217*F217^0.5)))/E217/G217)),1-((1/E217+G217)*EXP((1/E217+G217)^2*F217)*ERFC((1/E217+G217)*F217^0.5)-(1/E217-G217)*EXP((1/E217-G217)^2*F217)*ERFC((1/E217-G217)*F217^0.5))/2/G217),1)","v":0.3243266485527051}]
["PCB 182",7.2,6.8013999999999992,6.2439558160089854,0.83621457742527083,1.784111293485334E-2,0.48397161236392433,{"$f":"IFERROR(IF(E218>1,1-(EXP((1/E218^2-G218^2)*F218)*((COS(G218/E218*F218*2)*(1-erfzR(1/E218*F218^0.5,G218*F218^0.5))-SIN(G218/E218*F218*2)*(-erfzI(1/E218*F218^0.5,G218*F218^0.5)))+(COS(G218/E218*F218*2)*(-erfzI(1/E218*F218^0.5,G218*F218^0.5))+SIN(G218/E218*F218*2)*(1-erfzR(1/E218*F218^0.5,G218*F218^0.5)))/E218/G218)),1-((1/E218+G218)*EXP((1/E218+G218)^2*F218)*ERFC((1/E218+G218)*F218^0.5)-(1/E218-G218)*EXP((1/E218-G218)^2*F218)*ERFC((1/E218-G218)*F218^0.5))/2/G218),1)","v":0.29212001433979728}]
["PCB 183",7.2,6.8013999999999992,6.2439558160089854,0.83621457742527083,1.784111293485334E-2,0.48397161236392433,{"$f":"IFERROR(IF(E219>1,1-(EXP((1/E219^2-G219^2)*F219)*((COS(G219/E219*F219*2)*(1-erfzR(1/E219*F219^0.5,G219*F219^0.5))-SIN(G219/E219*F219*2)*(-erfzI(1/E219*F219^0.5,G219*F219^0.5)))+(COS(G219/E219*F219*2)*(-erfzI(1/E219*F219^0.5,G219*F219^0.5))+SIN(G219/E219*F219*2)*(1-erfzR(1/E219*F219^0.5,G219*F219^0.5)))/E219/G219)),1-((1/E219+G219)*EXP((1/E219+G219)^2*F219)*ERFC((1/E219+G219)*F219^0.5)-(1/E219-G219)*EXP((1/E219-G219)^2*F219)*ERFC((1/E219-G219)*F219^0.5))/2/G219),1)","v":0.29212001433979728}]
["PCB 184",6.85,6.469949999999999,6.0444008441854127,0.61719543613359873,2.8247298163838055E-2,1.0024572184403253,{"$f":"IFERROR(IF(E220>1,1-(EXP((1/E220^2-G220^2)*F220)*((COS(G220/E220*F220*2)*(1-erfzR(1/E220*F220^0.5,G220*F220^0.5))-SIN(G220/E220*F220*2)*(-erfzI(1/E220*F220^0.5,G220*F220^0.5)))+(COS(G220/E220*F220*2)*(-erfzI(1/E220*F220^0.5,G220*F220^0.5))+SIN(G220/E220*F220*2)*(1-erfzR(1/E220*F220^0.5,G220*F220^0.5)))/E220/G220)),1-((1/E220+G220)*EXP((1/E220+G220)^2*F220)*ERFC((1/E220+G220)*F220^0.5)-(1/E220-G220)*EXP((1/E220-G220)^2*F220)*ERFC((1/E220-G220)*F220^0.5))/2/G220),1)","v":0.42828856405189564}]
["PCB 185",7.11,6.71617,6.1926416803972097,0.77339590778281941,2.0078722517760154E-2,0.61550559412910899,{"$f":"IFERROR(IF(E221>1,1-(EXP((1/E221^2-G221^2)*F221)*((COS(G221/E221*F221*2)*(1-erfzR(1/E221*F221^0.5,G221*F221^0.5))-SIN(G221/E221*F221*2)*(-erfzI(1/E221*F221^0.5,G221*F221^0.5)))+(COS(G221/E221*F221*2)*(-erfzI(1/E221*F221^0.5,G221*F221^0.5))+SIN(G221/E221*F221*2)*(1-erfzR(1/E221*F221^0.5,G221*F221^0.5)))/E221/G221)),1-((1/E221+G221)*EXP((1/E221+G221)^2*F221)*ERFC((1/E221+G221)*F221^0.5)-(1/E221-G221)*EXP((1/E221-G221)^2*F221)*ERFC((1/E221-G221)*F221^0.5))/2/G221),1)","v":0.3243266485527051}]
["PCB 186",6.69,6.3184299999999993,5.953175714208923,0.5371898966755061,3.4849940754502741E-2,1.2664078083772417,{"$f":"IFERROR(IF(E222>1,1-(EXP((1/E222^2-G222^2)*F222)*((COS(G222/E222*F222*2)*(1-erfzR(1/E222*F222^0.5,G222*F222^0.5))-SIN(G222/E222*F222*2)*(-erfzI(1/E222*F222^0.5,G222*F222^0.5)))+(COS(G222/E222*F222*2)*(-erfzI(1/E222*F222^0.5,G222*F222^0.5))+SIN(G222/E222*F222*2)*(1-erfzR(1/E222*F222^0.5,G222*F222^0.5)))/E222/G222)),1-((1/E222+G222)*EXP((1/E222+G222)^2*F222)*ERFC((1/E222+G222)*F222^0.5)-(1/E222-G222)*EXP((1/E222-G222)^2*F222)*ERFC((1/E222-G222)*F222^0.5))/2/G222),1)","v":0.49799763788137119}]
["PCB 187",7.17,6.7729899999999992,6.2268511041383938,0.81472763222170652,1.855780701801122E-2,0.52831492512170186,{"$f":"IFERROR(IF(E223>1,1-(EXP((1/E223^2-G223^2)*F223)*((COS(G223/E223*F223*2)*(1-erfzR(1/E223*F223^0.5,G223*F223^0.5))-SIN(G223/E223*F223*2)*(-erfzI(1/E223*F223^0.5,G223*F223^0.5)))+(COS(G223/E223*F223*2)*(-erfzI(1/E223*F223^0.5,G223*F223^0.5))+SIN(G223/E223*F223*2)*(1-erfzR(1/E223*F223^0.5,G223*F223^0.5)))/E223/G223)),1-((1/E223+G223)*EXP((1/E223+G223)^2*F223)*ERFC((1/E223+G223)*F223^0.5)-(1/E223-G223)*EXP((1/E223-G223)^2*F223)*ERFC((1/E223-G223)*F223^0.5))/2/G223),1)","v":0.30261415640203726}]
["PCB 188",6.82,6.4415399999999998,6.027296132314822,0.60133629558031565,2.9382018376256501E-2,1.0499918572424012,{"$f":"IFERROR(IF(E224>1,1-(EXP((1/E224^2-G224^2)*F224)*((COS(G224/E224*F224*2)*(1-erfzR(1/E224*F224^0.5,G224*F224^0.5))-SIN(G224/E224*F224*2)*(-erfzI(1/E224*F224^0.5,G224*F224^0.5)))+(COS(G224/E224*F224*2)*(-erfzI(1/E224*F224^0.5,G224*F224^0.5))+SIN(G224/E224*F224*2)*(1-erfzR(1/E224*F224^0.5,G224*F224^0.5)))/E224/G224)),1-((1/E224+G224)*EXP((1/E224+G224)^2*F224)*ERFC((1/E224+G224)*F224^0.5)-(1/E224-G224)*EXP((1/E224-G224)^2*F224)*ERFC((1/E224-G224)*F224^0.5))/2/G224),1)","v":0.44112441238450684}]
["PCB 189",7.71,7.2843699999999991,6.5347359178090469,1.3016901915430377,9.1335968975231312E-3,0.42196163165171324,{"$f":"IFERROR(IF(E225>1,1-(EXP((1/E225^2-G225^2)*F225)*((COS(G225/E225*F225*2)*(1-erfzR(1/E225*F225^0.5,G225*F225^0.5))-SIN(G225/E225*F225*2)*(-erfzI(1/E225*F225^0.5,G225*F225^0.5)))+(COS(G225/E225*F225*2)*(-erfzI(1/E225*F225^0.5,G225*F225^0.5))+SIN(G225/E225*F225*2)*(1-erfzR(1/E225*F225^0.5,G225*F225^0.5)))/E225/G225)),1-((1/E225+G225)*EXP((1/E225+G225)^2*F225)*ERFC((1/E225+G225)*F225^0.5)-(1/E225-G225)*EXP((1/E225-G225)^2*F225)*ERFC((1/E225-G225)*F225^0.5))/2/G225),1)","v":0.15194745376461516}]
["PCB 190",7.46,7.0476199999999993,6.3921966522207816,1.0478446442514737,1.2681806024391427E-2,0.20874677127845329,{"$f":"IFERROR(IF(E226>1,1-(EXP((1/E226^2-G226^2)*F226)*((COS(G226/E226*F226*2)*(1-erfzR(1/E226*F226^0.5,G226*F226^0.5))-SIN(G226/E226*F226*2)*(-erfzI(1/E226*F226^0.5,G226*F226^0.5)))+(COS(G226/E226*F226*2)*(-erfzI(1/E226*F226^0.5,G226*F226^0.5))+SIN(G226/E226*F226*2)*(1-erfzR(1/E226*F226^0.5,G226*F226^0.5)))/E226/G226)),1-((1/E226+G226)*EXP((1/E226+G226)^2*F226)*ERFC((1/E226+G226)*F226^0.5)-(1/E226-G226)*EXP((1/E226-G226)^2*F226)*ERFC((1/E226-G226)*F226^0.5))/2/G226),1)","v":0.21171475574111742}]
["PCB 191",7.55,7.1328499999999995,6.4435107878325573,1.1329552659672681,1.1268522352402659E-2,0.32183999232992622,{"$f":"IFERROR(IF(E227>1,1-(EXP((1/E227^2-G227^2)*F227)*((COS(G227/E227*F227*2)*(1-erfzR(1/E227*F227^0.5,G227*F227^0.5))-SIN(G227/E227*F227*2)*(-erfzI(1/E227*F227^0.5,G227*F227^0.5)))+(COS(G227/E227*F227*2)*(-erfzI(1/E227*F227^0.5,G227*F227^0.5))+SIN(G227/E227*F227*2)*(1-erfzR(1/E227*F227^0.5,G227*F227^0.5)))/E227/G227)),1-((1/E227+G227)*EXP((1/E227+G227)^2*F227)*ERFC((1/E227+G227)*F227^0.5)-(1/E227-G227)*EXP((1/E227-G227)^2*F227)*ERFC((1/E227-G227)*F227^0.5))/2/G227),1)","v":0.18829055196406386}]
["PCB 192",7.52,7.1044399999999985,6.4264060759619648,1.103843422697468,1.1721189365127114E-2,0.29193221525988172,{"$f":"IFERROR(IF(E228>1,1-(EXP((1/E228^2-G228^2)*F228)*((COS(G228/E228*F228*2)*(1-erfzR(1/E228*F228^0.5,G228*F228^0.5))-SIN(G228/E228*F228*2)*(-erfzI(1/E228*F228^0.5,G228*F228^0.5)))+(COS(G228/E228*F228*2)*(-erfzI(1/E228*F228^0.5,G228*F228^0.5))+SIN(G228/E228*F228*2)*(1-erfzR(1/E228*F228^0.5,G228*F228^0.5)))/E228/G228)),1-((1/E228+G228)*EXP((1/E228+G228)^2*F228)*ERFC((1/E228+G228)*F228^0.5)-(1/E228-G228)*EXP((1/E228-G228)^2*F228)*ERFC((1/E228-G228)*F228^0.5))/2/G228),1)","v":0.1958526770641118}]
["PCB 193",7.52,7.1044399999999985,6.4264060759619648,1.103843422697468,1.1721189365127114E-2,0.29193221525988172,{"$f":"IFERROR(IF(E229>1,1-(EXP((1/E229^2-G229^2)*F229)*((COS(G229/E229*F229*2)*(1-erfzR(1/E229*F229^0.5,G229*F229^0.5))-SIN(G229/E229*F229*2)*(-erfzI(1/E229*F229^0.5,G229*F229^0.5)))+(COS(G229/E229*F229*2)*(-erfzI(1/E229*F229^0.5,G229*F229^0.5))+SIN(G229/E229*F229*2)*(1-erfzR(1/E229*F229^0.5,G229*F229^0.5)))/E229/G229)),1-((1/E229+G229)*EXP((1/E229+G229)^2*F229)*ERFC((1/E229+G229)*F229^0.5)-(1/E229-G229)*EXP((1/E229-G229)^2*F229)*ERFC((1/E229-G229)*F229^0.5))/2/G229),1)","v":0.1958526770641118}]
["PCB 194",7.8,{"$f":"B230*0.947-0.017","v":7.3695999999999993},{"$f":"B230*$B$30+$B$31","v":6.5860500534208226},{"$f":"10^C230*($C$8^2-$C$7^2)/10^D230/$C$8^2","v":1.407419282292669},{"$f":"$B$29*$C$9*86400/10^D230/$C$8^2","v":8.1157321441142297E-3},{"$f":"IF(E230>1,(1/E230-1/E230^2)^0.5,(1/E230^2-1/E230)^0.5)","v":0.45352088652752387},{"$f":"IFERROR(IF(E230>1,1-(EXP((1/E230^2-G230^2)*F230)*((COS(G230/E230*F230*2)*(1-erfzR(1/E230*F230^0.5,G230*F230^0.5))-SIN(G230/E230*F230*2)*(-erfzI(1/E230*F230^0.5,G230*F230^0.5)))+(COS(G230/E230*F230*2)*(-erfzI(1/E230*F230^0.5,G230*F230^0.5))+SIN(G230/E230*F230*2)*(1-erfzR(1/E230*F230^0.5,G230*F230^0.5)))/E230/G230)),1-((1/E230+G230)*EXP((1/E230+G230)^2*F230)*ERFC((1/E230+G230)*F230^0.5)-(1/E230-G230)*EXP((1/E230-G230)^2*F230)*ERFC((1/E230-G230)*F230^0.5))/2/G230),1)","v":0.13428857662755367}]
["PCB 195",7.56,7.1423199999999989,6.4492123584560881,1.1428288404992415,1.1121552079402344E-2,0.33069434132349151,{"$f":"IFERROR(IF(E231>1,1-(EXP((1/E231^2-G231^2)*F231)*((COS(G231/E231*F231*2)*(1-erfzR(1/E231*F231^0.5,G231*F231^0.5))-SIN(G231/E231*F231*2)*(-erfzI(1/E231*F231^0.5,G231*F231^0.5)))+(COS(G231/E231*F231*2)*(-erfzI(1/E231*F231^0.5,G231*F231^0.5))+SIN(G231/E231*F231*2)*(1-erfzR(1/E231*F231^0.5,G231*F231^0.5)))/E231/G231)),1-((1/E231+G231)*EXP((1/E231+G231)^2*F231)*ERFC((1/E231+G231)*F231^0.5)-(1/E231-G231)*EXP((1/E231-G231)^2*F231)*ERFC((1/E231-G231)*F231^0.5))/2/G231),1)","v":0.18582373027267085}]
["PCB 196",7.65,7.2275499999999999,6.5005264940678638,1.235654502836923,9.8821459624217518E-3,0.39286271637912434,{"$f":"IFERROR(IF(E232>1,1-(EXP((1/E232^2-G232^2)*F232)*((COS(G232/E232*F232*2)*(1-erfzR(1/E232*F232^0.5,G232*F232^0.5))-SIN(G232/E232*F232*2)*(-erfzI(1/E232*F232^0.5,G232*F232^0.5)))+(COS(G232/E232*F232*2)*(-erfzI(1/E232*F232^0.5,G232*F232^0.5))+SIN(G232/E232*F232*2)*(1-erfzR(1/E232*F232^0.5,G232*F232^0.5)))/E232/G232)),1-((1/E232+G232)*EXP((1/E232+G232)^2*F232)*ERFC((1/E232+G232)*F232^0.5)-(1/E232-G232)*EXP((1/E232-G232)^2*F232)*ERFC((1/E232-G232)*F232^0.5))/2/G232),1)","v":0.1648083304738891}]
["PCB 197",7.3,6.8960999999999988,6.3009715222442919,0.91201509801116964,1.5646104843256504E-2,0.32523857482890117,{"$f":"IFERROR(IF(E233>1,1-(EXP((1/E233^2-G233^2)*F233)*((COS(G233/E233*F233*2)*(1-erfzR(1/E233*F233^0.5,G233*F233^0.5))-SIN(G233/E233*F233*2)*(-erfzI(1/E233*F233^0.5,G233*F233^0.5)))+(COS(G233/E233*F233*2)*(-erfzI(1/E233*F233^0.5,G233*F233^0.5))+SIN(G233/E233*F233*2)*(1-erfzR(1/E233*F233^0.5,G233*F233^0.5)))/E233/G233)),1-((1/E233+G233)*EXP((1/E233+G233)^2*F233)*ERFC((1/E233+G233)*F233^0.5)-(1/E233-G233)*EXP((1/E233-G233)^2*F233)*ERFC((1/E233-G233)*F233^0.5))/2/G233),1)","v":0.25893932491459049}]
["PCB 198",7.62,7.199139999999999,6.4834217821972722,1.203903752120828,1.0279120947448291E-2,0.37507735154611821,{"$f":"IFERROR(IF(E234>1,1-(EXP((1/E234^2-G234^2)*F234)*((COS(G234/E234*F234*2)*(1-erfzR(1/E234*F234^0.5,G234*F234^0.5))-SIN(G234/E234*F234*2)*(-erfzI(1/E234*F234^0.5,G234*F234^0.5)))+(COS(G234/E234*F234*2)*(-erfzI(1/E234*F234^0.5,G234*F234^0.5))+SIN(G234/E234*F234*2)*(1-erfzR(1/E234*F234^0.5,G234*F234^0.5)))/E234/G234)),1-((1/E234+G234)*EXP((1/E234+G234)^2*F234)*ERFC((1/E234+G234)*F234^0.5)-(1/E234-G234)*EXP((1/E234-G234)^2*F234)*ERFC((1/E234-G234)*F234^0.5))/2/G234),1)","v":0.17157931414189542}]
["PCB 199",7.2,6.8013999999999992,6.2439558160089854,0.83621457742527083,1.784111293485334E-2,0.48397161236392433,{"$f":"IFERROR(IF(E235>1,1-(EXP((1/E235^2-G235^2)*F235)*((COS(G235/E235*F235*2)*(1-erfzR(1/E235*F235^0.5,G235*F235^0.5))-SIN(G235/E235*F235*2)*(-erfzI(1/E235*F235^0.5,G235*F235^0.5)))+(COS(G235/E235*F235*2)*(-erfzI(1/E235*F235^0.5,G235*F235^0.5))+SIN(G235/E235*F235*2)*(1-erfzR(1/E235*F235^0.5,G235*F235^0.5)))/E235/G235)),1-((1/E235+G235)*EXP((1/E235+G235)^2*F235)*ERFC((1/E235+G235)*F235^0.5)-(1/E235-G235)*EXP((1/E235-G235)^2*F235)*ERFC((1/E235-G235)*F235^0.5))/2/G235),1)","v":0.29212001433979728}]
["PCB 200",7.27,6.8676899999999987,6.2838668103736994,0.8885804211174414,1.6274623411945365E-2,0.37565053917855262,{"$f":"IFERROR(IF(E236>1,1-(EXP((1/E236^2-G236^2)*F236)*((COS(G236/E236*F236*2)*(1-erfzR(1/E236*F236^0.5,G236*F236^0.5))-SIN(G236/E236*F236*2)*(-erfzI(1/E236*F236^0.5,G236*F236^0.5)))+(COS(G236/E236*F236*2)*(-erfzI(1/E236*F236^0.5,G236*F236^0.5))+SIN(G236/E236*F236*2)*(1-erfzR(1/E236*F236^0.5,G236*F236^0.5)))/E236/G236)),1-((1/E236+G236)*EXP((1/E236+G236)^2*F236)*ERFC((1/E236+G236)*F236^0.5)-(1/E236-G236)*EXP((1/E236-G236)^2*F236)*ERFC((1/E236-G236)*F236^0.5))/2/G236),1)","v":0.26859945060085089}]
["PCB 201",7.62,7.199139999999999,6.4834217821972722,1.203903752120828,1.0279120947448291E-2,0.37507735154611821,{"$f":"IFERROR(IF(E237>1,1-(EXP((1/E237^2-G237^2)*F237)*((COS(G237/E237*F237*2)*(1-erfzR(1/E237*F237^0.5,G237*F237^0.5))-SIN(G237/E237*F237*2)*(-erfzI(1/E237*F237^0.5,G237*F237^0.5)))+(COS(G237/E237*F237*2)*(-erfzI(1/E237*F237^0.5,G237*F237^0.5))+SIN(G237/E237*F237*2)*(1-erfzR(1/E237*F237^0.5,G237*F237^0.5)))/E237/G237)),1-((1/E237+G237)*EXP((1/E237+G237)^2*F237)*ERFC((1/E237+G237)*F237^0.5)-(1/E237-G237)*EXP((1/E237-G237)^2*F237)*ERFC((1/E237-G237)*F237^0.5))/2/G237),1)","v":0.17157931414189542}]
["PCB 202",7.24,6.8392799999999996,6.2667620985031078,0.86574790978249594,1.6928390155508656E-2,0.42322281973764775,{"$f":"IFERROR(IF(E238>1,1-(EXP((1/E238^2-G238^2)*F238)*((COS(G238/E238*F238*2)*(1-erfzR(1/E238*F238^0.5,G238*F238^0.5))-SIN(G238/E238*F238*2)*(-erfzI(1/E238*F238^0.5,G238*F238^0.5)))+(COS(G238/E238*F238*2)*(-erfzI(1/E238*F238^0.5,G238*F238^0.5))+SIN(G238/E238*F238*2)*(1-erfzR(1/E238*F238^0.5,G238*F238^0.5)))/E238/G238)),1-((1/E238+G238)*EXP((1/E238+G238)^2*F238)*ERFC((1/E238+G238)*F238^0.5)-(1/E238-G238)*EXP((1/E238-G238)^2*F238)*ERFC((1/E238-G238)*F238^0.5))/2/G238),1)","v":0.27851258576175342}]
["PCB 203",7.65,7.2275499999999999,6.5005264940678638,1.235654502836923,9.8821459624217518E-3,0.39286271637912434,{"$f":"IFERROR(IF(E239>1,1-(EXP((1/E239^2-G239^2)*F239)*((COS(G239/E239*F239*2)*(1-erfzR(1/E239*F239^0.5,G239*F239^0.5))-SIN(G239/E239*F239*2)*(-erfzI(1/E239*F239^0.5,G239*F239^0.5)))+(COS(G239/E239*F239*2)*(-erfzI(1/E239*F239^0.5,G239*F239^0.5))+SIN(G239/E239*F239*2)*(1-erfzR(1/E239*F239^0.5,G239*F239^0.5)))/E239/G239)),1-((1/E239+G239)*EXP((1/E239+G239)^2*F239)*ERFC((1/E239+G239)*F239^0.5)-(1/E239-G239)*EXP((1/E239-G239)^2*F239)*ERFC((1/E239-G239)*F239^0.5))/2/G239),1)","v":0.1648083304738891}]
["PCB 204",7.3,6.8960999999999988,6.3009715222442919,0.91201509801116964,1.5646104843256504E-2,0.32523857482890117,{"$f":"IFERROR(IF(E240>1,1-(EXP((1/E240^2-G240^2)*F240)*((COS(G240/E240*F240*2)*(1-erfzR(1/E240*F240^0.5,G240*F240^0.5))-SIN(G240/E240*F240*2)*(-erfzI(1/E240*F240^0.5,G240*F240^0.5)))+(COS(G240/E240*F240*2)*(-erfzI(1/E240*F240^0.5,G240*F240^0.5))+SIN(G240/E240*F240*2)*(1-erfzR(1/E240*F240^0.5,G240*F240^0.5)))/E240/G240)),1-((1/E240+G240)*EXP((1/E240+G240)^2*F240)*ERFC((1/E240+G240)*F240^0.5)-(1/E240-G240)*EXP((1/E240-G240)^2*F240)*ERFC((1/E240-G240)*F240^0.5))/2/G240),1)","v":0.25893932491459049}]
["PCB 205",8,7.5589999999999993,6.7000814658914356,1.6741411997572666,6.2416051663298647E-3,0.49043713926044447,{"$f":"IFERROR(IF(E241>1,1-(EXP((1/E241^2-G241^2)*F241)*((COS(G241/E241*F241*2)*(1-erfzR(1/E241*F241^0.5,G241*F241^0.5))-SIN(G241/E241*F241*2)*(-erfzI(1/E241*F241^0.5,G241*F241^0.5)))+(COS(G241/E241*F241*2)*(-erfzI(1/E241*F241^0.5,G241*F241^0.5))+SIN(G241/E241*F241*2)*(1-erfzR(1/E241*F241^0.5,G241*F241^0.5)))/E241/G241)),1-((1/E241+G241)*EXP((1/E241+G241)^2*F241)*ERFC((1/E241+G241)*F241^0.5)-(1/E241-G241)*EXP((1/E241-G241)^2*F241)*ERFC((1/E241-G241)*F241^0.5))/2/G241),1)","v":0.10142424003671902}]
["PCB 206",8.09,7.6442299999999994,6.7513956015032113,1.8101224247728811,5.5460292640010771E-3,0.49724151188608695,{"$f":"IFERROR(IF(E242>1,1-(EXP((1/E242^2-G242^2)*F242)*((COS(G242/E242*F242*2)*(1-erfzR(1/E242*F242^0.5,G242*F242^0.5))-SIN(G242/E242*F242*2)*(-erfzI(1/E242*F242^0.5,G242*F242^0.5)))+(COS(G242/E242*F242*2)*(-erfzI(1/E242*F242^0.5,G242*F242^0.5))+SIN(G242/E242*F242*2)*(1-erfzR(1/E242*F242^0.5,G242*F242^0.5)))/E242/G242)),1-((1/E242+G242)*EXP((1/E242+G242)^2*F242)*ERFC((1/E242+G242)*F242^0.5)-(1/E242-G242)*EXP((1/E242-G242)^2*F242)*ERFC((1/E242-G242)*F242^0.5))/2/G242),1)","v":8.918345172279063E-2}]
["PCB 207",7.74,7.3127799999999992,6.5518406296796394,1.3360198800322201,8.7808615313211269E-3,0.43387993428428423,{"$f":"IFERROR(IF(E243>1,1-(EXP((1/E243^2-G243^2)*F243)*((COS(G243/E243*F243*2)*(1-erfzR(1/E243*F243^0.5,G243*F243^0.5))-SIN(G243/E243*F243*2)*(-erfzI(1/E243*F243^0.5,G243*F243^0.5)))+(COS(G243/E243*F243*2)*(-erfzI(1/E243*F243^0.5,G243*F243^0.5))+SIN(G243/E243*F243*2)*(1-erfzR(1/E243*F243^0.5,G243*F243^0.5)))/E243/G243)),1-((1/E243+G243)*EXP((1/E243+G243)^2*F243)*ERFC((1/E243+G243)*F243^0.5)-(1/E243-G243)*EXP((1/E243-G243)^2*F243)*ERFC((1/E243-G243)*F243^0.5))/2/G243),1)","v":0.14584835812345998}]
["PCB 208",7.71,7.2843699999999991,6.5347359178090469,1.3016901915430377,9.1335968975231312E-3,0.42196163165171324,{"$f":"IFERROR(IF(E244>1,1-(EXP((1/E244^2-G244^2)*F244)*((COS(G244/E244*F244*2)*(1-erfzR(1/E244*F244^0.5,G244*F244^0.5))-SIN(G244/E244*F244*2)*(-erfzI(1/E244*F244^0.5,G244*F244^0.5)))+(COS(G244/E244*F244*2)*(-erfzI(1/E244*F244^0.5,G244*F244^0.5))+SIN(G244/E244*F244*2)*(1-erfzR(1/E244*F244^0.5,G244*F244^0.5)))/E244/G244)),1-((1/E244+G244)*EXP((1/E244+G244)^2*F244)*ERFC((1/E244+G244)*F244^0.5)-(1/E244-G244)*EXP((1/E244-G244)^2*F244)*ERFC((1/E244-G244)*F244^0.5))/2/G244),1)","v":0.15194745376461516}]
["PCB 209",8.18,7.7294599999999987,6.8027097371149869,1.9571486521810164,4.9279696131824752E-3,0.49988014023742877,{"$f":"IFERROR(IF(E245>1,1-(EXP((1/E245^2-G245^2)*F245)*((COS(G245/E245*F245*2)*(1-erfzR(1/E245*F245^0.5,G245*F245^0.5))-SIN(G245/E245*F245*2)*(-erfzI(1/E245*F245^0.5,G245*F245^0.5)))+(COS(G245/E245*F245*2)*(-erfzI(1/E245*F245^0.5,G245*F245^0.5))+SIN(G245/E245*F245*2)*(1-erfzR(1/E245*F245^0.5,G245*F245^0.5)))/E245/G245)),1-((1/E245+G245)*EXP((1/E245+G245)^2*F245)*ERFC((1/E245+G245)*F245^0.5)-(1/E245-G245)*EXP((1/E245-G245)^2*F245)*ERFC((1/E245-G245)*F245^0.5))/2/G245),1)","v":7.8326622861704109E-2}]

{"sheet":"Dioxins in PDMS","index":2,"n_rows":99,"n_cols":26,"rows_kept":99,"cut":false,"hidden":false,"merged":[]}
["Dioxins/Furans PRC CALIBRATION MODEL FOR PDMS SAMPLER"]
["Shen, X., & Reible, D. (2019). An analytical model for the fate and transport of performance reference compounds and target compounds around cylindrical passive samplers. Chemosphere."]
["Version 1.7"]
["2021-08-05",null,null,null,null,null,"Brief techical note"]
[null,null,null,null,null,null,"1. The 'Fss' values refer to the fractional approach to steady state, which is the 1-C/C0 for PRCs and C/Ceq for target compounds"]
["Parameters","Symbol","Value","Unit",null,null,"2. The 'Kpw' values refer to the PDMS-water partition coefficients, and can be estimated from octanol-water coefficients Kow using the correlations "]
["Inner radius","Li",2.4850000000000001E-2,"cm",null,null,null,"Log Kpw = 0.947 * Log Kow-0.017",null,"(Ghosh et al., 2014)"]
["Outer radius","Lo",2.835E-2,"cm",null,null,"3. The fitting process is to find parameters for the following correlation between sediment retardation factor R and Kow at given effective diffusivities D"]
["Sampling time","t",14,"days",null,null,null,"Log R = α * Log Kow + β"]
[null,null,null,null,null,null,"4. The fitted parameters (Row 28) is automatically derived by maximizing r2 from simulated results at different Ds  "]
["Number of PRCs",4,null,null,null,null,"5. The ‘Nonlinear’ in 'Option' is set to minimize the difference in Fss from calibrated to measurements, 'Linearized' is to minimuze the calibrated R values "]
["PRC #",{"$f":"PRCNumber(1,$B$11)","v":1},{"$f":"PRCNumber(2,$B$11)","v":2},{"$f":"PRCNumber(3,$B$11)","v":3},{"$f":"PRCNumber(4,$B$11)","v":4},{"$f":"PRCNumber(5,$B$11)","v":""},"6. The alpha value of the above correlation could be fixed to a given constant  ",null,null,null,{"$f":"PRCNumber(13,$B$11)","v":""},{"$f":"PRCNumber(14,$B$11)","v":""},{"$f":"PRCNumber(15,$B$11)","v":""},{"$f":"PRCNumber(16,$B$11)","v":""},{"$f":"PRCNumber(14,$B$11)","v":""},{"$f":"PRCNumber(15,$B$11)","v":""},{"$f":"PRCNumber(16,$B$11)","v":""},{"$f":"PRCNumber(17,$B$11)","v":""},{"$f":"PRCNumber(18,$B$11)","v":""},{"$f":"PRCNumber(19,$B$11)","v":""},{"$f":"PRCNumber(20,$B$11)","v":""},{"$f":"PRCNumber(21,$B$11)","v":""},{"$f":"PRCNumber(22,$B$11)","v":""},{"$f":"PRCNumber(23,$B$11)","v":""},{"$f":"PRCNumber(24,$B$11)","v":""},{"$f":"PRCNumber(25,$B$11)","v":""}]
["PRC name","C13-1234-TCDD","C13-123789-HxCDD","C13-2,7/2,8 DiCDD","C13-1234678 HpCDD"]
["Log Kow",6.53,7.92,5.19,8.64,null,"Procedure"]
["Log Kpw",{"$f":"B14*0.947-0.017","v":6.1669099999999997},{"$f":"C14*0.947-0.017","v":7.4832399999999994},4.8979299999999997,8.1650800000000014,null,"1. Update the properties of sampler and PRCs on this sheet in Green "]
["Measured PRC Fss",0.7,0.5,0.8,0.3,null,"2. Input a list of desired effective diffusivity (D) in column A starting row 33."]
[null,null,null,null,null,null,"3. Start the fitting by clicking on  \"Fit fss Data\""]
[null,null,null,null,null,null,"4. Check the fitted results (parameters in Row 28, results in the following figure), if it is not desired, change the list of D  "]
[null,null,null,null,null,null,"5. View model results in the following figure, the returned data are in cyl_fitted_plot"]
[]
[null,null,null,null,null,null,"Database of frequently used PRCs"]
[]
[null,null,null,null,null,null,"PRCs set 1"]
[null,null,null,null,null,null,"PRC name","C13-1234-TCDD","C13-123789-HxCDD","C13-2,7/2,8 DiCDD","C13-1234678 HpCDD"]
[null,null,null,null,null,null,"Log Kow",6.53,7.92,5.19,8.64]
[null,null,null,null,null,null,"Log Kpw",6.1669099999999997,7.4832399999999994,4.8979299999999997,8.1650800000000014]
["Results"]
["Cylindrical diffusion model","Log R = α * Log Kow + β"]
["D",3.7404343444773626E-6]
["α",1.3930258547325278]
["β",-2.0562105918468117]
["r2",0.99520560964674887]
[]
[]
["Model prediction"]
["Target Compound","Log Kow","Log Kpw","Log R","ξ","τ","ω","fss"]
["2-MCDD",4.58,{"$f":"B37*0.947-0.017","v":4.3202599999999993},{"$f":"B37*$B$30+$B$31","v":4.3238478228281663},{"$f":"10^C37*($C$8^2-$C$7^2)/10^D37/$C$8^2","v":0.22976598078975338},{"$f":"$B$29*$C$9*86400/10^D37/$C$8^2","v":0.26706062736142655},{"$f":"IF(E37>1,(1/E37-1/E37^2)^0.5,(1/E37^2-1/E37)^0.5)","v":3.8196680396858262},{"$f":"IFERROR(IF(E37>1,1-(EXP((1/E37^2-G37^2)*F37)*((COS(G37/E37*F37*2)*(1-erfzR(1/E37*F37^0.5,G37*F37^0.5))-SIN(G37/E37*F37*2)*(-erfzI(1/E37*F37^0.5,G37*F37^0.5)))+(COS(G37/E37*F37*2)*(-erfzI(1/E37*F37^0.5,G37*F37^0.5))+SIN(G37/E37*F37*2)*(1-erfzR(1/E37*F37^0.5,G37*F37^0.5)))/E37/G37)),1-((1/E37+G37)*EXP((1/E37+G37)^2*F37)*ERFC((1/E37+G37)*F37^0.5)-(1/E37-G37)*EXP((1/E37-G37)^2*F37)*ERFC((1/E37-G37)*F37^0.5))/2/G37),1)","v":0.91322275963364064}]
["2,3-DiCDD",5.23,{"$f":"B38*0.947-0.017","v":4.93581},5.2293146284043095,{"$f":"10^C38*($C$8^2-$C$7^2)/10^D38/$C$8^2","v":0.11786067439440906},3.3200380366292782E-2,{"$f":"IF(E38>1,(1/E38-1/E38^2)^0.5,(1/E38^2-1/E38)^0.5)","v":7.9689237228644183},{"$f":"IFERROR(IF(E38>1,1-(EXP((1/E38^2-G38^2)*F38)*((COS(G38/E38*F38*2)*(1-erfzR(1/E38*F38^0.5,G38*F38^0.5))-SIN(G38/E38*F38*2)*(-erfzI(1/E38*F38^0.5,G38*F38^0.5)))+(COS(G38/E38*F38*2)*(-erfzI(1/E38*F38^0.5,G38*F38^0.5))+SIN(G38/E38*F38*2)*(1-erfzR(1/E38*F38^0.5,G38*F38^0.5)))/E38/G38)),1-((1/E38+G38)*EXP((1/E38+G38)^2*F38)*ERFC((1/E38+G38)*F38^0.5)-(1/E38-G38)*EXP((1/E38-G38)^2*F38)*ERFC((1/E38-G38)*F38^0.5))/2/G38),1)","v":0.84428577415824968}]
["2,7/2,8-DiCDD",5.19,4.8979299999999997,5.1735935942150082,0.12280327696711385,3.7745405337116837E-2,7.626733028890671,{"$f":"IFERROR(IF(E39>1,1-(EXP((1/E39^2-G39^2)*F39)*((COS(G39/E39*F39*2)*(1-erfzR(1/E39*F39^0.5,G39*F39^0.5))-SIN(G39/E39*F39*2)*(-erfzI(1/E39*F39^0.5,G39*F39^0.5)))+(COS(G39/E39*F39*2)*(-erfzI(1/E39*F39^0.5,G39*F39^0.5))+SIN(G39/E39*F39*2)*(1-erfzR(1/E39*F39^0.5,G39*F39^0.5)))/E39/G39)),1-((1/E39+G39)*EXP((1/E39+G39)^2*F39)*ERFC((1/E39+G39)*F39^0.5)-(1/E39-G39)*EXP((1/E39-G39)^2*F39)*ERFC((1/E39-G39)*F39^0.5))/2/G39),1)","v":0.84879667588710928}]
["2,3,7-TrCDD",5.84,5.5134799999999995,6.0790603997911514,6.2993124532354089E-2,4.6924244380516997E-3,15.366615989116641,{"$f":"IFERROR(IF(E40>1,1-(EXP((1/E40^2-G40^2)*F40)*((COS(G40/E40*F40*2)*(1-erfzR(1/E40*F40^0.5,G40*F40^0.5))-SIN(G40/E40*F40*2)*(-erfzI(1/E40*F40^0.5,G40*F40^0.5)))+(COS(G40/E40*F40*2)*(-erfzI(1/E40*F40^0.5,G40*F40^0.5))+SIN(G40/E40*F40*2)*(1-erfzR(1/E40*F40^0.5,G40*F40^0.5)))/E40/G40)),1-((1/E40+G40)*EXP((1/E40+G40)^2*F40)*ERFC((1/E40+G40)*F40^0.5)-(1/E40-G40)*EXP((1/E40-G40)^2*F40)*ERFC((1/E40-G40)*F40^0.5))/2/G40),1)","v":0.77069955251404298}]
["2378-TCDF",6.46,6.1006199999999993,6.9427364297253185,3.3323999590582333E-2,6.4227535520246584E-4,29.504166335703331,{"$f":"IFERROR(IF(E41>1,1-(EXP((1/E41^2-G41^2)*F41)*((COS(G41/E41*F41*2)*(1-erfzR(1/E41*F41^0.5,G41*F41^0.5))-SIN(G41/E41*F41*2)*(-erfzI(1/E41*F41^0.5,G41*F41^0.5)))+(COS(G41/E41*F41*2)*(-erfzI(1/E41*F41^0.5,G41*F41^0.5))+SIN(G41/E41*F41*2)*(1-erfzR(1/E41*F41^0.5,G41*F41^0.5)))/E41/G41)),1-((1/E41+G41)*EXP((1/E41+G41)^2*F41)*ERFC((1/E41+G41)*F41^0.5)-(1/E41-G41)*EXP((1/E41-G41)^2*F41)*ERFC((1/E41-G41)*F41^0.5))/2/G41),1)","v":0.68544385510395567}]
["2378-TCDD",6.49,6.1290299999999993,6.9845272053672947,3.2312930374091886E-2,5.8335171950511821E-4,30.443257714343606,{"$f":"IFERROR(IF(E42>1,1-(EXP((1/E42^2-G42^2)*F42)*((COS(G42/E42*F42*2)*(1-erfzR(1/E42*F42^0.5,G42*F42^0.5))-SIN(G42/E42*F42*2)*(-erfzI(1/E42*F42^0.5,G42*F42^0.5)))+(COS(G42/E42*F42*2)*(-erfzI(1/E42*F42^0.5,G42*F42^0.5))+SIN(G42/E42*F42*2)*(1-erfzR(1/E42*F42^0.5,G42*F42^0.5)))/E42/G42)),1-((1/E42+G42)*EXP((1/E42+G42)^2*F42)*ERFC((1/E42+G42)*F42^0.5)-(1/E42-G42)*EXP((1/E42-G42)^2*F42)*ERFC((1/E42-G42)*F42^0.5))/2/G42),1)","v":0.68104967609547551}]
["12378-PeCDF",7.15,6.7540499999999994,7.9039242694907621,1.6405870559634418E-2,7.0231738378370069E-5,60.451722948727806,{"$f":"IFERROR(IF(E43>1,1-(EXP((1/E43^2-G43^2)*F43)*((COS(G43/E43*F43*2)*(1-erfzR(1/E43*F43^0.5,G43*F43^0.5))-SIN(G43/E43*F43*2)*(-erfzI(1/E43*F43^0.5,G43*F43^0.5)))+(COS(G43/E43*F43*2)*(-erfzI(1/E43*F43^0.5,G43*F43^0.5))+SIN(G43/E43*F43*2)*(1-erfzR(1/E43*F43^0.5,G43*F43^0.5)))/E43/G43)),1-((1/E43+G43)*EXP((1/E43+G43)^2*F43)*ERFC((1/E43+G43)*F43^0.5)-(1/E43-G43)*EXP((1/E43-G43)^2*F43)*ERFC((1/E43-G43)*F43^0.5))/2/G43),1)","v":0.57950936817934906}]
["23478-PeCDF",7.14,6.7445799999999991,7.8899940109434361,1.6575229076383362E-2,7.2520982094039329E-5,59.828901972686502,{"$f":"IFERROR(IF(E44>1,1-(EXP((1/E44^2-G44^2)*F44)*((COS(G44/E44*F44*2)*(1-erfzR(1/E44*F44^0.5,G44*F44^0.5))-SIN(G44/E44*F44*2)*(-erfzI(1/E44*F44^0.5,G44*F44^0.5)))+(COS(G44/E44*F44*2)*(-erfzI(1/E44*F44^0.5,G44*F44^0.5))+SIN(G44/E44*F44*2)*(1-erfzR(1/E44*F44^0.5,G44*F44^0.5)))/E44/G44)),1-((1/E44+G44)*EXP((1/E44+G44)^2*F44)*ERFC((1/E44+G44)*F44^0.5)-(1/E44-G44)*EXP((1/E44-G44)^2*F44)*ERFC((1/E44-G44)*F44^0.5))/2/G44),1)","v":0.58110022152106899}]
["12378-PeCDD",7.2,6.8013999999999992,7.9735755622273885,1.5584683538903101E-2,5.9824919855708885E-5,63.663600005165961,{"$f":"IFERROR(IF(E45>1,1-(EXP((1/E45^2-G45^2)*F45)*((COS(G45/E45*F45*2)*(1-erfzR(1/E45*F45^0.5,G45*F45^0.5))-SIN(G45/E45*F45*2)*(-erfzI(1/E45*F45^0.5,G45*F45^0.5)))+(COS(G45/E45*F45*2)*(-erfzI(1/E45*F45^0.5,G45*F45^0.5))+SIN(G45/E45*F45*2)*(1-erfzR(1/E45*F45^0.5,G45*F45^0.5)))/E45/G45)),1-((1/E45+G45)*EXP((1/E45+G45)^2*F45)*ERFC((1/E45+G45)*F45^0.5)-(1/E45-G45)*EXP((1/E45-G45)^2*F45)*ERFC((1/E45-G45)*F45^0.5))/2/G45),1)","v":0.5715405794158811}]
["123478-HxCDF",7.87,7.4358899999999997,8.9069028848981819,7.8317833532777128E-3,6.9751700970383401E-6,127.18385661566568,{"$f":"IFERROR(IF(E46>1,1-(EXP((1/E46^2-G46^2)*F46)*((COS(G46/E46*F46*2)*(1-erfzR(1/E46*F46^0.5,G46*F46^0.5))-SIN(G46/E46*F46*2)*(-erfzI(1/E46*F46^0.5,G46*F46^0.5)))+(COS(G46/E46*F46*2)*(-erfzI(1/E46*F46^0.5,G46*F46^0.5))+SIN(G46/E46*F46*2)*(1-erfzR(1/E46*F46^0.5,G46*F46^0.5)))/E46/G46)),1-((1/E46+G46)*EXP((1/E46+G46)^2*F46)*ERFC((1/E46+G46)*F46^0.5)-(1/E46-G46)*EXP((1/E46-G46)^2*F46)*ERFC((1/E46-G46)*F46^0.5))/2/G46),1)","v":0.46425662169110526}]
["123678-HxCDF",7.83,7.3980099999999993,8.8511818507088815,8.1602168426470455E-3,7.9300483820766284E-6,122.04473888437593,{"$f":"IFERROR(IF(E47>1,1-(EXP((1/E47^2-G47^2)*F47)*((COS(G47/E47*F47*2)*(1-erfzR(1/E47*F47^0.5,G47*F47^0.5))-SIN(G47/E47*F47*2)*(-erfzI(1/E47*F47^0.5,G47*F47^0.5)))+(COS(G47/E47*F47*2)*(-erfzI(1/E47*F47^0.5,G47*F47^0.5))+SIN(G47/E47*F47*2)*(1-erfzR(1/E47*F47^0.5,G47*F47^0.5)))/E47/G47)),1-((1/E47+G47)*EXP((1/E47+G47)^2*F47)*ERFC((1/E47+G47)*F47^0.5)-(1/E47-G47)*EXP((1/E47-G47)^2*F47)*ERFC((1/E47-G47)*F47^0.5))/2/G47),1)","v":0.47059751808284811}]
["234678-HxCDF",7.83,7.3980099999999993,8.8511818507088815,8.1602168426470455E-3,7.9300483820766284E-6,122.04473888437593,{"$f":"IFERROR(IF(E48>1,1-(EXP((1/E48^2-G48^2)*F48)*((COS(G48/E48*F48*2)*(1-erfzR(1/E48*F48^0.5,G48*F48^0.5))-SIN(G48/E48*F48*2)*(-erfzI(1/E48*F48^0.5,G48*F48^0.5)))+(COS(G48/E48*F48*2)*(-erfzI(1/E48*F48^0.5,G48*F48^0.5))+SIN(G48/E48*F48*2)*(1-erfzR(1/E48*F48^0.5,G48*F48^0.5)))/E48/G48)),1-((1/E48+G48)*EXP((1/E48+G48)^2*F48)*ERFC((1/E48+G48)*F48^0.5)-(1/E48-G48)*EXP((1/E48-G48)^2*F48)*ERFC((1/E48-G48)*F48^0.5))/2/G48),1)","v":0.47059751808284811}]
["123478-HxCDD",7.95,7.5116499999999995,9.0183449532767845,7.2140408450027055E-3,5.3965068720045438E-6,138.11766139340219,{"$f":"IFERROR(IF(E49>1,1-(EXP((1/E49^2-G49^2)*F49)*((COS(G49/E49*F49*2)*(1-erfzR(1/E49*F49^0.5,G49*F49^0.5))-SIN(G49/E49*F49*2)*(-erfzI(1/E49*F49^0.5,G49*F49^0.5)))+(COS(G49/E49*F49*2)*(-erfzI(1/E49*F49^0.5,G49*F49^0.5))+SIN(G49/E49*F49*2)*(1-erfzR(1/E49*F49^0.5,G49*F49^0.5)))/E49/G49)),1-((1/E49+G49)*EXP((1/E49+G49)^2*F49)*ERFC((1/E49+G49)*F49^0.5)-(1/E49-G49)*EXP((1/E49-G49)^2*F49)*ERFC((1/E49-G49)*F49^0.5))/2/G49),1)","v":0.45163648442780069}]
["123678-HxCDD",7.89,7.4548299999999994,8.9347634019928321,7.6725574358837353E-3,6.5417551612090351E-6,129.83367576246695,{"$f":"IFERROR(IF(E50>1,1-(EXP((1/E50^2-G50^2)*F50)*((COS(G50/E50*F50*2)*(1-erfzR(1/E50*F50^0.5,G50*F50^0.5))-SIN(G50/E50*F50*2)*(-erfzI(1/E50*F50^0.5,G50*F50^0.5)))+(COS(G50/E50*F50*2)*(-erfzI(1/E50*F50^0.5,G50*F50^0.5))+SIN(G50/E50*F50*2)*(1-erfzR(1/E50*F50^0.5,G50*F50^0.5)))/E50/G50)),1-((1/E50+G50)*EXP((1/E50+G50)^2*F50)*ERFC((1/E50+G50)*F50^0.5)-(1/E50-G50)*EXP((1/E50-G50)^2*F50)*ERFC((1/E50-G50)*F50^0.5))/2/G50),1)","v":0.46109352390824465}]
["123789-HxCDD",7.92,7.4832399999999994,8.9765541776348083,7.4397676528299393E-3,5.94160135674178E-6,133.91186634295883,{"$f":"IFERROR(IF(E51>1,1-(EXP((1/E51^2-G51^2)*F51)*((COS(G51/E51*F51*2)*(1-erfzR(1/E51*F51^0.5,G51*F51^0.5))-SIN(G51/E51*F51*2)*(-erfzI(1/E51*F51^0.5,G51*F51^0.5)))+(COS(G51/E51*F51*2)*(-erfzI(1/E51*F51^0.5,G51*F51^0.5))+SIN(G51/E51*F51*2)*(1-erfzR(1/E51*F51^0.5,G51*F51^0.5)))/E51/G51)),1-((1/E51+G51)*EXP((1/E51+G51)^2*F51)*ERFC((1/E51+G51)*F51^0.5)-(1/E51-G51)*EXP((1/E51-G51)^2*F51)*ERFC((1/E51-G51)*F51^0.5))/2/G51),1)","v":0.45635873569909868}]
["123789-HxCDF",7.87,7.4358899999999997,8.9069028848981819,7.8317833532777128E-3,6.9751700970383401E-6,127.18385661566568,{"$f":"IFERROR(IF(E52>1,1-(EXP((1/E52^2-G52^2)*F52)*((COS(G52/E52*F52*2)*(1-erfzR(1/E52*F52^0.5,G52*F52^0.5))-SIN(G52/E52*F52*2)*(-erfzI(1/E52*F52^0.5,G52*F52^0.5)))+(COS(G52/E52*F52*2)*(-erfzI(1/E52*F52^0.5,G52*F52^0.5))+SIN(G52/E52*F52*2)*(1-erfzR(1/E52*F52^0.5,G52*F52^0.5)))/E52/G52)),1-((1/E52+G52)*EXP((1/E52+G52)^2*F52)*ERFC((1/E52+G52)*F52^0.5)-(1/E52-G52)*EXP((1/E52-G52)^2*F52)*ERFC((1/E52-G52)*F52^0.5))/2/G52),1)","v":0.46425662169110526}]
["1234678-HpCDF",8.5500000000000007,8.0798500000000004,9.8541604661163014,3.8954988822491369E-3,{"$f":"$B$29*$C$9*86400/10^D53/$C$8^2","v":7.8758461088816991E-7},{"$f":"IF(E53>1,(1/E53-1/E53^2)^0.5,(1/E53^2-1/E53)^0.5)","v":256.20604193706117},{"$f":"IFERROR(IF(E53>1,1-(EXP((1/E53^2-G53^2)*F53)*((COS(G53/E53*F53*2)*(1-erfzR(1/E53*F53^0.5,G53*F53^0.5))-SIN(G53/E53*F53*2)*(-erfzI(1/E53*F53^0.5,G53*F53^0.5)))+(COS(G53/E53*F53*2)*(-erfzI(1/E53*F53^0.5,G53*F53^0.5))+SIN(G53/E53*F53*2)*(1-erfzR(1/E53*F53^0.5,G53*F53^0.5)))/E53/G53)),1-((1/E53+G53)*EXP((1/E53+G53)^2*F53)*ERFC((1/E53+G53)*F53^0.5)-(1/E53-G53)*EXP((1/E53-G53)^2*F53)*ERFC((1/E53-G53)*F53^0.5))/2/G53),1)","v":0.36094531714491662}]
["1234678-HpCDD",8.64,8.1650800000000014,9.97953279304223,3.5515730935393912E-3,5.9009902173846071E-7,281.06492746947038,{"$f":"IFERROR(IF(E54>1,1-(EXP((1/E54^2-G54^2)*F54)*((COS(G54/E54*F54*2)*(1-erfzR(1/E54*F54^0.5,G54*F54^0.5))-SIN(G54/E54*F54*2)*(-erfzI(1/E54*F54^0.5,G54*F54^0.5)))+(COS(G54/E54*F54*2)*(-erfzI(1/E54*F54^0.5,G54*F54^0.5))+SIN(G54/E54*F54*2)*(1-erfzR(1/E54*F54^0.5,G54*F54^0.5)))/E54/G54)),1-((1/E54+G54)*EXP((1/E54+G54)^2*F54)*ERFC((1/E54+G54)*F54^0.5)-(1/E54-G54)*EXP((1/E54-G54)^2*F54)*ERFC((1/E54-G54)*F54^0.5))/2/G54),1)","v":0.34813530804000292}]
["1234789-HpCDF",8.56,8.0893200000000007,9.8680907246636274,3.8556963606879054E-3,7.6272321120806342E-7,258.85603962629176,{"$f":"IFERROR(IF(E55>1,1-(EXP((1/E55^2-G55^2)*F55)*((COS(G55/E55*F55*2)*(1-erfzR(1/E55*F55^0.5,G55*F55^0.5))-SIN(G55/E55*F55*2)*(-erfzI(1/E55*F55^0.5,G55*F55^0.5)))+(COS(G55/E55*F55*2)*(-erfzI(1/E55*F55^0.5,G55*F55^0.5))+SIN(G55/E55*F55*2)*(1-erfzR(1/E55*F55^0.5,G55*F55^0.5)))/E55/G55)),1-((1/E55+G55)*EXP((1/E55+G55)^2*F55)*ERFC((1/E55+G55)*F55^0.5)-(1/E55-G55)*EXP((1/E55-G55)^2*F55)*ERFC((1/E55-G55)*F55^0.5))/2/G55),1)","v":0.35951007212040165}]
["OCDD",9.35,8.8374500000000005,10.968581149902324,1.7129409832935944E-3,6.0516881157707612E-8,583.29106032708285,{"$f":"IFERROR(IF(E56>1,1-(EXP((1/E56^2-G56^2)*F56)*((COS(G56/E56*F56*2)*(1-erfzR(1/E56*F56^0.5,G56*F56^0.5))-SIN(G56/E56*F56*2)*(-erfzI(1/E56*F56^0.5,G56*F56^0.5)))+(COS(G56/E56*F56*2)*(-erfzI(1/E56*F56^0.5,G56*F56^0.5))+SIN(G56/E56*F56*2)*(1-erfzR(1/E56*F56^0.5,G56*F56^0.5)))/E56/G56)),1-((1/E56+G56)*EXP((1/E56+G56)^2*F56)*ERFC((1/E56+G56)*F56^0.5)-(1/E56-G56)*EXP((1/E56-G56)^2*F56)*ERFC((1/E56-G56)*F56^0.5))/2/G56),1)","v":0.25655464109311665}]
["OCDF",9.27,8.7616899999999998,10.857139081523721,1.8596211147596988E-3,7.8220143109068129E-8,537.24371531212887,{"$f":"IFERROR(IF(E57>1,1-(EXP((1/E57^2-G57^2)*F57)*((COS(G57/E57*F57*2)*(1-erfzR(1/E57*F57^0.5,G57*F57^0.5))-SIN(G57/E57*F57*2)*(-erfzI(1/E57*F57^0.5,G57*F57^0.5)))+(COS(G57/E57*F57*2)*(-erfzI(1/E57*F57^0.5,G57*F57^0.5))+SIN(G57/E57*F57*2)*(1-erfzR(1/E57*F57^0.5,G57*F57^0.5)))/E57/G57)),1-((1/E57+G57)*EXP((1/E57+G57)^2*F57)*ERFC((1/E57+G57)*F57^0.5)-(1/E57-G57)*EXP((1/E57-G57)^2*F57)*ERFC((1/E57-G57)*F57^0.5))/2/G57),1)","v":0.26597183746526853}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"A96*10^0.02","v":0},1,14.883034744223696,0.98710318949221576]
[0,1,-81.52211188194967,0.98659157472021164]
[0,1,17.534850078544217,0.98538337426517375]

{"sheet":"PAHs in PE","index":3,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["PAH CALIBRATION MODEL FOR PE SAMPLER"]
["Shen, X., & Reible, D. (2019). An analytical model for the fate and transport of performance reference compounds and target compounds around cylindrical passive samplers. Chemosphere."]
["Version 1.7"]
["2021-08-05",null,null,null,null,null,"Brief techical note"]
[null,null,null,null,null,null,"1. The 'Fss' values refer to the fractional approach to steady state, which is the 1-C/C0 for PRCs and C/Ceq for target compounds"]
["Parameters","Symbol","Value","Unit",null,null,"2. The 'Kpw' values refer to the polymer-water partition coefficients, and can be estimated from octanol-water coefficients Kow using the correlations "]
["Thickness","L",2.5400000000000002E-3,"cm",null,null,null,"Log Kpw = 1.22 * Log Kow - 1.36",null,"(Ghosh et al., 2014)"]
["Sampling time","t",14,"days",null,null,"3. The fitting process is to find parameters for the following correlation between Kow and the product of retardation factor R and effective diffusivities D   "]
[null,null,null,null,null,null,null,"Log RD = a * Log Kow + b"]
[null,null,null,null,null,null,"4. The ‘Nonlinear’ in 'Option' is set to minimize the difference in Fss from calibrated to measurements, 'Linearized' is to minimuze the calibrated R values "]
["Number of PRCs",4,null,null,null,null,"5. The a value of the above correlation could be fixed to a given constant  ",null,null,null,{"$f":"PRCNumber(13,$B$11)","v":""}]
["PRC #",{"$f":"PRCNumber(1,$B$11)","v":1},{"$f":"PRCNumber(2,$B$11)","v":2},{"$f":"PRCNumber(3,$B$11)","v":3},{"$f":"PRCNumber(4,$B$11)","v":4}]
["PRC name","C13-phenanthrene","C13-fluoranthene","C13-chrysene","C13-indeno[1,2,3-CD]pyrene",null,"Procedure"]
["Log Kow",4.74,5.29,5.9,7.09,null,"1. Update the properties of sampler and PRCs on this sheet in Green "]
["Log Kpw",4.4227999999999996,5.0937999999999999,5.8380000000000001,7.2897999999999987,null,"2. Start the fitting by clicking on  \"Fit fss Data\""]
["Measured PRC Fss",0.8,0.7,0.5,0.3,null,"3. Check the fitted results (parameters in Row 25 results in the following figure)"]
[null,null,null,null,null,null,"4. View model results in the following figure, the returned data are in rec_fitted_plot"]
[]
[null,null,null,null,null,null,"Database of frequently used PRCs"]
[]
[null,null,null,null,null,null,"PRCs set 1"]
[null,null,null,null,null,null,"PRC name","C13-phenanthrene","C13-fluoranthene","C13-chrysene","C13-indeno[1,2,3-CD]pyrene"]
[null,null,null,null,null,null,"Log Kow",4.74,5.29,5.9,7.09]
[null,null,null,null,null,null,"Log Kpw",{"$f":"H23*1.22-1.36","v":4.4227999999999996},{"$f":"I23*1.22-1.36","v":5.0937999999999999},5.8380000000000001,7.2897999999999987]
[]
[]
["Results"]
["Cylindrical diffusion model","Log RD = a * Log Kow + b"]
[]
["a",1.7009216847817143]
["b",-9.7048698813076175]
["r2",0.99583628545041891]
[]
[]
["Model prediction"]
["Target Compound","Log Kow","Log Kpw","Log RD","fss"]
["naphthalene ",3.41,{"$f":"B37*1.22 - 1.36","v":2.8001999999999994},{"$f":"B37*$B$30+$B$31","v":-3.9047269362019712},{"$f":"IF((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2<700, 1-EXP((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2)*ERFC((10^D37) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C37)), 1-1/((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2*3.14)^0.5)","v":0.92690776041889589}]
["acenaphthylene ",4,{"$f":"B38*1.22 - 1.36","v":3.5199999999999996},{"$f":"B38*$B$30+$B$31","v":-2.9011831421807601},{"$f":"IF((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2<700, 1-EXP((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2)*ERFC((10^D38) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C38)), 1-1/((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2*3.14)^0.5)","v":0.88089084317413247}]
["acenaphthene ",4.0599999999999996,3.5931999999999995,-2.799127841093858,0.87493270298011339]
["fluorene ",4.2,3.7639999999999993,-2.5609988052244166,0.85996683844320687]
["phenanthrene ",4.74,4.4227999999999996,-1.6425010954422916,0.78682820507555995]
["anthracene ",4.6900000000000004,4.3617999999999997,-1.7275471796813768,0.7946898906663763]
["fluoranthene ",5.29,5.0937999999999999,-0.70699416881234889,0.68577241765035635]
["pyrene ",5.25,5.0449999999999999,-0.77503103620361635,0.69396539875483665]
["benz(a)anthracene",5.85,5.7769999999999992,0.24552197466541159,0.56122119586761787]
["chrysene ",5.9,5.8380000000000001,0.33056805890449859,0.54951877645889713]
["benzo(b)fluoranthene ",6.58,6.6675999999999993,1.4871948045560632,0.39232322806435682]
["benzo(k)fluoranthene ",6.5,6.5699999999999994,1.3511210697735265,0.41009400439519461]
["benzo(a)pyrene ",6.54,6.6187999999999994,1.419157937164794,0.40116882952677313]
["indeno(123-cd)pyrene ",7.09,7.2897999999999987,2.3546648637947367,0.28831975415097377]
["dibenzo(ah)anthracene ",7.39,7.6557999999999984,2.8649413692292516,0.23623323731107604]
["benzo(ghi)perylene ",7.04,7.2287999999999988,2.2696187795556515,0.29769720392236598]

{"sheet":"PCBs in PE","index":4,"n_rows":245,"n_cols":17,"rows_kept":245,"cut":false,"hidden":false,"merged":[]}
["PCB CALIBRATION MODEL FOR PE SAMPLER"]
["Shen, X., & Reible, D. (2019). An analytical model for the fate and transport of performance reference compounds and target compounds around cylindrical passive samplers. Chemosphere."]
["Version 1.7"]
["2021-08-05",null,null,null,null,null,null,null,null,"Brief techical note"]
[null,null,null,null,null,null,null,null,null,"1. The 'Fss' values refer to the fractional approach to steady state, which is the 1-C/C0 for PRCs and C/Ceq for target compounds"]
["Parameters","Symbol","Value","Unit",null,null,null,null,null,"2. The 'Kpw' values refer to the polymer-water partition coefficients, and can be estimated from octanol-water coefficients Kow using the correlations "]
["Thickness","L",3.284E-3,"cm",null,null,null,null,null,null,"Log Kpw = 1.18 * Log Kow - 1.26",null,"(Ghosh et al., 2014)"]
["Sampling time","t",28,"days",null,null,null,null,null,"3. The fitting process is to find parameters for the following correlation between Kow and the product of retardation factor R and effective diffusivities D   "]
[null,null,null,null,null,null,null,null,null,null,"Log RD = a * Log Kow + b"]
[null,null,null,null,null,null,null,null,null,"4. The ‘Nonlinear’ in 'Option' is set to minimize the difference in Fss from calibrated to measurements, 'Linearized' is to minimuze the calibrated R values "]
["Number of PRCs",7,null,null,null,null,null,null,null,"5. The a value of the above correlation could be fixed to a given constant  ",null,null,null,{"$f":"PRCNumber(13,$B$11)","v":""}]
["PRC #",{"$f":"PRCNumber(1,$B$11)","v":1},{"$f":"PRCNumber(2,$B$11)","v":2},{"$f":"PRCNumber(3,$B$11)","v":3},{"$f":"PRCNumber(4,$B$11)","v":4},{"$f":"PRCNumber(5,$B$11)","v":5},{"$f":"PRCNumber(6,$B$11)","v":6},{"$f":"PRCNumber(7,$B$11)","v":7},null,null,null,null,null,null,{"$f":"PRCNumber(16,$B$11)","v":""},{"$f":"PRCNumber(14,$B$11)","v":""},{"$f":"PRCNumber(15,$B$11)","v":""}]
["PRC name","13C-PCB28","13C-PCB47","13C-PCB70","13C-PCB80","13C-PCB111","13C-PCB141","13C-PCB182",null,"Procedure"]
["Log Kow",5.67,5.85,6.2,6.48,6.76,6.82,7.2,null,"1. Update the properties of sampler and PRCs on this sheet in Green "]
["Log Kpw",{"$f":"1.18*B14-1.26","v":5.4306000000000001},{"$f":"1.18*C14-1.26","v":5.6429999999999998},6.056,6.3864000000000001,6.7167999999999992,6.7875999999999994,7.2360000000000007,null,"2. Start the fitting by clicking on  \"Fit fss Data\""]
["Measured PRC Fss",0.9,0.8,0.7,0.6,0.5,0.4,0.3,null,"3. Check the fitted results (parameters in Row 25 results in the following figure)"]
[null,null,null,null,null,null,null,null,null,"4. View model results in the following figure, the returned data are in rec_fitted_plot"]
[]
[null,null,null,null,null,null,null,null,null,"Database of frequently used PRCs"]
[null,null,null,null,null,null,null,null,null,"High sensitivity group"]
[null,null,null,null,null,null,null,null,null,"PRC name","13C-PCB28","13C-PCB47","13C-PCB70","13C-PCB80","13C-PCB111","13C-PCB141","13C-PCB182"]
[null,null,null,null,null,null,null,null,null,"Log Kow",5.67,5.85,6.2,6.48,6.76,6.82,7.2]
[null,null,null,null,null,null,null,null,null,"Log Kpw",{"$f":"1.18*K22-1.26","v":5.4306000000000001},{"$f":"1.18*L22-1.26","v":5.6429999999999998},6.056,6.3864000000000001,6.7167999999999992,6.7875999999999994,7.2360000000000007]
[]
[null,null,null,null,null,null,null,null,null,"Low sensitivity group"]
[null,null,null,null,null,null,null,null,null,"PRC name","13C-PCB 37 ","13C-PCB 47 ","13C-PCB 54 ","13C-PCB 111","13C-PCB 138 ","13C-PCB 178 "]
["Results",null,null,null,null,null,null,null,null,"Log Kow",5.83,5.85,5.21,6.76,6.83,7.14]
["Rectangularl diffusion model","Log RD = a * Log Kow + b",null,null,null,null,null,null,null,"Log Kpw",{"$f":"1.18*K27-1.26","v":5.6193999999999997},{"$f":"1.18*L27-1.26","v":5.6429999999999998},4.8877999999999995,6.7167999999999992,6.7994000000000003,7.1651999999999987]
[]
["a",0.81104731566284705]
["b",-3.7381585386114917]
["r2",0.88043030072242323]
[]
[]
["Model prediction"]
["Target Compound","Log Kow","Log Kpw","Log RD","fss"]
["PCB 1",4.46,{"$f":"1.18*B37-1.26","v":4.0027999999999997},{"$f":"B37*$B$30+$B$31","v":-0.12088751075519388},{"$f":"IF((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2<700, 1-EXP((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2)*ERFC((10^D37) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C37)), 1-1/((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2*3.14)^0.5)","v":0.98621692266657157}]
["PCB 2",4.6900000000000004,{"$f":"1.18*B38-1.26","v":4.2742000000000004},{"$f":"B38*$B$30+$B$31","v":6.5653371847261166E-2},{"$f":"IF((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2<700, 1-EXP((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2)*ERFC((10^D38) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C38)), 1-1/((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2*3.14)^0.5)","v":0.97922812255486735}]
["PCB 3",4.6900000000000004,4.2742000000000004,6.5653371847261166E-2,0.97922812255486735]
["PCB 4",4.6500000000000004,4.2270000000000003,3.3211479220747187E-2,0.98065820847754226]
["PCB 5",4.97,4.6045999999999996,0.29274662023285813,0.96584737968866863]
["PCB 6",5.0599999999999996,4.7107999999999999,0.36574087864251403,0.95992921258457131]
["PCB 7",5.07,4.7225999999999999,0.37385135179914286,0.95921192839482539]
["PCB 8",5.07,4.7225999999999999,0.37385135179914286,0.95921192839482539]
["PCB 9",5.0599999999999996,4.7107999999999999,0.36574087864251403,0.95992921258457131]
["PCB 10",4.84,4.4512,0.18731046919668781,0.97289582346621195]
["PCB 11",5.28,4.9704000000000006,0.54417128808834114,0.94085384328672506]
["PCB 12",5.22,4.8995999999999995,0.49550844914856995,0.94680001451607954]
["PCB 13",5.29,4.9821999999999997,0.55228176124496908,0.93980144518681397]
["PCB 14",5.28,4.9704000000000006,0.54417128808834114,0.94085384328672506]
["PCB 15",5.3,4.9939999999999998,0.56039223440159791,0.93873074604211881]
["PCB 16",5.16,4.8288000000000002,0.44684561020879876,0.9521578355540119]
["PCB 17",5.25,4.9349999999999996,0.51983986861845555,0.94390413436098264]
["PCB 18",5.24,4.9232000000000005,0.51172939546182672,0.94488621318363286]
["PCB 19",5.0199999999999996,4.6635999999999997,0.3332989860160005,0.96267554367120689]
["PCB 20",5.57,5.3125999999999998,0.7793750096305665,0.90174288222745003]
["PCB 21",5.51,5.2417999999999996,0.7307121706907953,0.91146412862095616]
["PCB 22",5.58,5.3243999999999998,0.78748548278719444,0.90002764399892488]
["PCB 23",5.57,5.3125999999999998,0.7793750096305665,0.90174288222745003]
["PCB 24",5.51,5.2417999999999996,0.7307121706907953,0.91146412862095616]
["PCB 25",5.58,5.3243999999999998,0.78748548278719444,0.90002764399892488]
["PCB 26",5.57,5.3125999999999998,0.7793750096305665,0.90174288222745003]
["PCB 27",5.35,5.052999999999999,0.60094460018473939,0.93309225894183534]
["PCB 28",5.67,5.4306000000000001,0.86047974119685122,0.88327990417342517]
["PCB 29",5.66,5.4188000000000001,0.85236926804022239,0.88526170855825725]
["PCB 30",5.44,5.1592000000000002,0.67393885859439617,0.92164732619991696]
["PCB 31",5.67,5.4306000000000001,0.86047974119685122,0.88327990417342517]
["PCB 32",5.44,5.1592000000000002,0.67393885859439617,0.92164732619991696]
["PCB 33",5.6,5.3479999999999999,0.8037064291004512,0.89651239135135175]
["PCB 34",5.66,5.4188000000000001,0.85236926804022239,0.88526170855825725]
["PCB 35",5.82,5.6076000000000006,0.98213683854627831,0.84957853665111649]
["PCB 36",5.88,5.6783999999999999,1.0307996774860486,0.83385854551619454]
["PCB 37",5.83,5.6193999999999997,0.99024731170290625,0.84705147780225976]
["PCB 38",5.76,5.5367999999999995,0.93347399960650712,0.86398454635136235]
["PCB 39",5.89,5.690199999999999,1.0389101506426774,0.83110660937373815]
["PCB 40",5.66,5.4188000000000001,0.85236926804022239,0.88526170855825725]
["PCB 41",5.69,5.4542000000000002,0.87670068751010799,0.8792215362802378]
["PCB 42",5.76,5.5367999999999995,0.93347399960650712,0.86398454635136235]
["PCB 43",5.75,5.5249999999999995,0.92536352644987918,0.86626242927301389]
["PCB 44",5.75,5.5249999999999995,0.92536352644987918,0.86626242927301389]
["PCB 45",5.53,5.2654000000000005,0.74693311700405296,0.9083298720230123]
["PCB 46",5.53,5.2654000000000005,0.74693311700405296,0.9083298720230123]
["PCB 47",5.85,5.6429999999999998,1.006468258016163,0.84188664350937747]
["PCB 48",5.78,5.5604000000000005,0.94969494591976478,0.85932454306581862]
["PCB 49",5.85,5.6429999999999998,1.006468258016163,0.84188664350937747]
["PCB 50",5.63,5.3834,0.8280378485703368,0.89102200568445478]
["PCB 51",5.63,5.3834,0.8280378485703368,0.89102200568445478]
["PCB 52",5.84,5.6311999999999998,0.99835778485953508,0.84448760670408918]
["PCB 53",5.62,5.3715999999999999,0.81992737541370886,0.89288163017928301]
["PCB 54",5.21,4.8877999999999995,0.48739797599194112,0.94773228129359799]
["PCB 55",6.11,5.9498000000000006,1.2173405600885037,0.76061068090190898]
["PCB 56",6.11,5.9498000000000006,1.2173405600885037,0.76061068090190898]
["PCB 57",6.17,6.0206,1.2660033990282749,0.73805899603887071]
["PCB 58",6.17,6.0206,1.2660033990282749,0.73805899603887071]
["PCB 59",5.95,5.7610000000000001,1.0875729895824486,0.81378271664556356]
["PCB 60",6.11,5.9498000000000006,1.2173405600885037,0.76061068090190898]
["PCB 61",6.04,5.8671999999999995,1.1605672479921045,0.78513089668044289]
["PCB 62",5.89,5.690199999999999,1.0389101506426774,0.83110660937373815]
["PCB 63",6.17,6.0206,1.2660033990282749,0.73805899603887071]
["PCB 64",5.95,5.7610000000000001,1.0875729895824486,0.81378271664556356]
["PCB 65",5.86,5.6547999999999998,1.0145787311727918,0.83924831766908348]
["PCB 66",6.2,{"$f":"1.18*B102-1.26","v":6.056},{"$f":"B102*$B$30+$B$31","v":1.2903348184981605},{"$f":"IF((10^D102)*$C$8*86400/$C$7^2/(10^C102)^2<700, 1-EXP((10^D102)*$C$8*86400/$C$7^2/(10^C102)^2)*ERFC((10^D102) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C102)), 1-1/((10^D102)*$C$8*86400/$C$7^2/(10^C102)^2*3.14)^0.5)","v":0.72626761832776299}]
["PCB 67",6.2,6.056,1.2903348184981605,0.72626761832776299]
["PCB 68",6.26,6.1267999999999994,1.3389976574379308,0.70170068049601375]
["PCB 69",6.04,5.8671999999999995,1.1605672479921045,0.78513089668044289]
["PCB 70",6.2,6.056,1.2903348184981605,0.72626761832776299]
["PCB 71",5.98,5.7964000000000002,1.1119044090523342,0.80459068021293745]
["PCB 72",6.26,6.1267999999999994,1.3389976574379308,0.70170068049601375]
["PCB 73",6.04,5.8671999999999995,1.1605672479921045,0.78513089668044289]
["PCB 74",6.2,6.056,1.2903348184981605,0.72626761832776299]
["PCB 75",6.05,5.8789999999999996,1.1686777211487325,0.7817476083640964]
["PCB 76",6.13,5.9733999999999998,1.2335615064017604,0.75324871326145537]
["PCB 77",6.36,6.2448000000000006,1.4201023890042155,0.65809238465860664]
["PCB 78",6.35,6.2329999999999997,1.4119919158475867,0.66258941057690901]
["PCB 79",6.42,6.3155999999999999,1.4687652279439867,0.63055609749912855]
["PCB 80",6.48,6.3864000000000001,1.5174280668837579,0.60219999580035688]
["PCB 81",6.36,6.2448000000000006,1.4201023890042155,0.65809238465860664]
["PCB 82",6.2,6.056,1.2903348184981605,0.72626761832776299]
["PCB 83",6.26,6.1267999999999994,1.3389976574379308,0.70170068049601375]
["PCB 84",6.04,5.8671999999999995,1.1605672479921045,0.78513089668044289]
["PCB 85",6.3,6.1739999999999995,1.3714395500644443,0.68463381332105744]
["PCB 86",6.23,6.0914000000000001,1.314666237968046,0.71414439701548504]
["PCB 87",6.29,6.1621999999999995,1.3633290769078164,0.68894978884472158]
["PCB 88",6.07,5.9026000000000005,1.1848986674619901,0.7748611275751458]
["PCB 89",6.07,5.9026000000000005,1.1848986674619901,0.7748611275751458]
["PCB 90",6.36,6.2448000000000006,1.4201023890042155,0.65809238465860664]
["PCB 91",6.13,5.9733999999999998,1.2335615064017604,0.75324871326145537]
["PCB 92",6.35,6.2329999999999997,1.4119919158475867,0.66258941057690901]
["PCB 93",6.04,5.8671999999999995,1.1605672479921045,0.78513089668044289]
["PCB 94",6.13,5.9733999999999998,1.2335615064017604,0.75324871326145537]
["PCB 95",6.13,5.9733999999999998,1.2335615064017604,0.75324871326145537]
["PCB 96",5.71,5.4778000000000002,0.89292163382336476,0.87503440324790238]
["PCB 97",6.29,6.1621999999999995,1.3633290769078164,0.68894978884472158]
["PCB 98",6.13,5.9733999999999998,1.2335615064017604,0.75324871326145537]
["PCB 99",6.39,6.2801999999999998,1.4444338084741011,0.64443822027209741]
["PCB 100",6.23,6.0914000000000001,1.314666237968046,0.71414439701548504]
["PCB 101",6.38,6.2683999999999997,1.4363233353174722,0.64901601482647109]
["PCB 102",6.16,6.0087999999999999,1.257892925871646,0.74191403558286551]
["PCB 103",6.22,6.0795999999999992,1.3065557648114163,0.71822168249435059]
["PCB 104",5.81,5.5957999999999997,0.97402636538964948,0.85206907187640035]
["PCB 105",6.65,6.5870000000000006,1.6553061105464417,0.51917932290073576]
["PCB 106",6.64,6.5751999999999997,1.647195637389812,0.52411371158877584]
["PCB 107",6.71,6.6577999999999999,1.703968949486212,0.4896041654610167]
["PCB 108",6.71,6.6577999999999999,1.703968949486212,0.4896041654610167]
["PCB 109",6.48,6.3864000000000001,1.5174280668837579,0.60219999580035688]
["PCB 110",6.48,6.3864000000000001,1.5174280668837579,0.60219999580035688]
["PCB 111",6.76,6.7167999999999992,1.7445213152693544,0.46510895343393754]
["PCB 112",6.45,6.351,1.4930966474138723,0.61646868674017219]
["PCB 113",6.54,6.4572000000000003,1.5660909058235282,0.57322037161547856]
["PCB 114",6.65,6.5870000000000006,1.6553061105464417,0.51917932290073576]
["PCB 115",6.49,6.3982000000000001,1.5255385400403858,0.59740780037746266]
["PCB 116",6.33,6.2093999999999996,1.3957709695343299,0.67149742289549319]
["PCB 117",6.46,6.3628,1.5012071205705002,0.61173137801791255]
["PCB 118",6.74,6.6932,1.7283003689560976,0.4748817700721083]
["PCB 119",6.58,6.5043999999999995,1.5985327984500417,0.55365822352189609]
["PCB 120",6.79,6.7522000000000002,1.76885273473924,0.4505318125496528]
["PCB 121",6.64,6.5751999999999997,1.647195637389812,0.52411371158877584]
["PCB 122",6.64,6.5751999999999997,1.647195637389812,0.52411371158877584]
["PCB 123",6.74,6.6932,1.7283003689560976,0.4748817700721083]
["PCB 124",6.73,6.6814,1.7201898957994697,0.47978177470743699]
["PCB 125",6.51,6.4217999999999993,1.5417594863536426,0.58777518580314037]
["PCB 126",6.89,6.8701999999999988,1.8499574663055238,0.40294104656434515]
["PCB 127",6.95,6.9410000000000007,1.898620305245295,0.37536972844122596]
["PCB 128",6.74,6.6932,1.7283003689560976,0.4748817700721083]
["PCB 129",6.73,6.6814,1.7201898957994697,0.47978177470743699]
["PCB 130",6.8,{"$f":"1.18*B166-1.26","v":6.7639999999999993},{"$f":"B166*$B$30+$B$31","v":1.7769632078958679},{"$f":"IF((10^D166)*$C$8*86400/$C$7^2/(10^C166)^2<700, 1-EXP((10^D166)*$C$8*86400/$C$7^2/(10^C166)^2)*ERFC((10^D166) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C166)), 1-1/((10^D166)*$C$8*86400/$C$7^2/(10^C166)^2*3.14)^0.5)","v":0.44569832980791901}]
["PCB 131",6.58,6.5043999999999995,1.5985327984500417,0.55365822352189609]
["PCB 132",6.58,6.5043999999999995,1.5985327984500417,0.55365822352189609]
["PCB 133",6.86,6.8347999999999995,1.8256260468356391,0.41702728159252278]
["PCB 134",6.55,6.4689999999999994,1.5742013789801561,0.56834450185575247]
["PCB 135",6.64,6.5751999999999997,1.647195637389812,0.52411371158877584]
["PCB 136",6.22,6.0795999999999992,1.3065557648114163,0.71822168249435059]
["PCB 137",6.83,6.7994000000000003,1.8012946273657535,0.43128701398576197]
["PCB 138",6.83,6.7994000000000003,1.8012946273657535,0.43128701398576197]
["PCB 139",6.67,6.6105999999999998,1.6715270568596976,0.50931094294370494]
["PCB 140",6.67,6.6105999999999998,1.6715270568596976,0.50931094294370494]
["PCB 141",6.82,6.7875999999999994,1.7931841542091256,0.43607506349196545]
["PCB 142",6.51,6.4217999999999993,1.5417594863536426,0.58777518580314037]
["PCB 143",6.6,6.5279999999999996,1.6147537447632985,0.54382868281263241]
["PCB 144",6.67,6.6105999999999998,1.6715270568596976,0.50931094294370494]
["PCB 145",6.25,6.1150000000000002,1.3308871842813019,0.70588341470849203]
["PCB 146",6.89,6.8701999999999988,1.8499574663055238,0.40294104656434515]
["PCB 147",6.64,6.5751999999999997,1.647195637389812,0.52411371158877584]
["PCB 148",6.73,6.6814,1.7201898957994697,0.47978177470743699]
["PCB 149",6.67,6.6105999999999998,1.6715270568596976,0.50931094294370494]
["PCB 150",6.32,6.1976000000000004,1.3876604963777019,0.67590698364806956]
["PCB 151",6.64,6.5751999999999997,1.647195637389812,0.52411371158877584]
["PCB 152",6.22,6.0795999999999992,1.3065557648114163,0.71822168249435059]
["PCB 153",6.92,6.9055999999999997,1.8742888857754094,0.38904883987372973]
["PCB 154",6.76,6.7167999999999992,1.7445213152693544,0.46510895343393754]
["PCB 155",6.41,6.3037999999999998,1.4606547547873578,0.63520743025101667]
["PCB 156",7.18,7.2123999999999988,2.0851611878477501,0.27917227106853093]
["PCB 157",7.18,7.2123999999999988,2.0851611878477501,0.27917227106853093]
["PCB 158",7.02,7.0236000000000001,1.9553936173416941,0.34437610637922134]
["PCB 159",7.24,7.2832000000000008,2.1338240267875213,0.25695748404534902]
["PCB 160",6.93,6.9173999999999989,1.8823993589320382,0.38446456068724144]
["PCB 161",7.08,7.0944000000000003,2.0040564562814653,0.31895191402468959]
["PCB 162",7.24,7.2832000000000008,2.1338240267875213,0.25695748404534902]
["PCB 163",6.99,6.9882000000000009,1.9310621978718094,0.35749248882391471]
["PCB 164",7.02,7.0236000000000001,1.9553936173416941,0.34437610637922134]
["PCB 165",7.05,7.0589999999999993,1.9797250368115797,0.3315251617561441]
["PCB 166",6.93,6.9173999999999989,1.8823993589320382,0.38446456068724144]
["PCB 167",7.27,7.3186,2.158155446257406,0.2463291058925815]
["PCB 168",7.11,7.1297999999999995,2.0283878757513509,0.3066670430386903]
["PCB 169",7.42,7.4955999999999996,2.2798125436068331,0.19801583566952907]
["PCB 170",7.27,7.3186,2.158155446257406,0.2463291058925815]
["PCB 171",7.11,7.1297999999999995,2.0283878757513509,0.3066670430386903]
["PCB 172",7.33,7.3894000000000002,2.2068182851971772,0.22603932863074128]
["PCB 173",7.02,7.0236000000000001,1.9553936173416941,0.34437610637922134]
["PCB 174",7.11,7.1297999999999995,2.0283878757513509,0.3066670430386903]
["PCB 175",7.17,7.2005999999999997,2.0770507146911212,0.28299743914174813]
["PCB 176",6.76,6.7167999999999992,1.7445213152693544,0.46510895343393754]
["PCB 177",7.08,7.0944000000000003,2.0040564562814653,0.31895191402468959]
["PCB 178",7.14,7.1651999999999987,2.0527192952212356,0.29467967815805418]
["PCB 179",6.73,6.6814,1.7201898957994697,0.47978177470743699]
["PCB 180",7.36,7.4247999999999994,2.2311497046670627,0.21637809896986104]
["PCB 181",7.11,7.1297999999999995,2.0283878757513509,0.3066670430386903]
["PCB 182",7.2,7.2360000000000007,2.1013821341610068,0.27162648754895868]
["PCB 183",7.2,7.2360000000000007,2.1013821341610068,0.27162648754895868]
["PCB 184",6.85,6.8229999999999986,1.8175155736790103,0.42176230283927252]
["PCB 185",7.11,7.1297999999999995,2.0283878757513509,0.3066670430386903]
["PCB 186",6.69,6.6341999999999999,1.6877480031729553,0.49944987103349092]
["PCB 187",7.17,7.2005999999999997,2.0770507146911212,0.28299743914174813]
["PCB 188",6.82,6.7875999999999994,1.7931841542091256,0.43607506349196545]
["PCB 189",7.71,7.8377999999999997,2.5150162651490593,0.12631549179907831]
["PCB 190",7.46,7.5427999999999997,2.3122544362333475,0.18647651261421749]
["PCB 191",7.55,7.6489999999999991,2.3852486946430034,0.16250967615952638]
["PCB 192",7.52,7.6135999999999999,2.3609172751731178,0.17019702384761837]
["PCB 193",7.52,7.6135999999999999,2.3609172751731178,0.17019702384761837]
["PCB 194",7.8,{"$f":"1.18*B230-1.26","v":7.9439999999999991},{"$f":"B230*$B$30+$B$31","v":2.5880105235587152},{"$f":"IF((10^D230)*$C$8*86400/$C$7^2/(10^C230)^2<700, 1-EXP((10^D230)*$C$8*86400/$C$7^2/(10^C230)^2)*ERFC((10^D230) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C230)), 1-1/((10^D230)*$C$8*86400/$C$7^2/(10^C230)^2*3.14)^0.5)","v":0.10923911991589186}]
["PCB 195",7.56,7.6608000000000001,2.3933591677996313,0.16001285464373816]
["PCB 196",7.65,7.7669999999999995,2.4663534262092881,0.13897238406844081]
["PCB 197",7.3,7.3539999999999992,2.1824868657272916,0.23602284716823341]
["PCB 198",7.62,7.7316000000000003,2.4420220067394025,0.14570484560044061]
["PCB 199",7.2,7.2360000000000007,2.1013821341610068,0.27162648754895868]
["PCB 200",7.27,7.3186,2.158155446257406,0.2463291058925815]
["PCB 201",7.62,7.7316000000000003,2.4420220067394025,0.14570484560044061]
["PCB 202",7.24,7.2832000000000008,2.1338240267875213,0.25695748404534902]
["PCB 203",7.65,7.7669999999999995,2.4663534262092881,0.13897238406844081]
["PCB 204",7.3,7.3539999999999992,2.1824868657272916,0.23602284716823341]
["PCB 205",8,8.18,2.7502199866912846,7.8536420848799415E-2]
["PCB 206",8.09,8.2861999999999991,2.8232142451009405,6.7519593000284428E-2]
["PCB 207",7.74,7.8732000000000006,2.5393476846189449,0.12037638606605183]
["PCB 208",7.71,7.8377999999999997,2.5150162651490593,0.12631549179907831]
["PCB 209",8.18,8.3923999999999985,2.8962085035105964,5.7970588831963599E-2]

{"sheet":"Dioxins in PE","index":5,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
["Dioxins/Furans CALIBRATION MODEL FOR PE SAMPLER"]
["Shen, X., & Reible, D. (2019). An analytical model for the fate and transport of performance reference compounds and target compounds around cylindrical passive samplers. Chemosphere."]
["Version 1.7"]
["2021-08-05",null,null,null,null,null,"Brief techical note"]
[null,null,null,null,null,null,"1. The 'Fss' values refer to the fractional approach to steady state, which is the 1-C/C0 for PRCs and C/Ceq for target compounds"]
["Parameters","Symbol","Value","Unit",null,null,"2. The 'Kpw' values refer to the polymer-water partition coefficients, and can be estimated from octanol-water coefficients Kow using the correlations "]
["Thickness","L",2.5400000000000002E-3,"cm",null,null,null,"Log Kpw = 1.18 * Log Kow - 1.26",null,"(Ghosh et al., 2014)"]
["Sampling time","t",14,"days",null,null,"3. The fitting process is to find parameters for the following correlation between Kow and the product of retardation factor R and effective diffusivities D   "]
[null,null,null,null,null,null,null,"Log RD = a * Log Kow + b"]
[null,null,null,null,null,null,"4. The ‘Nonlinear’ in 'Option' is set to minimize the difference in Fss from calibrated to measurements, 'Linearized' is to minimuze the calibrated R values "]
["Number of PRCs",4,null,null,null,null,"5. The a value of the above correlation could be fixed to a given constant  ",null,null,null,{"$f":"PRCNumber(13,$B$11)","v":""}]
["PRC #",{"$f":"PRCNumber(1,$B$11)","v":1},{"$f":"PRCNumber(2,$B$11)","v":2},{"$f":"PRCNumber(3,$B$11)","v":3},{"$f":"PRCNumber(4,$B$11)","v":4}]
["PRC name","C13-1234-TCDD","C13-123789-HxCDD","C13-2,7/2,8 DiCDD","C13-1234678 HpCDD",null,"Procedure"]
["Log Kow",6.53,7.92,5.19,8.64,null,"1. Update the properties of sampler and PRCs on this sheet in Green "]
["Log Kpw",{"$f":"1.18*B14-1.26","v":6.4454000000000002},{"$f":"1.18*C14-1.26","v":8.0855999999999995},4.8642000000000003,8.9352,null,"2. Start the fitting by clicking on  \"Fit fss Data\""]
["Measured PRC Fss",0.7,0.5,0.8,0.3,null,"3. Check the fitted results (parameters in Row 25 results in the following figure)"]
[null,null,null,null,null,null,"4. View model results in the following figure, the returned data are in rec_fitted_plot"]
[]
[null,null,null,null,null,null,"Database of frequently used PRCs"]
[]
[null,null,null,null,null,null,"PRCs set 1"]
[null,null,null,null,null,null,"PRC name","C13-1234-TCDD","C13-123789-HxCDD","C13-2,7/2,8 DiCDD","C13-1234678 HpCDD"]
[null,null,null,null,null,null,"Log Kow",6.53,7.92,5.19,8.64]
[null,null,null,null,null,null,"Log Kpw",6.4454000000000002,8.0855999999999995,4.8642000000000003,8.9352]
[]
[]
["Results"]
["Cylindrical diffusion model","Log RD = a * Log Kow + b"]
[]
["a",1.8676716595495448]
["b",-10.272158632236479]
["r2",0.99687564975541609]
[]
[]
["Model prediction"]
["Target Compound","Log Kow","Log Kpw","Log RD","fss"]
["2-MCDD",4.58,{"$f":"1.18*B37-1.26","v":4.1444000000000001},{"$f":"B37*$B$30+$B$31","v":-1.718222431499564},{"$f":"IF((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2<700, 1-EXP((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2)*ERFC((10^D37) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C37)), 1-1/((10^D37)*$C$8*86400/$C$7^2/(10^C37)^2*3.14)^0.5)","v":0.87194811010543893}]
["2,3-DiCDD",5.23,{"$f":"1.18*B38-1.26","v":4.9114000000000004},{"$f":"B38*$B$30+$B$31","v":-0.50423585279235894},{"$f":"IF((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2<700, 1-EXP((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2)*ERFC((10^D38) ^ 0.5*($C$8*86400)^ 0.5/$C$7/(10^C38)), 1-1/((10^D38)*$C$8*86400/$C$7^2/(10^C38)^2*3.14)^0.5)","v":0.81943377824299224}]
["2,7/2,8-DiCDD",5.19,4.8642000000000003,-0.57894271917434104,0.82312712459757242]
["2,3,7-TrCDD",5.84,5.6311999999999998,0.63504385953286224,0.75516276304443219]
["2378-TCDF",6.46,6.3628,1.7930002884535803,0.67506913074852859]
["2378-TCDD",6.49,6.3982000000000001,1.8490304382400673,0.67085963506975999]
["12378-PeCDF",7.15,7.1769999999999996,3.0816937335427674,0.57262655536678908]
["23478-PeCDF",7.14,7.1651999999999987,3.0630170169472706,0.57417442562378218]
["12378-PeCDD",7.2,7.2360000000000007,3.1750773165202446,0.5648706636802312]
["123478-HxCDF",7.87,8.0266000000000002,4.426417328418438,0.46020486721759946]
["123678-HxCDF",7.83,7.9794,4.3517104620364577,0.46639945525683746]
["234678-HxCDF",7.83,7.9794,4.3517104620364577,0.46639945525683746]
["123478-HxCDD",7.95,8.1210000000000004,4.5758310611824022,0.4478736908701112]
["123678-HxCDD",7.89,8.0501999999999985,4.4637707616094282,0.45711447019560347]
["123789-HxCDD",7.92,8.0855999999999995,4.5198009113959152,0.4524881599721261]
["123789-HxCDF",7.87,8.0266000000000002,4.426417328418438,0.46020486721759946]
["1234678-HpCDF",8.5500000000000007,8.8290000000000006,5.6964340569121301,0.35917064233679497]
["1234678-HpCDD",8.64,8.9352,5.8645245062715894,0.34662681358968628]
["1234789-HpCDF",8.56,8.8407999999999998,5.7151107735076252,0.35776543573931918]
["OCDD",9.35,9.7729999999999997,7.1905713845517631,0.25678483764577809]
["OCDF",9.27,9.6785999999999994,7.041157651787799,0.26603993915633306]